Draft Standard MOD-017-TRE-1 — Aggregated Actual and Forecast Demands and Net Energy for Load

A. Introduction

1. Title
:
Aggregated Actual and Forecast Demands and Net Energy for Load

2. Number:
MOD-017-TRE-1
3. Purpose:
To ensure that assessments and validation of past events and databases can be performed, reporting of actual Demand data is needed.  Forecast demand data is needed to perform future system assessment to identify the need for system reinforcement for continued reliability.  In addition to assist in proper real-time operating, load information related to controllable Demand-Side Management programs is needed.  Regional Difference: Load Serving Entities removed for ERCOT Interconnection.
4. Applicability:
4.1. 
4.2. Planning Authority

4.3. Resource Planner
5. (Proposed) Effective Date:
April 1, 2005

B. Requirements

R1. The Planning Authority and Resource Planner shall each provide the following information annually on an aggregated Regional, subregional, Power Pool, or individual system basis to NERC, the Regional Reliability Organizations, and any other entities specified by the documentation in Standard MOD-016-1_R1.
R1.1. Integrated hourly demands in megawatts (MW) for the prior year.

R1.2. Monthly and annual peak hour actual demands in MW and Net Energy for Load in gigawatthours (GWh) for the prior year.

R1.3. Monthly peak hour forecast demands in MW and Net Energy for Load in GWh for the next two years.

R1.4. Annual peak hour forecast demands (summer and winter) in MW and annual Net Energy for load in GWh for at least five years and up to ten years into the future, as requested.

C. Measures

M1. Planning Authority and Resource planner shall each provide evidence to its Compliance Monitor that it provided load data per Standard MOD-017-0_R1.
D. Compliance

6. Compliance Monitoring Process

6.1. Compliance Enforcement Authority
Compliance Monitor: Regional Reliability organization
6.2. Compliance Monitoring Period and Reset Time Frame
Annually or as specified in the documentation (Standard MOD-016-1_R1.)
6.3. Data Retention
None specified.
6.4. Compliance Monitoring and Assessment Processes

Text
6.5. Additional Compliance Information

None.
7. Violation Severity Levels
	R #
	Lower VSL
	Moderate VSL
	High VSL
	Severe VSL

	R1
	Did not provide actual and forecast demands and Net Energy for Load data in one of the four areas as required in Reliability Standard MOD-017-0_R1.
	Did not provide actual and forecast demands and Net Energy for Load data in two of the four areas as required in Reliability Standard MOD-017-0_R1.
	Did not provide actual and forecast demands and Net Energy for Load data in three of the four areas as required in Reliability Standard MOD-017-0_R1.
	Did not provide actual and forecast demands and Net Energy for Load data in any of the areas as required in Reliability Standard MOD-017-0_R1.


E. Regional Variances
For MOD-017, this action will remove the LSE Applicability.  This standard states in R 1: “the Load-Serving Entity, Planning Authority and Resource Planner shall each provide the following information (R 1.1-1.4) annually on an aggregated Regional, subregional, Power Pool, individual system, or Load-Serving Entity basis to NERC, the Regional Reliability Organizations, and any other entities specified by the documentation in Standard MOD-016-1_R1.” However, in the ERCOT Interconnection, ERCOT ISO as the Planning Authority (PA) and Resource Planner (RP) provides this information to NERC.  The process for ERCOT ISO to obtain the data from the market participants is in the ERCOT Protocols, Section 11.  It would not be appropriate to register all of the DPs as LSEs in the ERCOT Interconnection because of the large number of DPs.  ERCOT ISO performs this for the Interconnection and it would be redundant to register DPs as well.
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