BSWG - EOP-005-2, R6

Intended Function Definition

* The intended function for each ERCOT Transmission Operator restoration plan is to, as applicable
  + 1. Prepare transmission to allow Black Start Resource(s) to come online;
    2. Energize the Cranking Path(s), as available, to the next start Resource(s);
    3. Provide offsite power to additional generation and/or provide stabilizing load to control voltages and frequency within acceptable operating limits;
    4. Energize the Synchronization Corridor(s) to the synchronization points between Islands, as available;
    5. Coordinate with ERCOT on synchronizing Islands at the synchronization points; and
    6. Continue to follow ERCOT Reliability Coordinator directives as the restoration continues.