**TAC Open Action Items (as of 8/20/14)**

|  |  |
| --- | --- |
| **Open Action Items from Previous Meeting(s)** | **Responsible Party** |
| * 8/5/10 – Creation of operational checklist for Resource interconnection. | ROS |
| * 8/4/11 - NPRR340, Introduction and Definition of Duration-Limited Resources (formerly “Unannounced HSL Test for Duration-Limited Resources”) – Urgent, tabled indefinitely to work through language. | TAC |
| * 11/3/11 - NPRR181, FIP Definition Revision, tabled. | TAC |
| * 4/5/12 – Request ERCOT collect and provide data to ROS to analyze ERS impact to system performance. (Related to changes made in NPRR451) | ERCOT/ROS |
| * 7/9/12 – Consider long-term solution for credit requirements in light of revisions to System Wide Offer Cap. | WMS |
| * 11/1/12 – Quarterly update to TAC on work to resolve issues discussed in NOGRR095, Type 2 Special Protection System Submissions. | ERCOT |
| * 1/3/13 - Review alternatives to definition of Wholesale Storage Load created by NPRR461, Energy Storage Settlements Consistent With PUCT Project 39917. | PRS/WMS/ROS |
| * 6/6/13 – Review manual ERCOT reports to evaluate whether still required. | COPS/ERCOT |
| * 7/2/13 – Review alternatives to implement an ancillary service product for Primary Frequency Response that can be provided on a technology-neutral basis by qualified resources. | ERCOT |
| * 9/5/13 – Review steps ERCOT utilizes in the CDR load forecasts. | WMS |
| * 9/5/13 – Review mass transition timelines for possible efficiencies. | RMS |
| * 11/7/13 – Provide monthly reports on NPRR568, Real-Time Reserve Price Adder Based on Operating Reserve Demand Curve. | ERCOT |
| * 11/7/13 – Related to NPRR524, Resource Limits in Providing Ancillary Service – provide clarification appropriate telemetering of HSL. | ROS |
| * 12/10/13 – Related to NPRR571, ERS Weather-Sensitive Loads Requirements – ERCOT Board requested that TAC report back in October 2014 with an update on ERS performance through the summer months. | TAC |
| * 2/27/14 – Review Operating Procedure that ERCOT uses to determine when they need RUC (specifically RUC for bad weather) | WMS |
| * 2/27/14 – Related to NPRR582, Refinements to Testing ERS – address testing requirements for all Resources. | WMS |
| * 2/24/14 – Related to NPRR598, Clarify Inputs to PRC and ORDC – address additional ORDC enhancements including addressing bandwidth oscillations. | WMS |
| * 4/24/14 – Evaluate concerns with bringing RUC units earlier than required because of start-up failures | ROS |
| * 5/29/14 – Review post NPRR589 SASM Performance | ERCOT |