10.12 EPS Meter Communications

10.12.1 ERCOT Acquisition of Meter Data

(1) ERCOT shall acquire EPS Meter data via the following communication links with a TDSP:

(a) Existing ERCOT Wide Area Network (WAN) interface with a TDSP; or

(b) Alternate ERCOT Wide area Network (WAN) interface requested by a TDSP. This will be an identical WAN connection to the TDSP dedicated for the purpose of EPS Meter data acquisition. .

Looking to implement January 1, 2022. This allows nearly 3 years for design, deployment and implementation of solutions.