**Section 1:**

**NOGRR194 – Relocate Black Start Training Attendance Requirements to Nodal Operating Guides**

This Nodal Operating Guide Revision Request (NOGRR) clarifies Black Start training attendance requirements originally located in Nodal Protocol Section 3.14.2, Black Start, and relocates them to the Nodal Operating Guides.

**Revised Subsections: 1.5.2 and 1.5.3**

**Section 2:**

**NOGRR185 – Related to NPRR921, RTF-2 Elimination of the Terms All-Inclusive Generation Resource and All-Inclusive Resource**

This NOGRR uses the terms created in Nodal Protocol Revision Request (NPRR) 889, RTF-1 Replace Non-Modeled Generator with Settlement Only Generator, to replace the terms All-Inclusive Generation Resource and All-Inclusive Resource in the Nodal Operating Guide.

**Revised Subsections: 2.2.7 and 2.2.8 [unboxed due to system implementation of NPRR921]**

**Section 4:**

**NOGRR191 – Related to NPRR939, Modification to Load Resources Providing RRS to Maintain Minimum PRC on Generators During Scarcity Conditions**

This NOGRR, along with NPRR939, allows ERCOT to manually deploy Load Resources other than Controllable Load Resources providing Responsive Reserve (RRS) to maintain a minimum 500 MWs of Physical Responsive Capability (PRC) reserves on Generation Resources to continuously balance the Demand with supply while maintaining the stable grid frequency for smaller disturbances.

**Revised Subsection: 4.8.1 [effective upon system implementation of NPRR939]**

**NOGRR194 – Relocate Black Start Training Attendance Requirements to Nodal Operating Guides**

*See Section 1 above.*

**Revised Subsection: 4.6.4**

**NOGRR198 – Alignment Changes for November 1, 2019 Nodal Operating Guides – NPRR939**

This NOGRR aligns Energy Emergency Alert (EEA) language in Protocol Section 6.5.9.4.2, EEA Levels, with the related Operating Guide Section 4.5.3.3. On October 8, 2019, the ERCOT Board approved NPRR939, which modified language in Protocol Section 6.5.9.4.2. Paragraph (6) of Nodal Operating Guide Section 1.3.1 provides that ERCOT can make changes to the Nodal Operating Guide to maintain duplicate language between the Protocols and Nodal Operating Guide.

**Revised Subsection: 4.5.3.3 [effective upon system implementation of NPRR939]**

**Section 8:**

**NOGRR185 – Related to NPRR921, RTF-2 Elimination of the Terms All-Inclusive Generation Resource and All-Inclusive Resource**

*See Section 2 above.*

**Revised Subsection: 8J [unboxed due to system implementation of NPRR921]**

**Administrative Changes:**

Non-substantive administrative changes were made such as spelling corrections, formatting, and correcting Section numbering and references.

**Revised Subsections: 2.2.7 and 2.9.1**