|  |  |  |  |
| --- | --- | --- | --- |
| Key Topic Concept (KTC) Number | 2 | KTC Title | Physical Responsive Capability, and ORDC Reserve |
| Date Posted | | November 5, 2019 | |
|  | |  | |
| Executive Summary | | This KTC recommends how Energy Storage Resources (ESRs) shall be treated in the calculation of Physical Responsive Capability (PRC) and Operating Reserve Demand Curve (ORDC) reserves. | |
| Recommendation Description | | PRC provided by ESRs should consider energy limitations of the Storage Resource as well as droop settings and potential higher PRC contribution when charging.  RT On-Line Reserve Capacity (RTOLCAP) provided by ESRs should also consider energy limitations of the ESR besides potential higher RTOLCAP contributions when charging. | |
| BESTF Discussion | | On 10/18/19, ERCOT staff presented material related to proposed contributions from ESRs to PRC, and ORDC Reserve.  On 11/4/19, the BESTF reached consensus on KTC 2 items 1 and 2. | |
| TAC Action Requested | | BESTF plans to request at the 11/20/19 TAC meeting a vote to approve KTC 2. | |
| TAC Action Summary | |  | |

|  |
| --- |
| Proposed KTC Recommendation Language |

# *Key Topic/Concept recommendation Language for TAC Approval*

11/20/19 TAC Meeting (Consensus from 11/4/19 BESTF meeting):

1. PRC provided by ESRs should also consider energy limitations of the Storage Resources besides droop settings and potential higher PRC contribution when charging. To consider energy limitations, a specific time period is required. This time period is currently recommended to be 15 minutes.

When online and sitting idle or discharging;

When Charging;

*ESR-Gen: Energy Storage Resource modeled as Generation Resource*

*ESR-CLR: Energy Storage Resource modeled as Controllable Load Resource (CLR)*

*SOC: State of Charge*

1. RTOLCAP provided by ESRs should also consider energy limitations of the Storage Resources besides potential higher RTOLCAP contribution when charging. To consider energy limitations, a specific time period is required. This time period is currently recommended to be 15 minutes.

When online and sitting idle or discharging;

When Charging;

*ESR-Gen: Energy Storage Resource modeled as Generation Resource*

*ESR-CLR: Energy Storage Resource modeled as Controllable Load Resource (CLR)*

*SOC: State of Charge*

# *Key Topic/Concept recommendation Language Previously approved by tac*

None.

# *Key Topic/Concept recommendation Language IN DISCUSSION AT BESTF*

None.

# *Future Decision Points and Issues for Developing Key topic/Concept recommendation Language*

None.

|  |  |
| --- | --- |
| Applicable Protocol Section(s) |  |
| Impacted System(s) / Application(s) |  |