|  |  |  |  |
| --- | --- | --- | --- |
| Key Topic Concept (KTC) Number | 8 | KTC Title | Wholesale Storage Load Treatment |
| Date Posted | | January 29, 2020 | |
|  | |  | |
| Executive Summary | | This KTC recommends whether provisions related to Wholesale Storage Load (WSL) treatment for battery energy storage should be modified. | |
| Recommendation Description | | WSL treatment should not be extended to Energy Storage Resources (ESRs) that are capable of self-serving retail Load, such as Private Use Network (PUN) Load, with the stored energy. | |
| BESTF Discussion | | On 11/15/19, ERCOT staff presented on KTC 8 item 1, which asked about the appropriateness of WSL treatment for batteries located within PUNs.  On 12/6/19, the BESTF reached consensus on KTC 8 item 1. | |
| TAC Action Requested | | BESTF plans to request at the 1/29/20 TAC meeting a vote to approve KTC 8 item 1. | |
| TAC Action Summary | | On 1/29/20, TAC approved KTC 8 item 1. | |

|  |
| --- |
| Proposed KTC Recommendation Language |

# *Key Topic/Concept recommendation Language for TAC Approval*

None.

# *Key Topic/Concept recommendation Language Previously Approved by tac*

1/29/20 TAC Meeting (BESTF Consensus at 12/6/19 BESTF Meeting):

The BESTF acknowledged the language in PUC Subst. Rule 25.501 (m) which states that WSL occurs when stored energy is “subsequently re-generated and sold at wholesale as energy or ancillary services.” Based on this provision in Rule, a battery that serves retail Load behind its Point of Interconnection should be ineligible for WSL treatment.

# *Key Topic/Concept recommendation Language IN DISCUSSION AT BESTF*

None.

# *Future Decision Points and Issues for Developing Key topic/Concept recommendation Language*

1. Item #2 in KTC-8 asks: *Should WSL treatment implementation extend to non-dispatched generators? If yes, should there be differentiation between a SOG that is co-located with customer load and one that only has auxiliary loads behind the metering point?*

Settlement Only Energy Storage is not yet a defined term, pending future NPRR submissions by the Resource Definition Task Force (RTF). Under current rules, a battery with capacity >1 MW that injects to the grid would register with ERCOT as a Settlement Only Distribution Generator or Settlement Only Transmission Generator. The BESTF has deferred discussion on WSL treatment for these resources until sometime early next year.

|  |  |
| --- | --- |
| Applicable Protocol Section(s) |  |
| Impacted System(s) / Application(s) |  |