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	Include Section No. and Title

	Related Documents Requiring Revision/Related Revision Requests
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  Other:  (explain)

(please select all that apply)

	Business Case
	A new PROFILETYPECODE (BUSLRG) will be used for > 700 kW/kVA premises where the TDSP can support a 4CP billing rate with an AMS profile. This PROFILETYPECODE will lead to the addition of sixteen PROFILECODES (one for each of eight weather zones plus WS, NWS). The existing BUSIDRRQ will remain. This approach allows for easy identification of >700 kW/kVA premises and provides aggregate level MWH data that can be utilized for ad-hoc analysis.  Without a separate profile type, the load for these large customers would be comingled with smaller business profile types.  This approach also provides more meaningful information to REPs which can be factored into their pricing programs and is a better long-term solution as opposed to trying to repurpose an existing profile code attribute.


	Sponsor

	Name
	Calvin Opheim

	E-mail Address
	Calvin.Opheim@ercot.com

	Company
	ERCOT

	Phone Number
	

	Cell Number
	

	Market Segment
	Not applicable.


	Market Rules Staff Contact

	Name
	

	E-Mail Address
	

	Phone Number
	


	Proposed Guide Language Revision


19 Definitions and Acronyms
19.1

Definitions

The defined terms in this Section are limited to those used specifically in the Load Profiling Guide (LPG).  Any additional defined terms used in the LPG can be found in Protocol Section 2, Definitions and Acronym
I
[Back to Top]
Interval Data Recorder (IDR) Requirement

The kW level at which the installation of interval data recorders are required for settlement purposes as set forth in Protocol Section 18.6.1, Interval Data Recorder  Mandatory Installation Requirements.

Appendix D, Profile Decision Tree – “Start -- 2014 v1.8” worksheet
	
	1.  Determine the Profile Type Code
	

	
	A.
	Select the Profile Group
	

	
	
	Select the appropriate Profile Group from the following:  NM (for Non-Metered), RES (for Residential), or BUS (for Business).

	
	
	
	

	
	B.
	Select the Profile Segment
	

	
	
	Valid Profile Segments are dependent upon the Profile Group and other factors.  Please see the Segment Assignment tab.

	
	
	Valid Segments for NM are:  LIGHT and FLAT.
	

	
	
	Valid Segments for RES are: LOWR, HIWR, LOPV, HIPV, LOWD, HIWD, LODG, and HIDG.

	
	
	Valid Segments for BUS are: NODEM, LOLF, MEDLF, HILF, IDRRQ, LRG, OGFLT, NODPV, LOPV, MEDPV, HIPV, OGFPV, NODWD, LOWD, MEDWD, HIWD, OGFWD, NODDG, LODG, MEDDG, HIDG, and OGFDG.

	
	
	
	

	
	C. 
	Concatenate the Profile Group and Profile Segment to form the Profile Type Code

	
	
	Convert the Profile Group and Profile Segment to one field, e.g., BUSLOLF.

	
	
	
	


	
	4. Select the Weather Sensitivity Code
	

	
	         Assign the Weather Sensitivity Code as follows unless notified by ERCOT to assign a

	
	         different Weather Sensitivity Code, per Protocol Section 11, Data Acquisition and Aggregation.

	
	A.
	Assign NWS for ESI IDs with a meter data type code of NIDR.

	
	B.
	Assign NWS for ESI IDs that have a profile type code of BUSIDRRQ or BUSLRG.

	
	C.
	Assign WS to all other ESI IDs.
	

	
	
	
	


	
	5. Select the Time-Of-Use Schedule Code
	

	
	A.
	Assign NOTOU for ESI IDs not served under a Time-Of-Use schedule (for kWh), or if Profile Type is BUSIDRRQ or BUSLRG.

	
	B.
	For ESI IDs served under a TOU schedule (for kWh), assign the appropriate Time-Of-Use Schedule Code from the TOU Schedules tab.  

	
	
	
	


Appendix D, Profile Decision Tree – “FAQ” worksheet
	7.
	Q.
	For a premise that has a Profile Type code of 'BUSIDRRQ' or ‘BUSLRG’, when should a TDSP change the Weather Sensitivity code to 'WS' ?

	
	
	
	
	

	
	A.
	When specified on the report resulting from the annual weather responsiveness determination, per Protocol Section 11, Data Acquisition and Aggregation.


Appendix D, Profile Decision Tree – “Use of Components” worksheet
	Weather Sensitivity     example:  NWS
	This component is utilized only if the Meter Data Type is 'IDR' and the ESI ID's interval data have not been received by ERCOT for a specific settlement period.  In this case, the Weather Sensitivity component of the Profile ID dictates whether a weather sensitive or non-weather sensitive proxy day routine will be used to estimate the interval data.  For ESI IDs that have the BUSIDDRQ or BUSLRG Profile Type assignment, ERCOT will determine which ones are weather sensitive (per Protocols Section 11) and will contact the TDSPs to have them implement the appropriate changes.


Appendix D, Profile Decision Tree – “Definitions” worksheet
	Definitions Used in Profile ID Assignments
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Term
	Description/Definition
	
	
	
	
	
	
	
	
	Additional info @

	
	ActiveDaysm
	Denotes the number of days in a particular Usage Month in which the ESI ID received service (please see ESI ID Status for further clarification).
	ESI ID Status definition

	
	ADUsem
	Denotes the Average Daily Usage (in kWh) for a specific Usage Month.  This is derived by dividing the Total kWh (kWhm) in the Usage Month by the Number of Active Days (ActiveDaysm) in the same Usage Month, and rounding to two decimal places per the Rounding instructions on this tab. 
	Usage Month Methodology tab

	
	ADUsep
	Denotes the Average Daily Usage (in kWh) for a specific Meter Read Period.  This is derived by dividing the Metered Usage (in kWh) for the Meter Read Period by the Number of Days in the Meter Read Period, and rounding to two decimal places per the Rounding instructions on this tab.
	Usage Month Methodology tab

	
	AHUsem
	Denotes the Average Hourly Usage (in kWh) for Usage Month m.  
	
	Segment Assignment tab

	
	Assignment Year
	Assignment Year refers to a specific set of 12 Usage Months used to determine Business Profile ID assignments.  An Assignment Year normally runs from May through the following April.  However, to determine Profile ID assignments it may be necessary to obtain data from outside the May through April period.  For example, to calculate complete Usage Months for May 2005 and April 2006, meter read data from April 2005 and May 2006 will most likely be required.

	
	AvgLF
	The Average Load Factor is defined as a weighted average of the individual monthly load factors, where demand levels are used to define the weights.
	Segment Assignment tab

	
	Business (BUS)
	Profile Group designation for non-residential ESI IDs whose service is metered.  This encompasses rate classes for business ESI IDs, in addition to other classes.

	
	Daily Demand
	Daily Demand is based on Max Metered Demand (in kW) and represents the kW applied to each day in that period. 

	
	Daily Usage
	Daily Usage is based on ADUsep and represents the kWh used for each day of that period.  
	
	

	
	Daysp
	The Meter Read Stop Date minus the Meter Read Start Date for a specific meter read.
	
	

	
	ESI ID Status
	Active -- ESI ID is presently receiving service (energized) and a REP is currently assigned to it in ERCOT's system.

	
	
	De-Energized -- ESI ID does not have a REP assigned in ERCOT's system, but has not been retired.  An 814_16 Move-In is necessary to change to Active status.  

	
	
	Inactive -- ESI ID is retired and is to never again receive service.
	
	

	
	ESI ID Year Use
	Denotes the sum of the kWhp for each year value of an ESI ID.
	
	
	Segment Assignment tab

	
	FLAT
	Profile Segment designation for any Non-Metered load that is not identified as lighting.
	
	

	
	HIDG
	Denotes a High Winter Ratio or High Load Factor Profile Segment for premises with Distributed Generation other than PV or wind.
	DG tab

	
	HILF
	Denotes a High Load Factor Profile Segment designation where AvgLF > 0.60.
	
	Segment Assignment tab

	
	HIPV
	Denotes a High Winter Ratio or High Load Factor Profile Segment for Premises with photovoltaic generation, applicable to ESI IDs that meet the criteria on the DG tab.
	Segment Assignment tab

	
	HIWD
	Denotes a High Winter Ratio or High Load Factor Profile Segment for Premises with  wind generation, applicable to ESI IDs that meet the criteria on the DG tab.
	Segment Assignment tab

	
	HIWR
	Denotes a High Winter Ratio Profile Segment designation as derived per the Segment Assignment tab.
	
	Segment Assignment tab

	
	IDR
	Interval Data Recorder -- A device that is capable of recording electrical usage in each settlement interval. 
	Protocols Sections 9 & 10

	
	IDRRQ or LRG
	Denotes a Profile Segment for which an Interval Data Recorder (IDR) is required.
	
	Protocols Section 18.6.1

	
	kWDaysm
	Denotes the number of days in a particular Usage Month for which there are Daily Demand values.
	
	

	
	kWhm
	Denotes the total energy consumed (in kilowatthours) in Usage Month m.  This is calculated by summing the values for Daily Usage over the entire Usage Month.

	
	kWhp
	Denotes the total energy consumed (in kilowatthours) in Meter Read Period.  This is calculated by summing the values for Daily Usage over the entire Meter Read Period.
	Segment Assignment tab

	
	LIGHT
	Profile Segment designation for all Non-Metered lighting load.
	
	
	

	
	Load Profile Group
	A high-level classification of a set of customers who have similar characteristics.  The Load Profile Groups are:  Non-Metered, Residential, and Business.  Together, the Load Profile Group and the Load Profile Segment form the Load Profile Type. 

	
	Load Profile ID
	The load profile designation string that contains: 1) the Load Profile Type Code; 2) the Weather Zone Code; 3) the Meter Data Type Code; 4) the Weather Sensitivity Code; and 5) the Time-Of-Use Schedule Code.  An example of a Profile ID:  RESLOWR_FWEST_NID
	Start tab

	
	Load Profile Segment
	A sub-classification of a Load Profile Group.  High Winter Ratio (HIWR) is an example of a Load Profile Segment.  Together, the Load Profile Group and the Load Profile Segment form the Load Profile Type.  

	
	Load Profile Type
	From Protocols, Section 2: "A classification of a group of Customers having similar energy usage patterns and that are assigned the same Load Profile."   Load Profile Type is also the concatenation of the Load Profile Group and Load Profile Segment.

	
	LODG
	Denotes a Low Winter Ratio or Low Load Factor Profile Segment for premises with Distributed Generation other than PV or wind.
	DG tab

	
	LOLF
	Denotes a Low Load Factor Profile Segment designation where AvgLF < 0.40.
	
	Segment Assignment tab

	
	LOPV
	Denotes a Low Winter Ratio or Low Load Factor Profile Segment for Premises with photovoltaic generation, applicable to ESI IDs that meet the criteria on the DG tab.
	Segment Assignment tab

	
	LOWD
	Denotes a Low Winter Ratio or Low Load Factor Profile Segment for Premises with Distributed Generation other than PV, applicable to ESI IDs that meet the criteria on the DG tab.
	Segment Assignment tab

	
	LOWR
	Denotes a Low Winter Ratio Profile Segment designation as derived per the Segment Assignment tab.  (This is sometimes assigned as the default if data not available.)
	Segment Assignment tab

	
	Max Metered Demand
	The highest measured demand (kW) during a Usage Period.  Please see the kVA to kW tab if demand is measured in kVA.  

	
	MaxkWm
	Denotes the straight average of the demand values assigned to the days in the Usage Month.  The values used for Daily Demand should be the maximum demand (kW) that occurred during that Usage Period.

	
	MEDDG
	Denotes a Medium Load Factor Profile Segment for premises with Distributed Generation other than PV or wind.
	DG tab

	
	MEDLF
	Denotes a Medium Load Factor Profile Segment designation where 0.40 ≤ AvgLF ≤ 0.60.  (This is sometimes assigned as the default if data not available or if the denominator equals zero.)
	Profile Segments tab

	
	MEDPV
	Denotes a Medium Load Factor Profile Segment for Premises with photovoltaic generation, applicable to ESI IDs that meet the criteria on the DG tab.
	Segment Assignment tab

	
	MEDWD
	Denotes a Medium Load Factor Profile Segment for Premises with wind generation, applicable to ESI IDs that meet the criteria on the DG tab.
	Segment Assignment tab

	
	Meter Read Start Date
	The Meter Read Start Date for a Usage Period corresponds with the date the meter was actually read.  For any given Usage Period the Meter Read Start Date is the prior meter read date, regardless of the time the meter was read.  If no prior meter read date exists, the date the account was energized or activated shall be considered the Meter Read Start Date.  

	
	Meter Read Stop Date
	The Meter Read Stop Date for a Usage Period corresponds with the date the meter was actually read.  For any given Usage Period the Meter Read Stop Date is the date of the meter read that ends that period, regardless of what time the meter is read.  

	
	Metered Usage
	In the context of Usage Month, Metered Usage is the total electricity consumption (in kWh) measured during a Usage Period.  This includes estimated usage if the values were submitted to ERCOT and actual measured usage for the same period was never submitted to ERCOT.

	
	NADUsep
	Denotes the normalized Average Daily Usage (in kWh) for a specific Meter Read Period.  This is derived by subtracting the mean Average Daily Usage over the Usage Period from the Average Daily Usage for a specific Meter Read Period and dividing by the standard deviation of the Average Daily Usage for the Usage Period, and rounding to two decimal places per the Rounding instructions on this tab.
	Segment Assignment tab

	
	NIDR
	An electricity meter that is not an Interval Data Recorder.  NIDR designation shall include IDRs installed for Load Research purposes and Time-Of-Use meters.
	Segment Assignment tab

	
	NODDG
	Denotes a Non-Demand Profile Segment for premises with Distributed Generation other than PV or wind, applicable to ESI IDs that meet the criteria on the DG tab.
	DG tab

	
	NODEM
	NODEM stands for Non-Demand. The TDSP may assign the NODEM Profile Segment for non-residential ESI IDs which are not billed demand. 

	
	NODPV
	Denotes a Non-Demand Profile Segment for Premises with photovoltaic generation, applicable to ESI IDs that meet the criteria on the DG tab.
	Segment Assignment tab

	
	NODWD
	Denotes a Non-Demand Profile Segment for Premises with wind generation, applicable to ESI IDs that meet the criteria on the DG tab.
	Segment Assignment tab

	
	Non-Metered (NM)
	Profile Group designation for ESI IDs served within a rate class specifically for non-metered loads, e.g., Street Lights and Traffic Signals.  Assignment of NM is not valid for any load that is metered.

	
	Number of Days in the Meter Read Period
	The Number of Days in the Meter Read Period is defined as the Meter Read Stop Date minus the Meter Read Start Date.  For example, if a meter was read on August 1st and again on August 31st, the Number of Days in the Meter Read Period is 30.  In another example, if a meter was read on June 12th and the next read occurred on July 13th, the Number of Days in the Meter Read Period is 31.  

	
	NWS
	Non-Weather Sensitive designation of the Weather Sensitivity Code. 
	
	

	
	OGFDG
	Denotes an Oil and Gas Flat Profile Segment for Premises with Distributed Generation other than PV or wind, applicable to ESI IDs that meet the criteria on the DG tab and the Oil & Gas tab.
	DG tab

	
	OGFLT
	Denotes a Profile Segment of Oil and Gas Flat, applicable to ESI IDs that meet the criteria on the Oil & Gas tab.
	Oil & Gas tab

	
	OGFPV
	Denotes a Profile Segment with photovoltaic generation, applicable to ESI IDs that meet the criteria on the DG tab
	Segment Assignment tab

	
	OGFWD
	Denotes a Profile Segment for Premises with wind generation, applicable to ESI IDs that meet the criteria on the DG tab
	Segment Assignment tab

	
	RESHIWR kWhp
	Denotes the sum of the kWh interval values for the RESHIWR backcasted profiles of a specific weather zone for the specific days in the Meter Reading Period p.
	Segment Assignment tab

	
	RESHIWR Year Use
	Denotes the sum of the RESHIWR kWhp for a specific weather zone for each year value of an ESI ID.
	
	Segment Assignment tab

	
	Residential (RES)
	Profile Group designation for ESI IDs served within a residential rate class.
	
	

	
	RESLOWR kWhp
	Denotes the sum of the kWh interval values for the RESLOWR backcasted profiles for a specific weather zone for the specific days in the Meter Reading Period p.
	Segment Assignment tab

	
	RESLOWR Year Use
	Denotes the sum of the RESLOWR kWhp for a specific weather zone for each year value of an ESI ID.
	
	Segment Assignment tab

	
	Rounding
	The following applies to all numbers that are to be rounded to two decimal places.  If the digit in the thousandth's place of a number is four or less, all digits to the right of the hundredth's place are dropped and the digit in the hundredth's place does not change.  For example, rounding 1.574 to the nearest hundredth's place would yield 1.57.  If the digit in the thousandth's place is five through nine, all digits to the right of the hundredth's place are dropped and the remaining number is increased by 0.01.  The number 1.235 rounded to the hundredth's place is 1.24.  Some more examples:

	
	
	
	original
	rounded
	original
	rounded
	
	

	
	
	
	number
	number
	number
	number
	
	

	
	
	
	1.7774
	
	1.78
	
	1.320
	
	1.32
	
	
	

	
	
	
	1.024
	
	1.02
	
	1.156
	
	1.16
	
	
	

	
	
	
	1.232
	
	1.23
	
	1.999
	
	2.00
	
	
	

	
	
	
	1.57482
	
	1.57
	
	1.645
	
	1.64
	
	
	

	
	
	
	1.379
	
	1.38
	
	1.258
	
	1.26
	
	
	

	
	S RESHIWR kWhp
	Scaled RESHIWR kWhP calculated by multiplying RESHIWR kWhP by the ESI ID Year Use and dividing by the RESHIWR Year Use.
	Segment Assignment tab

	
	S RESLOWR kWhp
	Scaled RESLOWR kWhP calculated by multiplying RESLOWR kWhP by the ESI ID Year Use and dividing by the RESLOWR Year Use.
	Segment Assignment tab

	
	Season
	Refers to the classification of Shoulder or Winter for each meter reading within the Usage Time Period of each ESI ID.

	
	Shoulder
	Refers to a meter read which falls between September 21 and November 15 inclusive or between March 15 and May 10 inclusive.  

	
	Usage Month
	Each Usage Month corresponds with a calendar month and is a combination of one or more Usage Periods for the purpose of applying usage and demand values in a consistent manner. 

	
	Usage Period
	The time period that data from a meter read encompasses.  The Usage Period covers the Usage Period Start Time through the Usage Period Stop Time.  

	
	Usage Period Start Time
	A Usage Period begins at 00:00:00 (midnight) of the Meter Read Start Date.  This convention helps to facilitate a smooth transfer of ESI ID 'ownership' between CRs, should a transfer occur (a transfer of ownership takes effect at 00:00:00).   

	
	Usage Period Stop Time
	A Usage Period ends at 23:59:59 on the DAY BEFORE the Meter Read Stop Date.
	
	

	
	Usage Time Period
	Refers to a specific set of Meter Read Periods used to determine Residential Profile ID assignments.
	
	

	
	WS
	Weather Sensitive designation of the Weather Sensitivity Code.  (calculated by ERCOT)
	
	Protocols Section 11.4.3.1

	
	Winter
	Refers to a meter read which falls between November 16 and March 14 inclusive.  
	
	

	
	Winter Max ADUsep
	For the ESI ID's entire Usage Time Period, identify the highest ADUsep of all meter readings classified as a Winter season.


Appendix D, Profile Decision Tree – “Segment Assignment” worksheet
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	III.  Business (BUS)
	
	
	
	
	
	
	
	
	
	
	

	
	
	Assignment Year for Average Load Factor calculations: The previous calendar year (January through December) will be used to calculate the Average Load Factor.

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	For each ESI ID, assign the applicable Profile Segment based on the steps below.  Because the steps below are not mutually exclusive, it is necessary to step through each of the following in the order listed, for each ESI ID, until an applicable case is found.  Once an applicable case has been found follow the instructions in 'E' below for ESI IDs that have Distributed Generation (per the DG tab).

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	A.  Assign the an LRG or IDRRQ ('IDR required')  Profile Segment to all BUS ESI IDs required to have an IDR Meter, per Section 18 of the ERCOT Nodal Protocols.

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	B.  Assign the OGFLT (Oil & Gas Flat) Profile Segment to:
	
	
	
	
	

	
	
	
	
	
	ESI IDs for which ERCOT has informed the TDSP that OGFLT should be assigned per the Oil & Gas tab.

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	C.  Assign the NODEM Profile Segment for non-residential ESI IDs which are not billed demand.
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	D.  Determine the Average Load Factor (AvgLF) for ESI IDs that were not assigned a Profile Segment in Steps 1, 2, or 3 above.

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	1.  Determine Usage Month values (ActiveDaysm, kWDaysm, kWhm, MaxkWm, and ADUsem) for each ESI ID for the 12 months of the Assignment Year, which is listed near the beginning of Section III. 

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	2.  Compute the Average Hourly Usage (AHUsem) for the Usage Months of the Assignment Year.

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	where 
	kWhm = consumption in kilowatthours in Usage Month m, and
	

	
	
	
	
	
	ActiveDaysm = Number of Active Days in Usage Month m.
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	        * Round to two decimal places, per the Rounding instructions on the Definitions tab.
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	3.  Compute the Average Load Factor (AvgLF) as shown below for the Usage Months of the current Assignment Year.  TDSPs that measure kVA at the ESI ID level should reference the 'kVA to kW' tab before proceeding.  The Average Load Factor is a weighted average of the individual monthly load factors, where demand levels are used to define the weights (presented in a mathematically equivalent calculation below).  AHUsem and MaxkWm values are required for each of the 12 months of the current Assignment Year in order to calculate AvgLF. 

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	where
	AHUsem = Average Hourly Use in Usage Month m as previously defined, and

	
	
	
	
	
	MaxkWm = Maximum metered kW Demand in Usage Month m, as defined on the Usage Month methodology tab.

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	        * Round to two decimal places, per the Rounding instructions on the Definitions tab.

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	4.  For each ESI ID, assign the appropriate Profile Segment based on A thru G below.  Because A thru G below are not mutually exclusive, it is necessary to step through each of the following in the order listed, for each ESI ID, until an applicable case is found.  (Please note that the breakpoint values below are subject to change periodically.)

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	a.
	If there is no existing assignment then
	
	
	
	
	

	
	
	
	
	
	
	if the required data were not available to calculate the AvgLF** then 
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if data were available (e.g., for Opt-in entities) to calculate the AvgLF then

	
	
	
	
	
	
	
	if the AvgLF < 0.40 then 
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	else if 0.40 ≤ AvgLF ≤ 0.60 then
	
	
	
	
	

	
	
	
	
	
	
	
	
	assign MEDLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	else assign HILF.
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	b.
	If the existing assignment is LOLF (or a DG variation, such as LOWD) then 
	

	
	
	
	
	
	
	if the required data were not available to calculate the AvgLF** then 
	

	
	
	
	
	
	
	
	do not change assignment from LOLF;
	
	
	

	
	
	
	
	
	
	else if the AvgLF < 0.40 then 
	
	
	
	
	
	

	
	
	
	
	
	
	
	do not change assignment from LOLF;
	
	
	

	
	
	
	
	
	
	else if 0.40 ≤ AvgLF ≤ 0.60 then
	
	
	
	
	

	
	
	
	
	
	
	
	assign MEDLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else assign HILF.
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	c.
	If the existing assignment is MEDLF (or a DG variation) then 
	

	
	
	
	
	
	
	if the required data were not available to calculate the AvgLF** then 
	

	
	
	
	
	
	
	
	do not change assignment from MEDLF;
	
	
	

	
	
	
	
	
	
	else if the AvgLF < 0.40 then 
	
	
	
	
	
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if 0.40 ≤ AvgLF ≤ 0.60 then
	
	
	
	
	

	
	
	
	
	
	
	
	do not change assignment from MEDLF;
	
	
	

	
	
	
	
	
	
	else assign HILF.
	
	
	
	
	
	
	


	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	d.
	If the existing assignment is HILF (or a DG variation) then 
	
	

	
	
	
	
	
	
	if the required data were not available to calculate the AvgLF** then 
	

	
	
	
	
	
	
	
	do not change assignment from HILF;
	
	
	
	

	
	
	
	
	
	
	else if the AvgLF < 0.40 then 
	
	
	
	
	
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if 0.40 ≤ AvgLF ≤ 0.60 then
	
	
	
	
	

	
	
	
	
	
	
	
	assign MEDLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else do not change assignment from HILF.
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	e.
	If the existing assignment is LRG or IDRRQ then 
	
	
	
	
	

	
	
	
	
	
	
	if the required data were not available to calculate the AvgLF** then 
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if the AvgLF < 0.40 then 
	
	
	
	
	
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if 0.40 ≤ AvgLF ≤ 0.60 then
	
	
	
	
	

	
	
	
	
	
	
	
	assign MEDLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else assign HILF.
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	f.
	If the existing assignment is NODEM (or a DG variation) then 
	

	
	
	
	
	
	
	if the required data were not available to calculate the AvgLF** then 
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if the AvgLF < 0.40 then 
	
	
	
	
	
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if 0.40 ≤ AvgLF ≤ 0.60 then
	
	
	
	
	

	
	
	
	
	
	
	
	assign MEDLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else assign HILF.
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	g.
	If the existing assignment is neither LOLF, MEDLF, HILF, LRG, IDRRQ, nor NODEM then 

	
	
	
	
	
	
	if the required data were not available to calculate the AvgLF** then 
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if the AvgLF < 0.40 then 
	
	
	
	
	
	

	
	
	
	
	
	
	
	assign LOLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else if 0.40 ≤ AvgLF ≤ 0.60 then
	
	
	
	
	

	
	
	
	
	
	
	
	assign MEDLF;
	
	
	
	
	
	
	

	
	
	
	
	
	
	else assign HILF.
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	** or if the mathematical calculation of the AvgLF is undefined due to a zero (0) in the denominator

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	E.
	Assign a DG Profile Segment as directed by ERCOT, per the DG tab.
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	1.
	If the ESI ID would otherwise be assigned LRG or IDRRQ then
	
	
	

	
	
	
	
	
	assign LRG or IDRRQ respectively;
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	2.
	Else if the ESI ID has any PV generation then
	
	
	
	
	

	
	
	
	
	
	if segment is determined to be HILF then assign HIPV;
	
	

	
	
	
	
	
	else if segment is determined to be MEDLF then assign MEDPV;
	

	
	
	
	
	
	else if segment is determined to be LOLF then assign LOPV;
	

	
	
	
	
	
	else if segment is determined to be NODEM then assign NODPV;
	

	
	
	
	
	
	else if segment is determined to be OGFLT then assign OGFPV;
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	3.
	Else if the ESI ID has wind generation then
	
	
	
	
	

	
	
	
	
	
	if segment is determined to be HILF then assign HIWD;
	
	

	
	
	
	
	
	else if segment is determined to be MEDLF then assign MEDWD;
	

	
	
	
	
	
	else if segment is determined to be LOLF then assign LOWD;
	

	
	
	
	
	
	else if segment is determined to be NODEM then assign NODWD;
	

	
	
	
	
	
	else if segment is determined to be OGFLT then assign OGFWD.;
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	4.
	Else if the ESI ID has other DG then
	
	
	
	
	
	

	
	
	
	
	
	if segment is determined to be HILF then assign HIDG;
	
	

	
	
	
	
	
	else if segment is determined to be MEDLF then assign MEDDG;
	

	
	
	
	
	
	else if segment is determined to be LOLF then assign LODG;
	

	
	
	
	
	
	else if segment is determined to be NODEM then assign NODDG;
	

	
	
	
	
	
	else if segment is determined to be OGFLT then assign OGFDG.
	

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	


Appendix D, Profile Decision Tree – “DG” worksheet
Distributed Generation Request Template Instructions

For ESI IDs that have a Distributed Generation (DG) capacity less than or equal to the DG registration threshold, have signed an interconnection agreement with the TDSP, and are not otherwise required to be assigned the LRG or IDRRQ Profile Segment, the TDSP is required to provide ERCOT (ERCOTLoadProfilingDepartment@ercot.com) with documentation of the following for each applicable ESI ID:

Appendix D, Profile Decision Tree – “Valid Profile IDs” worksheet
Insert the following list of BUSLRG Profile IDs into the table.

	IDR
	NWS
	NOTOU
	BUSLRG_COAST_IDR_NWS_NOTOU

	IDR
	WS
	NOTOU
	BUSLRG_COAST_IDR_WS_NOTOU

	IDR
	NWS
	NOTOU
	BUSLRG _EAST_IDR_NWS_NOTOU

	IDR
	WS
	NOTOU
	BUSLRG _EAST_IDR_WS_NOTOU

	IDR
	NWS
	NOTOU
	BUSLRG _FWEST_IDR_NWS_NOTOU

	IDR
	WS
	NOTOU
	BUSLRG _FWEST_IDR_WS_NOTOU

	IDR
	NWS
	NOTOU
	BUSLRG _NCENT_IDR_NWS_NOTOU

	IDR
	WS
	NOTOU
	BUSLRG _NCENT_IDR_WS_NOTOU

	IDR
	NWS
	NOTOU
	BUSLRG _NORTH_IDR_NWS_NOTOU

	IDR
	WS
	NOTOU
	BUSLRG _NORTH_IDR_WS_NOTOU

	IDR
	NWS
	NOTOU
	BUSLRG _SCENT_IDR_NWS_NOTOU

	IDR
	WS
	NOTOU
	BUSLRG _SCENT_IDR_WS_NOTOU

	IDR
	NWS
	NOTOU
	BUSLRG _SOUTH_IDR_NWS_NOTOU

	IDR
	WS
	NOTOU
	BUSLRG _SOUTH_IDR_WS_NOTOU

	IDR
	NWS
	NOTOU
	BUSLRG _WEST_IDR_NWS_NOTOU

	IDR
	WS
	NOTOU
	BUSLRG _WEST_IDR_WS_NOTOU
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