|  |  |  |  |
| --- | --- | --- | --- |
| NPRR Number | [1052](http://www.ercot.com/mktrules/issues/NPRR1052) | NPRR Title | Load Zone Pricing for Settlement Only Storage Prior to NPRR995 Implementation |
| Date of Decision | | November 11, 2020 | |
| Action | | Recommended Approval | |
| Timeline | | Normal | |
| Proposed Effective Date | | To be determined | |
| Priority and Rank Assigned | | To be determined | |
| Nodal Protocol Sections Requiring Revision | | 6.6.3.2, Real-Time Energy Imbalance Payment or Charge at a Load Zone  6.6.3.9, Real-Time Payment or Charge for Energy from a Settlement Only Distribution Generator (SODG) or a Settlement Only Transmission Generator (SOTG)  9.19.1, Default Uplift Invoices  16.5, Registration of a Resource Entity | |
| Related Documents Requiring Revision/Related Revision Requests | | None | |
| Revision Description | | This Nodal Protocol Revision Request (NPRR) ensures that Energy Storage Systems (ESSs) that are registered with ERCOT as Settlement Only Generators (SOGs) will continue to have their injections and withdrawals settled at Load Zone pricing until nodal pricing for injections and withdrawals is approved and implemented. This NPRR establishes the following Settlement and metering provisions for Energy Storage Systems (ESSs) that are registered as Settlement Only Generators (SOGs) pending the approval and implementation of NPRR995, RTF-6 Create Definition and Terms for Settlement Only Energy Storage:   * For any site with one or more ESS SOGs where the ESSs’ rated capacity constitutes more than 50% of the site’s overall nameplate capacity, energy injections and withdrawals will be settled at the Load Zone price; and * For any site with one or more ESS SOGs where the ESSs’ rated capacity constitutes 50% or less of the site’s overall nameplate capacity, energy injections will be settled at the applicable nodal price and withdrawals will be settled at the Load Zone price. This is the only scenario in which zonal/nodal arbitrage is possible. ERCOT expects that such configurations will be minimal, and emphasizes that this arbitrage possibility will expire upon implementation of NPRR995.   ERCOT proposes that the effective date of this NPRR should be simultaneous with system implementation of NPRR917, Nodal Pricing for Settlement Only Distribution Generators (SODGs) and Settlement Only Transmission Generators (SOTGs), and that all provisions in this NPRR should expire upon implementation of NPRR995. | |
| Reason for Revision | | Addresses current operational issues.  Meets Strategic goals (tied to the [ERCOT Strategic Plan](http://www.ercot.com/content/wcm/lists/144926/ERCOT_Strategic_Plan_2019-2023.pdf) or directed by the ERCOT Board).  Market efficiencies or enhancements  Administrative  Regulatory requirements  Other: (explain)  *(please select all that apply)* | |
| Business Case | | NPRR995 introduces the concept of a Settlement Only Energy Storage System (SOESS) and, if 10/19/20 ERCOT comments to NPRR995 are approved, will provide for nodal Settlement of SOESS withdrawals and injections. Until NPRR995 is implemented—which could take several years—an ESS may be registered as an SOG and receive nodal settlement for injections pursuant to NPRR917, which is expected to be implemented in 2021. However, because NPRR917 did not address ESSs, withdrawals by SOESSs would still be settled at zonal prices until NPRR995 is implemented. This would result in these ESSs having their injections settled at nodal pricing and their withdrawals settled at Load Zone pricing for the period between the implementation of NPRR917 and the implementation of NPRR995. This NPRR will avoid the possibility of inappropriate arbitrage—i.e., zonal charging and nodal discharging—for Settlement-only ESSs during this period. This is consistent with the original language in NPRR995, as submitted by Broad Reach Power on behalf of the Resource Definition Task Force (RTF). | |
| Credit Work Group Review | | To be determined | |
| PRS Decision | | On 11/11/20, PRS unanimously voted via roll call to recommend approval of NPRR1052 as submitted. All Market Segments were present for the vote. | |
| Summary of PRS Discussion | | On 11/11/20, there was no discussion. | |

|  |  |
| --- | --- |
| Sponsor | |
| Name | Sandip Sharma |
| E-mail Address | [Sandip.sharma@ercot.com](mailto:Sandip.sharma@ercot.com) |
| Company | ERCOT |
| Phone Number | 512-248-4298 |
| Cell Number |  |
| Market Segment | Not applicable |

|  |  |
| --- | --- |
| **Market Rules Staff Contact** | |
| **Name** | Cory Phillips |
| **E-Mail Address** | [cory.phillips@ercot.com](mailto:cory.phillips@ercot.com) |
| **Phone Number** | 512-248-6464 |

|  |  |
| --- | --- |
| **Comments Received** | |
| Comment Author | **Comment Summary** |
| None |  |

|  |
| --- |
| **Market Rules Notes** |

Please note the following NPRR(s) also propose revisions to the following section(s):

* NPRR995, RTF-6 Create Definition and Terms for Settlement Only Energy Storage
  + Section 6.6.3.9
* NPRR1010, RTC – NP 6: Adjustment Period and Real-Time Operations
  + Section 6.6.3.9
* NPRR1012, RTC – NP 9: Settlement and Billing
  + Section 9.19.1
* NPRR1043, Clarification of NPRR986 Language Related to Wholesale Storage Load
  + Section 6.6.3.2

|  |
| --- |
| Proposed Protocol Language Revision |

**6.6.3.2 Real-Time Energy Imbalance Payment or Charge at a Load Zone**

(1) The payment or charge to each QSE for Energy Imbalance Service is calculated based on the Real-Time Settlement Point Price for the following amounts at a particular Load Zone Settlement Point:

(a) The amount of its Self-Schedules with sink specified at the Settlement Point; plus

(b) The amount of its DAM Energy Bids cleared in the DAM at the Settlement Point; plus

(c) The amount of its Energy Trades at the Settlement Point where the QSE is the buyer; minus

(d) The amount of its Self-Schedules with source specified at the Settlement Point; minus

(e) The amount of its energy offers cleared in the DAM at the Settlement Point; minus

(f) The amount of its Energy Trades at the Settlement Point where the QSE is the seller; minus

(g) Its AML at the Settlement Point; plus

|  |
| --- |
| ***[NPRR986: Replace item (g) above with the following upon system implementation:]***  (g) Its AML at the Settlement Point excluding ESR Load that is not WSL; plus |

(h) The aggregated generation of its Settlement Only Generators (SOGs) in the Load Zone.

|  |
| --- |
| ***[NPRR917: Replace item (h) above with the following upon system implementation:]***  (h) The aggregated generation of its Settlement Only Transmission Self-Generators (SOTSGs) at the Settlement Point. SOTSG sites will be represented as a single unit in the ERCOT Settlement system.  (i) The aggregated generation of its Settlement Only Distribution Generators (SODGs) and Settlement Only Transmission Generators (SOTGs) that have elected to retain Load Zone pricing in accordance with Section 6.6.3.9, Real-Time Payment or Charge for Energy from a Settlement Only Distribution Generator (SODG) or a Settlement Only Transmission Generator (SOTG). SODG and SOTG sites will be represented as a single unit in the ERCOT Settlement system.  (j) The aggregated generation of its Energy Storage System (ESS) SODGs and SOTGs at sites where the ESS capacity constitutes more than 50% of the total SODG or SOTG nameplate capacity, as confirmed by an affidavit submitted by the Resource Entity for the site. SODG and SOTG sites will be represented as a single unit in the ERCOT Settlement system. |

(2) The payment or charge to each QSE for Energy Imbalance Service at a Load Zone for a given 15-minute Settlement Interval is calculated as follows:

**RTEIAMT *q, p* = (-1) \* {[RTSPP *p* \* [(SSSK *q, p* \* ¼) + (DAEP *q, p* \* ¼) + (RTQQEP *q, p* \* ¼) – (SSSR *q, p* \* ¼) – (DAES *q, p* \* ¼) – (RTQQES *q, p* \* ¼)]] + [RTSPPEW *p* \* (RTMGNM *q, p* – RTAML *q, p*)]}**

|  |
| --- |
| ***[NPRR917 and NPRR986: Replace applicable portions of the formula “RTEIAMT q, p” above with the following upon system implementation:]***  **RTEIAMT *q, p* = (-1) \* {[RTSPP *p* \* [(SSSK *q, p* \* ¼) + (DAEP *q, p* \* ¼) + (RTQQEP *q, p* \* ¼) – (SSSR *q, p* \* ¼) – (DAES *q, p* \* ¼) – (RTQQES *q, p* \* ¼)]] + [RTSPPEW *p* \* (RTMGSOGZ *q, p* – (RTAML *q, p* – RTAMLESRNW *q, p*))]}** |

And

**LZIMBAL *q, p =* (SSSK *q, p* \* ¼) + (DAEP *q, p* \* ¼) + (RTQQEP *q, p* \* ¼) – (SSSR *q, p* \* ¼) – (DAES *q, p* \* ¼) – (RTQQES *q, p* \* ¼) – RTAML *q, p* + RTMGNM *q, p***

|  |
| --- |
| ***[NPRR917 and NPRR986: Replace applicable portions of the formula “LZIMBAL q, p” above with the following upon system implementation:]***  **LZIMBAL *q, p =* (SSSK *q, p* \* ¼) + (DAEP *q, p* \* ¼) + (RTQQEP *q, p* \* ¼) – (SSSR *q, p* \* ¼) – (DAES *q, p* \* ¼) – (RTQQES *q, p* \* ¼) – (RTAML *q, p* –RTAMLESRNW *q, p*) + RTMGSOGZ *q, p*** |

The above variables are defined as follows:

| **Variable** | **Unit** | **Description** |
| --- | --- | --- |
| RTEIAMT *q, p* | $ | *Real-Time Energy Imbalance Amount per QSE per Settlement Point*—The payment or charge to QSE *q* for Real-Time Energy Imbalance Service at Settlement Point *p*, for the 15-minute Settlement Interval. |
| RTSPP *p* | $/MWh | *Real-Time Settlement Point Price per Settlement Point*—The Real-Time Settlement Point Price at Settlement Point *p*, for the 15-minute Settlement Interval. |
| LZIMBAL *q, p* | MWh | *Load Zone Energy Imbalance per QSE per Settlement Point*—The Load Zone volumetric imbalance for QSE *q* for Real-Time Energy Imbalance Service at Settlement Point *p*, for the 15-minute Settlement Interval. |
| RTSPPEW *p* | $/MWh | *Real-Time Settlement Point Price Energy-Weighted*⎯The Real-Time Settlement Point Price at the Settlement Point *p*, for the 15-minute Settlement Interval that is weighted by the State Estimated Load for the Load Zone of each SCED interval within the 15-minute Settlement Interval. |
| RTAML *q, p* | MWh | *Real-Time Adjusted Metered Load per QSE per Settlement Point*—The sum of the AML at the Electrical Buses that are included in Settlement Point *p* represented by QSE *q* for the 15-minute Settlement Interval. |
| |  |  |  |  | | --- | --- | --- | --- | | ***[NPRR986: Insert the variable “RTAMLESRNW q, p” below upon system implementation:]***   |  |  |  | | --- | --- | --- | | RTAMLESRNW *q, p* | MWh | *Real-Time Adjusted Metered Load for ESR Non-WSL per QSE per Settlement Point*—The sum of the AML for the ESR Load that is not WSL at the Electrical Buses that are included in Settlement Point *p* represented by QSE *q* for the 15-minute Settlement Interval, represented as a positive value. | | | | |
| SSSK *q, p* | MW | *Self-Schedule with Sink at Settlement Point per QSE per Settlement Point*—The QSE *q*’s Self-Schedule with sink at Settlement Point *p*, for the 15-minute Settlement Interval. |
| DAEP *q, p* | MW | *Day-Ahead Energy Purchase per QSE per Settlement Point*—The QSE *q*’s DAM Energy Bids at Settlement Point *p* cleared in the DAM, for the hour that includes the 15-minute Settlement Interval. |
| RTQQEP *q, p* | MW | *Real-Time QSE-to-QSE Energy Purchase per QSE per Settlement Point*⎯The amount of MW bought by QSE *q* through Energy Trades at Settlement Point *p*, for the 15-minute Settlement Interval. |
| SSSR *q, p* | MW | *Self-Schedule with Source at Settlement Point per QSE per Settlement Point*—The QSE *q*’s Self-Schedule with source at Settlement Point *p*, for the 15-minute Settlement Interval. |
| DAES *q, p* | MW | *Day-Ahead Energy Sale per QSE per Settlement Point*—The QSE *q*’s energy offers at Settlement Point *p* cleared in the DAM, for the hour that includes the 15-minute Settlement Interval. |
| RTQQES *q, p* | MW | *Real-Time QSE-to-QSE Energy Sale per QSE per Settlement Point*⎯The amount of MW sold by QSE *q* through Energy Trades at Settlement Point *p*, for the 15-minute Settlement Interval. |
| RTMGNM *q, p* | MWh | *Real-Time Metered Generation from Settlement Only Generators per QSE per Settlement Point*—The total Real-Time energy produced by SOGs represented by QSE *q* in Load Zone Settlement Point *p*, for the 15-minute Settlement Interval. |
| |  |  |  |  | | --- | --- | --- | --- | | ***[NPRR917: Replace the variable “RTMGNM q, p” above with the following upon system implementation:]***   |  |  |  | | --- | --- | --- | | RTMGSOGZ *q, p* | MWh | *Real-Time Metered Generation from Settlement Only Generators Zonal per QSE per Settlement Point*—The total Real-Time energy produced by SOTSGs represented by QSE *q* in Load Zone Settlement Point *p*, for the 15-minute Settlement Interval. MWh quantities for ESS SODGs and SOTGs at sites where the ESS capacity constitutes more than 50% of the total SOG nameplate capacity will be included in this value. MWh quantities for SODGs and SOTGs that have opted out of nodal pricing pursuant to Section 6.6.3.9 will also be included in this value. | | | | |
| *q* | none | A QSE. |
| *p* | none | A Load Zone Settlement Point. |

(3) The total net payments and charges to each QSE for Energy Imbalance Service at all Load Zones for the 15-minute Settlement Interval is calculated as follows:

**RTEIAMTQSETOT *q* = RTEIAMT *q, p***

The above variables are defined as follows:

|  |  |  |
| --- | --- | --- |
| **Variable** | **Unit** | **Definition** |
| RTEIAMTQSETOT *q* | $ | *Real-Time Energy Imbalance Amount QSE Total per QSE*⎯The total net payments and charges to QSE *q* for Real-Time Energy Imbalance Service at all Load Zone Settlement Points for the 15-minute Settlement Interval. |
| RTEIAMT *q, p* | $ | *Real-Time Energy Imbalance Amount per QSE per Settlement Point*—The charge to QSE *q* for Real-Time Energy Imbalance Service at Settlement Point *p*, for the 15-minute Settlement Interval. |
| *q* | none | A QSE. |
| *p* | none | A Load Zone Settlement Point. |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***[NPRR917: Insert Section 6.6.3.9 below upon system implementation:]***  **6.6.3.9 Real-Time Payment or Charge for Energy from a Settlement Only Distribution Generator (SODG) or a Settlement Only Transmission Generator (SOTG)**  (1) The payment or charge to each QSE for energy from an SODG or an SOTG shall be based on an identified nodal energy price, RTESOGPR, as described in this subsection, with the following exceptions:  (a) An SODG or SOTG that has opted out of nodal pricing as described in paragraph (5) below; or  (b) Any site with one or more ESS SODGs or SOTGs where the ESS capacity constitutes more than 50% of the site’s total SOG nameplate capacity.  (2) For an SODG, the price used as the basis for the 15-minute Real-Time price calculation is the time-weighted price at the Electrical Bus associated with this mapped Load in the Network Operations Model. For an SOTG, the price used as the basis for the 15-minute Real-Time price calculation is the time-weighted price at the Electrical Bus as determined by ERCOT in review of the meter location of the SOTG in the Network Operations Model. The outflow of energy into the grid as measured by each Settlement Meter for the 15-minute Settlement Interval shall be priced at the nodal energy price (RTESOGPR, as defined in paragraph (3) below), and the inflow of energy is treated as Load and shall be settled accordingly at the zonal energy price (the Load Zone Settlement Point Price). SODG and SOTG sites will be represented as a single unit in the ERCOT Settlement system.  (3) For an SODG or an SOTG, the total payment or charge for each 15-minute Settlement Interval shall be calculated as follows:  **RTESOGSAMT *q,* *gsc* = (-1) \* [( RTESOGPR *b* \* OFSOG *q, gsc, b*)]**  **Where the price for the SOTG or SODG is determined as follows:**  **RTESOGPR *b* = Max [-$251, ((SDWF *y* \* RTLMP *b, y*) + RTRSVPOR + RTRDP)]**  Where:  RTRSVPOR = (SDWF *y* \* RTORPA *y*)  RTRDP = (SDWF *y* \* RTORDPA *y*)  SDWF *y* = TLMP *y* / TLMP *y*  The above variables are defined as follows:   | **Variable** | **Unit** | **Description** | | --- | --- | --- | | RTESOGSAMT*q,**gsc* | $ | *Real-Time Energy for SODG and SOTG Site Amount* —The total payment or charge to QSE *q* for SODG or SOTG site *gsc* for the 15-minute Settlement Interval. | | RTESOGPR *b* | $/MWh | *Real-Time Price for the Energy Metered for each SODG or SOTG Site* ⎯The Real-Time price at Electrical Bus *b* for the Settlement Meter for the SODG or SOTG site for the 15-minute Settlement Interval. | | OFSOG *q,* *gsc, b* | MWh | *Outflow as Measured for an SODG or SOTG Site* ⎯The outflow as measured by the Settlement Meter(s) at Electrical Bus *b* for SODG or SOTG site *gsc* represented by QSE *q*. | | RTRSVPOR | $/MWh | *Real-Time Reserve Price for On-Line Reserves*⎯The Real-Time Reserve Price for On-Line Reserves for the 15-minute Settlement Interval. | | RTORPA*y* | $/MWh | *Real-Time On-Line Reserve Price Adder per interval*⎯The Real-Time On-Line Reserve Price Adder for the SCED interval *y*. | | RTRDP | $/MWh | *Real-Time On-Line Reliability Deployment Price* ⎯The Real-Time price for the 15-minute Settlement Interval, reflecting the impact of reliability deployments on energy prices that is calculated from the Real-Time On-Line Reliability Deployment Price Adder. | | RTORDPA*y* | $/MWh | *Real-Time On-Line Reliability Deployment Price Adder* ⎯The Real-Time Price Adder that captures the impact of reliability deployments on energy prices for the SCED interval *y*. | | SDWF *y* | None | *SCED Duration Weighting Factor per interval*⎯The weight used in the SODG or SOTG price calculation for the portion of the SCED interval *y* within the Settlement Interval. | | RTLMP *b, y* | $/MWh | *Real-Time Locational Marginal Price at bus per interval*⎯The Real-Time LMP at Electrical Bus *b*, for the SCED interval *y*. | | TLMP *y* | second | *Duration of SCED interval per interval*⎯The duration of the SCED interval *y* within the Settlement Interval. | | *gsc* | none | A generation site code. | | *b* | none | An Electrical Bus. | | *y* | None | A SCED interval in the 15-minute Settlement Interval. The summation is over the total number of SCED runs that cover the 15-minute Settlement Interval. |   (4) The total net payments and charges to each QSE for energy from SODGs and SOTGs for the 15-minute Settlement Interval is calculated as follows:  **RTESOGAMTQSETOT *q* = RTESOGSAMT *q, gsc***  The above variables are defined as follows:   | **Variable** | **Unit** | **Definition** | | --- | --- | --- | | RTESOGAMTQSETOT *q* | $ | *Real-Time Energy Payment or Charge per QSE for Energy from SODGs and SOTGs* —The payment or charge to QSE *q* for Real-Time energy from SODGs and SOTGs, for the 15-minute Settlement Interval. | | RTESOGSAMT *q, gsc* | $ | *Real-Time Energy for SODG and SOTG Site Amount* —The total payment or charge to QSE *q* for an SODG or SOTG site *gsc* for the 15-minute Settlement Interval. | | *q* | none | A QSE. | | *gsc* | none | A generation site code. |   (5) Notwithstanding anything else in this Section except paragraphs (6) and (7) below, a Resource Entity may opt out of nodal pricing and continue Load Zone Settlement for any SODG or SOTG if, by January 1, 2019, the SODG or SOTG was operational or was subject to a Power Purchase or Tolling Agreement (PPA) or Transmission and/or Distribution Service Provider (TDSP) interconnection agreement, or had an executed agreement with a developer. By December 31, 2019, the Resource Entity must submit a properly completed Section 23, Form N, Pricing Election for Settlement Only Distribution Generators and Settlement Only Transmission Generators. Any SODG or SOTG relying on a PPA or TDSP interconnection agreement or agreement with a developer must also have achieved Initial Synchronization for the full Resource capacity before June 1, 2020 to be eligible to opt out of nodal pricing. A Resource Entity must provide ERCOT documented proof of any PPA, TDSP interconnection agreement, or developer agreement that it relies on as a basis for any election under this paragraph. This election is valid through the earlier of December 31, 2029 or the date on which the election is revoked pursuant to paragraph (8) of this Section. On January 1, 2030, all SODGs and SOTGs will be subject to nodal pricing.  (6) For any SODG or SOTG for which the applicable Resource Entity has elected to opt out of nodal pricing, ERCOT shall settle the output of the SODG or SOTG using the Load Zone Settlement Point Price for the duration of the opt-out period so long as the SODG or SOTG is not physically modified for any purpose, including to increase the capacity of the unit or change the fuel type of the unit, except as necessary for routine maintenance or repairs to address normal wear and tear.  (7) If at any time ERCOT determines that the SODG or SOTG fails to meet the opt-out conditions in paragraph (6) above, ERCOT shall settle the output of the SODG or SOTG at the applicable nodal price as soon as practicable after providing written notice to the affected Resource Entity.  (8) A Resource Entity that has opted out of nodal pricing for one or more SODGs or SOTGs pursuant to paragraph (5) of this Section may withdraw that election and begin receiving applicable nodal pricing for one or more such generators by submitting a properly completed election form (Section 23, Form N). An election of nodal pricing is irrevocable. ERCOT will effectuate the transition of an SODG or SOTG to nodal pricing in ERCOT Settlement systems as soon as practicable. |

***9.19.1 Default Uplift Invoices***

(1) ERCOT shall collect the total short-pay amount for all Settlement Invoices for a month, less the total payments expected from a payment plan, from Qualified Scheduling Entities (QSEs) and CRR Account Holders. ERCOT must pay the funds it collects from payments on Default Uplift Invoices to the Entities previously short-paid. ERCOT shall notify those Entities of the details of the payment.

(2) Each Counter-Party’s share of the uplift is calculated using the best available Settlement data for each Operating Day in the month prior to the month in which the default occurred, and is calculated as follows:

**DURSCP*cp* = TSPA \* MMARS*cp***

Where:

MMARS *cp* = MMA *cp* / MMATOT

MMA *cp* = Max { ∑*mp* (URTMG *mp*+ URTDCIMP *mp*),

∑*mp* (URTAML *mp* + UWSLTOT *mp*),

∑*mp*URTQQES *mp*,

∑*mp* URTQQEP *mp*,

∑*mp* UDAES *mp*,

∑*mp* UDAEP *mp*,

∑*mp* (URTOBL *mp +* URTOBLLO *mp*),

∑*mp* (UDAOPT *mp*+ UDAOBL *mp*+UOPTS *mp*+UOBLS *mp*),

∑*mp* (UOPTP *mp*+ UOBLP *mp*)}

|  |
| --- |
| ***[NPRR917: Replace the formula “MMA cp” above with the following upon system implementation:]***  MMA *cp* = Max { ∑*mp* (URTMG *mp*+ URTDCIMP *mp*),  ∑*mp* (URTAML *mp* + UWSLTOT *mp*),  ∑*mp*URTQQES *mp*,  ∑*mp* URTQQEP *mp*,  ∑*mp* UDAES *mp*,  ∑*mp* UDAEP *mp*,  ∑*mp* (URTOBL *mp +* URTOBLLO *mp*),  ∑*mp* (UDAOPT *mp*+ UDAOBL *mp*+UOPTS *mp*+UOBLS *mp*),  ∑*mp* (UOPTP *mp*+ UOBLP *mp*),  ∑*mp* (USOGTOT *mp*)} |

MMATOT = ∑*cp* (MMA*cp*)

Where:

URTMG *mp* = ∑*p, r, i* (RTMG *mp, p, r, i*), excluding RTMG for RMR Resources and RTMG in Reliability Unit Commitment (RUC)-Committed Intervals for RUC-committed Resources

URTDCIMP *mp* = ∑*p, i* (RTDCIMP *mp, p, i*) / 4

URTAML *mp* = max(0,∑*p, i* (RTAML *mp, p, i*))

URTQQES *mp* = ∑*p, i* (RTQQES *mp, p, i*) / 4

URTQQEP *mp* = ∑*p, i* (RTQQEP *mp, p, i*) / 4

UDAES *mp* = ∑*p, h* (DAES *mp, p, h*)

UDAEP *mp* = ∑*p, h* (DAEP *mp, p, h*)

URTOBL *mp* = ∑*(j, k), h* (RTOBL*mp, (j, k), h*)

URTOBLLO *mp* = ∑*(j, k), h* (RTOBLLO*mp, (j, k), h*)

UDAOPT *mp* = ∑*(j, k), h* (DAOPT*mp, (j, k), h*)

UDAOBL *mp* = ∑*(j, k), h* (DAOBL*mp, (j, k), h*)

UOPTS *mp* = ∑*(j, k), h* (OPTS*mp, (j, k), h*)

UOBLS *mp* = ∑*(j, k), h* (OBLS*mp, (j, k), h*)

UOPTP *mp* = ∑*(j, k), h* (OPTP*mp, j, h*)

UOBLP *mp* = ∑*(j, k), h* (OBLP*mp, (j, k), h*)

UWSLTOT *mp* = (-1) \* ∑*r, b* (MEBL *mp, r, b*)

|  |
| --- |
| ***[NPRR917: Insert the formula “USOGTOT mp” below upon system implementation:]***  USOGTOT *mp* = ∑*gsc, b* (OFSOG *mp, gsc, b*) + ∑ *p, i* (RTMGSOGZ *mp, p, i*) |

The above variables are defined as follows:

| **Variable** | **Unit** | **Definition** |
| --- | --- | --- |
| DURSCP *cp* | $ | *Default Uplift Ratio Share per Counter-Party*—The Counter-Party’s pro rata portion of the total short-pay amount for all Day-Ahead Market (DAM) and Real-Time Market (RTM) Invoices for a month. |
| TSPA | $ | *Total Short Pay Amount*—The total short-pay amount calculated by ERCOT to be collected through the Default Uplift Invoice process. |
| MMARS *cp* | None | *Maximum MWh Activity Ratio Share*—The Counter-Party’s pro rata share of Maximum MWh Activity. |
| MMA *cp* | MWh | *Maximum MWh Activity*—The maximum MWh activity of all Market Participants represented by the Counter-Party in the DAM, RTM and CRR Auction for a month. |
| MMATOT | MWh | *Maximum MWh Activity Total*—The sum of all Counter-Party’s Maximum MWh Activity. |
| RTMG *mp, p, r, i* | MWh | *Real-Time Metered Generation per Market Participant per Settlement Point per Resource*—The Real-Time energy produced by the Generation Resource *r* represented by Market Participant *mp*, at Resource Node *p*, for the 15-minute Settlement Interval *i*, where the Market Participant is a QSE. |
| URTMG *mp* | MWh | *Uplift Real-Time Metered Generation per Market Participant*—The monthly sum of Real-Time energy produced by Generation Resources represented by Market Participant *mp*, excluding generation for RMR Resources and generation in RUC-Committed Intervals, where the Market Participant is a QSE assigned to the registered Counter-Party. |
| RTDCIMP *mp, p, i* | MW | *Real-Time DC Import per QSE per Settlement Point*—The aggregated Direct Current Tie (DC Tie) Schedule submitted by Market Participant *mp,* as an importer into the ERCOT System through DC Tie *p*, for the 15-minute Settlement Interval *i*, where the Market Participant is a QSE. |
| URTDCIMP *mp* | MW | *Uplift Real-Time DC Import per Market Participant*—The monthly sum of the aggregated DC Tie Schedule submitted by Market Participant *mp*, as an importer into the ERCOT System where the Market Participant is a QSE assigned to a registered Counter-Party. |
| RTAML *mp, p, i* | MWh | *Real-Time Adjusted Metered Load per Market Participant per Settlement Point*—The sum of the Adjusted Metered Load (AML) at the Electrical Buses that are included in Settlement Point *p* represented by Market Participant *mp* for the 15-minute Settlement Interval *i*, where the Market Participant is a QSE. |
| URTAML *mp* | MWh | *Uplift Real-Time Adjusted Metered Load per Market Participant*—The monthly sum of the AML represented by Market Participant *mp*, where the Market Participant is a QSE assigned to the registered Counter-Party. |
| RTQQES *mp, p, i* | MW | *QSE-to-QSE Energy Sale per Market Participant per Settlement Point*—The amount of MW sold by Market Participant *mp* through Energy Trades at Settlement Point *p* for the 15-minute Settlement Interval *i*, where the Market Participant is a QSE. |
| URTQQES *mp* | MWh | *Uplift QSE-to-QSE Energy Sale per Market Participant*—The monthly sum of MW sold by Market Participant *mp* through Energy Trades, where the Market Participant is a QSE assigned to the registered Counter-Party. |
| RTQQEP *mp, p, i* | MW | *QSE-to-QSE Energy Purchase per Market Participant per Settlement Point*—The amount of MW bought by Market Participant *mp* through Energy Trades at Settlement Point *p* for the 15-minute Settlement Interval *i*, where the Market Participant is a QSE. |
| URTQQEP *mp* | MWh | *Uplift QSE-to-QSE Energy Purchase per Market Participant*—The monthly sum of MW bought by Market Participant *mp* through Energy Trades, where the Market Participant is a QSE assigned to the registered Counter-Party. |
| DAES *mp, p, h* | MW | *Day-Ahead Energy Sale per Market Participant per Settlement Point per hour*—The total amount of energy represented by Market Participant *mp*’s cleared Three-Part Supply Offers in the DAM and cleared DAM Energy-Only Offers at Settlement Point *p*, for the hour *h*, where the Market Participant is a QSE. |
| UDAES *mp* | MWh | *Uplift Day-Ahead Energy Sale per Market Participant*—The monthly total of energy represented by Market Participant *mp*’s cleared Three-Part Supply Offers in the DAM and cleared DAM Energy-Only Offer Curves, where the Market Participant is a QSE assigned to the registered Counter-Party. |
| DAEP *mp, p, h* | MW | *Day-Ahead Energy Purchase per Market Participant per Settlement Point per hour*—The total amount of energy represented by Market Participant *mp*’s cleared DAM Energy Bids at Settlement Point *p* for the hour *h*, where the Market Participant is a QSE. |
| UDAEP *mp* | MWh | *Uplift Day-Ahead Energy Purchase per Market Participant*—The monthly total of energy represented by Market Participant *mp*’s cleared DAM Energy Bids, where the Market Participant is a QSE assigned to the registered Counter-Party. |
| RTOBL *mp, (j, k), h* | MW | *Real-Time Obligation per Market Participant per source and sink pair per hour*—The number of Market Participant *mp*’s Point-to-Point (PTP) Obligations with the source *j* and the sink *k* settled in Real-Time for the hour *h*, and where the Market Participant is a QSE. |
| URTOBL *mp* | MWh | *Uplift Real-Time Obligation per Market Participant*—The monthly total of Market Participant *mp*’s PTP Obligations settled in Real-Time, counting the quantity only once per source and sink pair, and where the Market Participant is a QSE assigned to the registered Counter-Party. |
| RTOBLLO *q, (j, k)* | MW | *Real-Time Obligation with Links to an Option per QSE per pair of source and sink*⎯The total MW of the QSE’s PTP Obligation with Links to an Option Bids cleared in the DAM and settled in Real-Time for the source *j* and the sink *k* for the hour. |
| URTOBLLO *q, (j, k)* | MW | *Uplift Real-Time Obligation with Links to an Option per QSE per pair of source and sink*⎯The monthly total of Market Participant *mp*’s MW of PTP Obligation with Links to Options Bids cleared in the DAM and settled in Real-Time for the source *j* and the sink *k* for the hour, where the Market Participant is a QSE assigned to the registered Counter-Party. |
| DAOPT *mp, (j, k), h* | MW | *Day-Ahead Option per Market Participant per source and sink pair per hour*⎯The number of Market Participant *mp*’s PTP Options with the source *j* and the sink *k* owned in the DAM for the hour *h*, and where the Market Participant is a CRR Account Holder. |
| UDAOPT *mp* | MWh | *Uplift Day-Ahead Option per Market Participant*⎯The monthly total of Market Participant *mp*’s PTP Options owned in the DAM, counting the ownership quantity only once per source and sink pair, and where the Market Participant is a CRR Account Holder assigned to the registered Counter-Party. |
| DAOBL *mp, (j, k), h* | MW | *Day-Ahead Obligation per Market Participant per source and sink pair per hour*—The number of Market Participant *mp*’s PTP Obligations with the source *j* and the sink *k* owned in the DAM for the hour *h*, and where the Market Participant is a CRR Account Holder. |
| UDAOBL *mp* | MWh | *Uplift Day-Ahead Obligation per Market Participant*⎯The monthly total of Market Participant *mp*’s PTP Obligations owned in the DAM, counting the ownership quantity only once per source and sink pair, where the Market Participant is a CRR Account Holder assigned to the registered Counter-Party. |
| OPTS *mp, (j, k), a, h* | MW | *PTP Option Sale per Market Participant per source and sink pair per CRR Auction per hour*—The MW quantity that represents the total of Market Participant *mp*’s PTP Option offers with the source *j* and the sink *k* awarded in CRR Auction *a*, for the hour *h*, where the Market Participant is a CRR Account Holder. |
| UOPTS *mp* | MWh | *Uplift PTP Option Sale per Market Participant*—The MW quantity that represents the monthly total of Market Participant *mp*’s PTP Option offers awarded in CRR Auctions, counting the awarded quantity only once per source and sink pair, where the Market Participant is a CRR Account Holder assigned to the registered Counter-Party. |
| OBLS *mp, (j, k), a, h* | MW | *PTP Obligation Sale per Market Participant per source and sink pair per CRR Auction per hour*—The MW quantity that represents the total of Market Participant *mp*’s PTP Obligation offers with the source *j* and the sink *k* awarded in CRR Auction *a*, for the hour *h*, where the Market Participant is a CRR Account Holder. |
| UOBLS *mp* | MWh | *Uplift PTP Obligation Sale per Market Participant*—The MW quantity that represents the monthly total of Market Participant *mp*’s PTP Obligation offers awarded in CRR Auctions, counting the quantity only once per source and sink pair, where the Market Participant is a CRR Account Holder assigned to the registered Counter-Party. |
| OPTP *mp, (j, k), a, h* | MW | *PTP Option Purchase per Market Participant per source and sink pair per CRR Auction per hour*—The MW quantity that represents the total of Market Participant *mp*’s PTP Option bids with the source *j* and the sink *k* awarded in CRR Auction *a*, for the hour *h*, where the Market Participant is a CRR Account Holder. |
| UOPTP *mp* | MWh | *Uplift PTP Option Purchase per Market Participant*—The MW quantity that represents the monthly total of Market Participant *mp*’s PTP Option bids awarded in CRR Auctions, counting the quantity only once per source and sink pair, where the Market Participant is a CRR Account Holder assigned to the registered Counter-Party. |
| OBLP *mp, (j, k), a, h* | MW | *PTP Obligation Purchase per Market Participant per source and sink pair per CRR Auction per hour*—The MW quantity that represents the total of Market Participant *mp*’s PTP Obligation bids with the source *j* and the sink *k* awarded in CRR Auction *a*, for the hour *h*, where the Market Participant is a CRR Account Holder. |
| UOBLP *mp* | MWh | *Uplift PTP Obligation Purchase per Market Participant*—The MW quantity that represents the monthly total of Market Participant *mp*’s PTP Obligation bids awarded in CRR Auctions, counting the quantity only once per source and sink pair, where the Market Participant is a CRR Account Holder assigned to the registered Counter-Party. |
| UWSLTOT *mp* | MWh | *Uplift Metered Energy for Wholesale Storage Load at bus per Market Participant*⎯The monthly sum of Market Participant *mp*’s Wholesale Storage Load (WSL) energy metered by the Settlement Meter which measures WSL. |
| MEBL *mp, r, b* | MWh | *Metered Energy for Wholesale Storage Load at bus*⎯The WSL energy metered by the Settlement Meter which measures WSL for the 15-minute Settlement Interval represented as a negative value, for the Market Participant *mp*, Resource *r*, at bus *b*. |
| |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | ***[NPRR917: Insert the variables “*** ***USOGTOT mp”, “*** ***RTMGSOGZ mp. p, i”, and “OFSOG mp, gsc, b” below upon system implementation:]***   |  |  |  | | --- | --- | --- | | USOGTOT *mp* | MWh | *Uplift Real- Time Settlement Only Generator Site per Market Participant*—The monthly sum of Real-Time energy produced by Settlement Only Generators (SOGs) represented by Market Participant *mp*, where the Market Participant is a QSE assigned to the registered Counter-Party. | | RTMGSOGZ *mp. p, i* | MWh | *Real-Time Metered Generation from Settlement Only Generators Zonal per QSE per Settlement Point*— The total Real-Time energy produced by Settlement Only Transmission Self-Generators (SOTSGs) for the Market Participant *mp* in Load Zone Settlement Point *p*, for the 15-minute Settlement Interval. MWh quantities for ESS SODGs and SOTGs at sites where the ESS capacity constitutes more than 50% of the total SOG nameplate capacity will be included in this value. MWh quantities for SODGs and Settlement Only Transmission Generators (SOTGs) that opted out of nodal pricing pursuant to Section 6.6.3.9, Real-Time Payment or Charge for Energy from a Settlement Only Distribution Generator (SODG) or a Settlement Only Transmission Generator (SOTG), will also be included in this value. | | OFSOG *mp, gsc, b* | MWh | *Outflow as measured for an SODG or SOTG Site* ⎯The outflow as measured by the Settlement Meter(s) at Electrical Bus *b* for SODG or SOTG site *gsc* represented by the Market Participant *mp*. | | | | |
| *cp* | none | A registered Counter-Party. |
| *mp* | none | A Market Participant that is a non-defaulting QSE or CRR Account Holder. |
| *j* | none | A source Settlement Point. |
| *k* | none | A sink Settlement Point. |
| *a* | none | A CRR Auction. |
| *p* | none | A Settlement Point. |
| *i* | none | A 15-minute Settlement Interval. |
| *h* | none | The hour that includes the Settlement Interval i. |
| *r* | none | A Resource. |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | ***[NPRR917: Insert the variables “gsc” and “b” below upon system implementation:]***   |  |  |  | | --- | --- | --- | | *gsc* | none | A generation site code. | | *b* | none | An Electrical Bus. | | | | |

(3) The uplifted short-paid amount will be allocated to the Market Participants (QSEs or CRR Account Holders) assigned to a registered Counter-Party based on the pro-rata share of MWhs that the QSE or CRR Account Holder contributed to its Counter-Party’s maximum MWh activity ratio share.

(4) Any uplifted short-paid amount greater than $2,500,000 must be scheduled so that no amount greater than $2,500,000 is charged on each set of Default Uplift Invoices until ERCOT uplifts the total short-paid amount. ERCOT must issue Default Uplift Invoices at least 30 days apart from each other.

(5) ERCOT shall issue Default Uplift Invoices no earlier than 90 days following a short-pay of a Settlement Invoice on the date specified in the Settlement Calendar. The Invoice Recipient is responsible for accessing the Invoice on the MIS Certified Area once posted by ERCOT.

(6) Each Default Uplift Invoice must contain:

(a) The Invoice Recipient’s name;

(b) The ERCOT identifier (Settlement identification number issued by ERCOT);

(c) Net Amount Due or Payable – the aggregate summary of all charges owed by a Default Uplift Invoice Recipient;

(d) Run Date – the date on which ERCOT created and published the Default Uplift Invoice;

(e) Invoice Reference Number – a unique number generated by the ERCOT applications for payment tracking purposes;

(f) Default Uplift Invoice Reference – an identification code used to reference the amount uplifted;

(g) Payment Date and Time – the date and time that Default Uplift Invoice amounts must be paid;

(h) Remittance Information Details – details including the account number, bank name, and electronic transfer instructions of the ERCOT account to which any amounts owed by the Invoice Recipient are to be paid or of the Invoice Recipient’s account from which ERCOT may draw payments due; and

(i) Overdue Terms – the terms that would apply if the Market Participant makes a late payment.

(7) Each Invoice Recipient shall pay any net debit shown on the Default Uplift Invoice on the payment due date whether or not there is any Settlement and billing dispute regarding the amount of the debit.

**16.5 Registration of a Resource Entity**

(1) A Resource Entity owns or controls a Generation Resource, Settlement Only Generator (SOG), or Load Resource connected to the ERCOT System. Each Resource Entity operating in the ERCOT Region must register with ERCOT. To become registered as a Resource Entity, an Entity must execute a Standard Form Market Participant Agreement (using the form in Section 22, Attachment A, Standard Form Market Participant Agreement), designate Resource Entity Authorized Representatives, contacts, and a User Security Administrator (USA) (per the Application for Registration as a Resource Entity), and demonstrate to ERCOT’s reasonable satisfaction that it is capable of performing the functions of a Resource Entity under these Protocols. The Resource Entity shall provide Resource Registration data pursuant to Planning Guide Section 6.8.2, Resource Registration Process, for each Generation Resource, SOG, or Load Resource through ERCOT registration, except for Distributed Generation (DG) with an installed capacity equal to or lower than the DG registration threshold that has chosen not to register with ERCOT. A Resource Entity may submit a proposal to register the aggregation of generators, with the exception of Intermittent Renewable Resources (IRRs) pursuant to paragraph (12) of Section 3.10.7.2, Modeling of Resources and Transmission Loads, as an Aggregate Generation Resource (AGR) which ERCOT may grant at its sole discretion. A Resource Entity may submit a proposal to register a SOG consisting of an Energy Storage System (ESS) or a combination of ESS and non-ESS generation. The Resource Entity must identify all components of the SOG as part of the Resource Registration process.

|  |
| --- |
| ***[NPRR1002: Replace paragraph (1) above with the following upon system implementation:]***  (1) A Resource Entity owns or controls a Generation Resource, Energy Storage Resource (ESR), Settlement Only Generator (SOG), or Load Resource connected to the ERCOT System. Each Resource Entity operating in the ERCOT Region must register with ERCOT. To become registered as a Resource Entity, an Entity must execute a Standard Form Market Participant Agreement (using the form in Section 22, Attachment A, Standard Form Market Participant Agreement), designate Resource Entity Authorized Representatives, contacts, and a User Security Administrator (USA) (per the Application for Registration as a Resource Entity), and demonstrate to ERCOT’s reasonable satisfaction that it is capable of performing the functions of a Resource Entity under these Protocols. The Resource Entity shall provide Resource Registration data pursuant to Planning Guide Section 6.8.2, Resource Registration Process, for each Resource or SOG through ERCOT registration, except for Distributed Generation (DG) with an installed capacity equal to or lower than the DG registration threshold that has chosen not to register with ERCOT. A Resource Entity may submit a proposal to register the aggregation of generators, with the exception of Intermittent Renewable Resources (IRRs) pursuant to paragraph (12) of Section 3.10.7.2, Modeling of Resources and Transmission Loads, as an Aggregate Generation Resource (AGR) which ERCOT may grant at its sole discretion. If a Resource Entity intends to register one or more Energy Storage Systems (ESS) and one or more non-ESS generators as SOGs at the same site, the Resource Entity must provide an affidavit attesting to the amount of ESS and non-ESS capacity at the site as a condition for registration. |

(2) Prior to commissioning, Resources Entities will regularly update the data necessary for modeling. These updates will reflect the best available information at the time submitted.

(3) Once ERCOT has received a new or amended Standard Generation Interconnection Agreement (SGIA) or a letter from a duly authorized official from the Municipally Owned Utility (MOU) or Electric Cooperative (EC) and has determined that the proposed Generation Resource or SOG meets the requirements of Planning Guide Section 6.9, Addition of Proposed Generation to the Planning Models, ERCOT shall review the description of the proposed Generation Resource or SOG in Exhibit “C” (or similar exhibit) to the SGIA and the data submitted pursuant to Planning Guide Section 6.8.2 to assess whether the Generation Resource or SOG, as proposed, would violate any operational standards established in the Protocols, Planning Guide, Nodal Operating Guides, and Other Binding Documents. ERCOT must provide its determination to the Transmission Service Provider (TSP) and the owner of the proposed Generation Resource or SOG within 90 days of the date the Generation Resource or SOG meets the conditions for review. Notwithstanding the foregoing, this determination shall not preclude ERCOT from subsequently determining that the Generation Resource or SOG violates any operational standards established in the Protocols, Planning Guide, Nodal Operating Guides, and Other Binding Documents or from taking any appropriate action based on that determination.

|  |
| --- |
| ***[NPRR1002: Replace paragraph (3) above with the following upon system implementation:]***  (3) Once ERCOT has received a new or amended Standard Generation Interconnection Agreement (SGIA) or a letter from a duly authorized official from the Municipally Owned Utility (MOU) or Electric Cooperative (EC) and has determined that the proposed Generation Resource, ESR, or SOG meets the requirements of Planning Guide Section 6.9, Addition of Proposed Generation to the Planning Models, ERCOT shall review the description of the proposed Generation Resource, ESR, or SOG in Exhibit “C” (or similar exhibit) to the SGIA and the data submitted pursuant to Planning Guide Section 6.8.2, to assess whether the Generation Resource, ESR, or SOG, as proposed, would violate any operational standards established in the Protocols, Planning Guide, Nodal Operating Guides, and Other Binding Documents. ERCOT must provide its determination to the Transmission Service Provider (TSP) and the owner of the proposed Generation Resource, ESR, or SOG within 90 days of the date the Generation Resource, ESR, or SOG meets the conditions for review. Notwithstanding the foregoing, this determination shall not preclude ERCOT from subsequently determining that the Generation Resource, ESR, or SOG violates any operational standards established in the Protocols, Planning Guide, Nodal Operating Guides, and Other Binding Documents or from taking any appropriate action based on that determination. |

(4) An Interconnecting Entity (IE) shall not proceed to Initial Synchronization of a Generation Resource, Settlement Only Transmission Generator (SOTG), or Settlement Only Transmission Self-Generator (SOTSG) in the event of any of the following conditions:

(a) Pursuant to paragraph (3) above, ERCOT has reasonably determined that the Generation Resource, SOTG, or SOTSG may violate operational standards established in the Protocols, Planning Guide, Nodal Operating Guides, and Other Binding Documents, and the Resource Entity has not yet demonstrated to ERCOT’s satisfaction that the Generation Resource, SOTG, or SOTSG can comply with these standards;

(b) The requirements of Planning Guide Section 5.9, Quarterly Stability Assessment, have not been completed for the Generation Resource, SOTG, or SOTSG; or

(c) Any required Subsynchronous Resonance (SSR) studies, SSR Mitigation Plan, SSR Protection, and SSR monitoring if required, have not been completed and approved by ERCOT.

|  |
| --- |
| ***[NPRR1002 and NPRR1016: Replace applicable portions of paragraph (4) above with the following upon system implementation:]***  (4) An Interconnecting Entity (IE) shall not proceed to Initial Synchronization of a Generation Resource, ESR, Settlement Only Transmission Generator (SOTG), or Settlement Only Transmission Self-Generator (SOTSG) in the event of any of the following conditions:  (a) Pursuant to paragraph (3) above, ERCOT has reasonably determined that the Generation Resource, ESR, SOTG, or SOTSG may violate operational standards established in the Protocols, Planning Guide, Nodal Operating Guides, and Other Binding Documents, and the Resource Entity has not yet demonstrated to ERCOT’s satisfaction that the Generation Resource, ESR, SOTG, or SOTSG can comply with these standards;  (b) The requirements of Planning Guide Section 5.9, Quarterly Stability Assessment, if applicable, have not been completed for the Generation Resource, ESR, SOTG, or SOTSG; or  (c) Any required Subsynchronous Resonance (SSR) studies, SSR Mitigation Plan, SSR Protection, and SSR monitoring if required, have not been completed and approved by ERCOT. |

(5) DG with an installed capacity greater than one MW, the DG registration threshold, which exports energy into a Distribution System, must register with ERCOT.

(6) A Resource Entity representing an Energy Storage Resource (ESR) shall register the ESR as both a Generation Resource and a Controllable Load Resource.

|  |
| --- |
| ***[NPRR1002: Replace paragraph (6) above with the following upon system implementation:]***  (6) A Resource Entity representing an ESR shall register the ESR as an ESR. ERCOT systems, including the Energy and Market Management System (EMMS) and Settlement system, shall continue to treat the ESR as both a Generation Resource and a Controllable Load Resource until such time as all ERCOT systems are capable of treating an ESR as a single Resource. |