|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | ONCOR | CNP | AEP | TNMP | |
| CURRENT STATUS |  |  |  | |  |
| Status of AMS deployment in BUSDIRRQ applications |  |  |  | |  |
| TRANSITION PLAN |  |  |  | |  |
| Existing ESIs with AMS subject to 4CP billing on a BUSHI/MED/LO profile |  |  |  | |  |
| Existing ESIs with AMS subject to 4CP billing on a BUSIDRRQ profile |  |  |  | |  |
| Existing ESIs with AMS on a BUSHI/MED/LO profile that have crossed 700 kW/kVA threshold |  |  |  | |  |
| New ESIs expected to cross 700 kW/kVA threshold |  |  |  | |  |
| ACCESS TO INTERVAL DATA |  |  |  | |  |
| Once an ESI has transitioned to BUSLRG or BUSLRGDG, how will 3rd parties access interval data |  |  |  | |  |