|  |  |  |  |
| --- | --- | --- | --- |
| NPRR Number | [1139](https://www.ercot.com/mktrules/issues/NPRR1139) | NPRR Title | Adjustments to Capacity Shortfall Ratio Share for IRRs |
| Date Posted | | May 25, 2022 | |
|  | |  | |
| Requested Resolution | | Normal | |
| Nodal Protocol Sections Requiring Revision | | 5.7.4.1, RUC Capacity-Short Charge  5.7.4.1.1, Capacity Shortfall Ratio Share | |
| Related Documents Requiring Revision/Related Revision Requests | | None | |
| Revision Description | | This Nodal Protocol Revision Request (NPRR) replaces the usage of the Wind-powered Generation Resource Production Potential (WGRPP) and PhotoVoltaic Generation Resource Production Potential (PVGRPP) with the High Sustained Limit (HSL) of an Intermittent Renewable Resource (IRR) as reflected in the Current Operating Plan (COP), similar to treatment afforded to Resources that are not IRRs.  Currently, the available capacity for a Wind-powered Generation Resource (WGR), for purposes of the Capacity Shortfall Ratio Share calculation, is the WGRPP, as described in Section 4.2.2, Wind-Powered Generation Resource Production Potential; for a PhotoVoltaic Generation Resource (PVGR), the available capacity, for purposes of the Capacity Shortfall Ratio Share calculation, is the PVGRPP, as described in Section 4.2.3, PhotoVoltaic Generation Resource Production Potential. However, due to netting of an IRR with large Loads behind the Point of Interconnection (POI), the capacity reflected in the WGRPP or PVGRPP may not be the available capacity at the POI.  This NPRR replaces the WGRPP and PVGRPP with the HSL values determined from COP data  Please note that while this NPRR replaces the WGRPP and PVGRPP with the HSL values determined from COP data, this NPRR does not affect the snapshot values to be used for IRR capacity currently in use today. For IRRs, the quantity used in the calculation is determined at the time of the Reliability Unit Commitment (RUC) Snapshot, as opposed to other Resource types which take the minimum value from the RUC Snapshot and the Adjustment Period snapshot.  This NPRR also makes a minor adjustment in Section 5.7.4.1, changing the name of a variable in a formula from HSL to RUCHSL in order to match the variable name in the Protocols to the data value available in the Settlement extracts. | |
| Reason for Revision | | Addresses current operational issues.  Meets Strategic goals (tied to the [ERCOT Strategic Plan](http://www.ercot.com/content/wcm/lists/144926/ERCOT_Strategic_Plan_2019-2023.pdf) or directed by the ERCOT Board).  Market efficiencies or enhancements  Administrative  Regulatory requirements  Other: (explain)  *(please select all that apply)* | |
| Business Case | | This NPRR improves the accuracy of the values used when determining the capacity shortfall ratio share by:   * Replacing the WGRPP and PVGRPP values with a value that more accurately reflects the capacity available to the ERCOT system due to netting behind the POI; and * Considering Ancillary Service(s) carried by the IRR by using the High Ancillary Service Limit (HASL) value when determining capacity, as is done for Resources that are not IRRs. | |

|  |  |
| --- | --- |
| Sponsor | |
| Name | Austin Rosel |
| E-mail Address | [Austin.Rosel@ercot.com](mailto:Austin.Rosel@ercot.com) |
| Company | ERCOT |
| Phone Number | 512-248-6686 |
| Cell Number |  |
| Market Segment | Not applicable |

|  |  |
| --- | --- |
| **Market Rules Staff Contact** | |
| **Name** | Cory Phillips |
| **E-Mail Address** | [cory.phillips@ercot.com](mailto:cory.phillips@ercot.com) |
| **Phone Number** | 512-248-6464 |

|  |
| --- |
| Proposed Protocol Language Revision |

5.7.4.1 RUC Capacity-Short Charge

(1) The dollar amount charged to each QSE, due to capacity shortfalls for a particular RUC, for a 15-minute Settlement Interval, is the QSE’s shortfall ratio share multiplied by the total RUC Make-Whole Payments, including amounts for RMR Units, to all QSEs for that RUC, subject to a cap. The cap on the charge to each QSE is two multiplied by the total RUC Make-Whole Payments, including amounts for RMR Units, for all QSEs multiplied by that QSE’s capacity shortfall for that RUC process divided by the total capacity of all RUC-committed Resources during that Settlement Interval for the RUC process. That dollar amount charged to each QSE is calculated as follows:

RUCCSAMT *ruc, i, q* = (-1) \* Max [(RUCSFRS *ruc, i, q* \* RUCMWAMTRUCTOT *ruc, h*),   
(2 \* RUCSF *ruc, i, q* \* RUCMWAMTRUCTOT *ruc, h* / RUCCAPTOT *ruc, h*)] / 4

Where:

RUCMWAMTRUCTOT *ruc, h*  = RUCMWAMT *ruc, q, r, h*

RUCCAPTOT *ruc, h* = (RUCHSL *ruc, h, r* – RUCHSL *ruc, h, beforeCCGR*)

The above variables are defined as follows:

| Variable | Unit | Definition |
| --- | --- | --- |
| RUCCSAMT *ruc, i, q* | $ | *RUC Capacity-Short Amount*—The charge to a QSE *q*, due to capacity shortfall for a particular RUC process *ruc*, for the 15-minute Settlement Interval *i*. |
| RUCMWAMTRUCTOT *ruc, h* | $ | *RUC Make-Whole Amount Total per RUC*—The sum of RUC Make-Whole Payments for a particular RUC process *ruc*, including amounts for RMR Units, for the hour *h* that includes the 15-minute Settlement Interval. |
| RUCMWAMT *ruc, q, r, h* | $ | *RUC Make-Whole Payment*—The RUC Make-Whole Payment to the QSE *q* for Resource *r*, for a particular RUC process *ruc*, for the hour *h* that includes the 15-minute Settlement Interval. See Section 5.7.1, RUC Make-Whole Payment. When one or more Combined Cycle Generation Resources are committed by RUC, payment is made to the Combined Cycle Train for all RUC-committed Combined Cycle Generation Resources. |
| RUCSFRS *ruc, i, q* | none | *RUC Shortfall Ratio Share*—The ratio of the QSE *q*’s capacity shortfall to the sum of all QSEs’ capacity shortfalls for a particular RUC process *ruc*, for the 15-minute Settlement Interval *i*. See Section 5.7.4.1.1, Capacity Shortfall Ratio Share. |
| RUCSF *ruc, i, q* | MW | *RUC Shortfall*—The QSE *q*’s capacity shortfall for a particular RUC process *ruc* for the 15-minute Settlement Interval *i*. See formula in Section 5.7.4.1.1. |
| RUCCAPTOT *ruc, h* | MW | *RUC Capacity Total*—The sum of the High Sustained Limits (HSLs) of all RUC-committed Resources for a particular RUC process *ruc*, for the hour *h* that includes the 15-minute Settlement Interval. See formula in Section 5.7.4.1.1. |
| RUCHSL *ruc, q, r, h* | MW | *High Sustained Limit at RUC Snapshot*—The HSL of Generation Resource *r* represented by QSE *q* for the hour *h*, according to the COP and Trades Snapshot for the RUC process *ruc*. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| *ruc* | none | The RUC process for which the RUC Capacity-Short Charge is calculated. |
| *i* | none | A 15-minute Settlement Interval. |
| *q* | none | A QSE. |
| *h* | none | The hour that includes the Settlement Interval *i*. |
| *r* | none | A Generation Resource that is RUC-committed for the hour that includes the Settlement Interval *i*, as a result of a particular RUC process. |
| *beforeCCGR* | none | The Combined Cycle Generation Resource that was QSE-committed in a RUCAC-Interval. |

5.7.4.1.1 Capacity Shortfall Ratio Share

(1) In calculating the amount short for each QSE, the HSL values as reflected in the COP at the time of the RUC execution shall be considered the available capacity of an IRR when determining responsibility for the corresponding RUC charges, regardless of the Real-Time output of the IRR. Therefore, for an IRR the HASLSNAP variable used below shall be equal to the HSL value as reflected in the QSE’s COP at the time of the RUC execution.

(2) In calculating the amount short for each QSE, the QSE must be given a capacity credit for non-Intermittent Renewable Resources (IRRs) that were given notice of decommitment within the two hours before the Operating Hour as a result of the RUC process by setting the HASLSNAP and HASLADJ variables used below equal to the HASLSNAP value for the Resource immediately before the decommitment instruction was given.

(3) In calculating the short amount for each QSE, if the High Ancillary Service Limit (HASL) for a Resource was credited to the QSE during the RUC snapshot but the Resource experiences a Forced Outage within two hours before the start of the Settlement Interval, then the HASL for that Resource is also credited to the QSE in the HASLADJ.

(4) In calculating the short amount for each QSE, if the DCIMPSNAP was credited to the QSE during the RUC snapshot but the entire Direct Current Tie (DC Tie) experiences a Forced Outage within two hours before the start of the Settlement Interval, then the DCIMPSNAP is also credited to the QSE in the DCIMPADJ.

(5) For Combined Cycle Generation Resources, if more than one Combined Cycle Generation Resource is shown On-Line in its COP for the same Settlement hour, then the provisions of paragraph (6)(a) of Section 3.9.1, Current Operating Plan (COP) Criteria, apply in the determination of the On-Line Combined Cycle Generation Resource for that Settlement hour.

(6) The capacity shortfall ratio share of a specific QSE for a particular RUC process is calculated, for a 15-minute Settlement Interval, as follows:

RUCSFRS *ruc, i, q* = RUCSF *ruc, i, q* / RUCSFTOT *ruc, i*

Where:

RUCSFTOT *ruc, i* = RUCSF *ruc, i, q*

(7) The RUC Shortfall in MW for one QSE for one 15-minute Settlement Interval is:

RUCSF *ruc, i, q* = Max (0, Max (RUCSFSNAP *ruc, q, i*, RUCSFADJ *ruc, q, i*) – RUCCAPCREDIT *q, i, z*)

(8) The RUC Shortfall in MW for one QSE for one 15-minute Settlement Interval, as measured at the snapshot, is:

RUCSFSNAP *ruc ,q ,i* = Max (0, ((RTAML *q, p, i* \* 4) +  RTDCEXP *q, p, i* – RUCCAPSNAP *ruc, q, i*))

(9) The amount of capacity that a QSE had according to the RUC snapshot for a 15-minute Settlement Interval is:

RUCCAPSNAP *ruc, q, i* = HASLSNAP *q, r, h* + (RUCCPSNAP *q, h* – RUCCSSNAP *q, h*) + (DAEP *q, p, h* –DAES *q, p, h*) + (RTQQEPSNAP *q, p, i* – RTQQESSNAP *q, p, i*) +  DCIMPSNAP *q, p, i*

(10) The RUC Shortfall in MW for one QSE for one 15-minute Settlement Interval, as measured at Real-Time, but including capacity from IRRs as seen in the RUC snapshot, is:

RUCSFADJ *ruc, q, i* = Max (0, ((RTAML *q, p, i*) \*4) +  RTDCEXP *q, p, i* – (HASLSNAP *ruc, q, r, h* + RUCCAPADJ *q, i*))

(11) The amount of capacity that a QSE had in Real-Time for a 15-minute Settlement Interval, excluding capacity from IRRs, is:

RUCCAPADJ *q, i* = HASLADJ *q, r, h* + (RUCCPADJ *q, h* – RUCCSADJ *q, h*) + (DAEP *q, p, h* – DAES *q, p, h*) + (RTQQEPADJ *q, p, i* – RTQQESADJ *q, p, i*) +  DCIMPADJ *q, p, i*

The above variables are defined as follows:

| Variable | Unit | Definition |
| --- | --- | --- |
| **RUCSFRS *ruc, i, q*** | none | *RUC Shortfall Ratio Share*—The ratio of the QSE *q*’s capacity shortfall to the sum of all QSEs’ capacity shortfalls, for the RUC process *ruc*, for the 15-minute Settlement Interval *i*. |
| RUCSF *ruc, i, q* | MW | *RUC Shortfall*—The QSE *q*’s capacity shortfall for the RUC process *ruc* for the 15-minute Settlement Interval *i*. |
| RUCSFTOT *ruc, i* | MW | *RUC Shortfall Total*—The sum of all QSEs’ capacity shortfalls, for a RUC process *ruc*, for a 15-minute Settlement Interval *i*. |
| RUCSFSNAP *ruc, q, i* | MW | *RUC Shortfall at Snapshot*—The QSE *q*’s capacity shortfall according to the snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. |
| RUCSFADJ *ruc, q, i* | MW | *RUC Shortfall at Adjustment Period*—The QSE *q*’s Adjustment Period capacity shortfall, including capacity from IRRs as seen in the snapshot for the RUC process *ruc*, for the 15-minute Settlement Interval *i*. |
| RUCCAPCREDIT *q, i, z* | MW | *RUC Capacity Credit by QSE*—The QSE *q*’s capacity credit resulting from capacity paid through the RUC Capacity-Short Amount for RUC process *z* for the 15-minute Settlement Interval *i*. |
| RTAML *q, p, i* | MWh | *Real-Time Adjusted Metered Load*—The QSE *q*’s Adjusted Metered Load (AML) at the Settlement Point *p* for the 15-minute Settlement Interval *i*. |
| RUCCAPSNAP *ruc, q, i* | MW | *RUC Capacity Snapshot at time of RUC*—The amount of the QSE *q*’s calculated capacity in the COP and Trades Snapshot for the RUC process *ruc* for a 15-minute Settlement Interval *i*. |
| HASLSNAP *q, r, h* | MW | *High Ancillary Services Limit at Snapshot*—The HASL of the Resource *r* represented by the QSE *q*, according to the COP and Trades Snapshot for the RUC process for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| RTDCEXP *q, p, i* | MW | *Real-Time DC Export per QSE per Settlement Point*—The aggregated DC Tie Schedule through DC Tie *p* submitted by QSE *q* that is under the Oklaunion Exemption as an exporter from the ERCOT Region, for the 15-minute Settlement Interval *i*. |
| DCIMPADJ *q, p, i* | MW | *DC Import per QSE per Settlement Point*—The approved aggregated DC Tie Schedule submitted by QSE *q* as an importer into the ERCOT System through DC Tie *p* according to the Adjustment Period snapshot, for the 15-minute Settlement Interval *i*. |
| DCIMPSNAP *q, p, i* | MW | *DC Import per QSE per Settlement Point*—The approved aggregated DC Tie Schedule submitted by QSE *q* as an importer into the ERCOT System through DC Tie *p*, according to the snapshot for the RUC process for the hour that includes the 15-minute Settlement Interval *i*. |
| RUCCPSNAP *q, h* | MW | *RUC Capacity Purchase at Snapshot*—The QSE *q*’s capacity purchase, according to the COP and Trades Snapshot for the RUC process for the hour *h* that includes the 15-minute Settlement Interval. |
| RUCCSSNAP *q, h* | MW | *RUC Capacity Sale at Snapshot*—The QSE *q*’s capacity sale, according to the COP and Trades Snapshot for the RUC process for the hour *h* that includes the 15-minute Settlement Interval. |
| RUCCAPADJ *q, i* | MW | *RUC Capacity Snapshot during Adjustment Period*—The amount of the QSE *q*’s calculated capacity in the RUC according to the COP and Trades Snapshot, excluding capacity for IRRs, at the end of the Adjustment Period for a 15-minute Settlement Interval *i.* |
| HASLADJ *q, r, h* | MW | *High Ancillary Services Limit at Adjustment Period*—The HASL of a non-IRR *r* represented by the QSE *q*, according to the Adjustment Period snapshot, for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| RUCCPADJ *q, h* | MW | *RUC Capacity Purchase at Adjustment Period*—The QSE *q*’s capacity purchase, according to the Adjustment Period COP and Trades Snapshot for the hour *h* that includes the 15-minute Settlement Interval. |
| RUCCSADJ *q, h* | MW | *RUC Capacity Sale at Adjustment Period*—The QSE *q*’s capacity sale, according to the Adjustment Period COP and Trades Snapshot for the hour *h* that includes the 15-minute Settlement Interval. |
| DAEP *q, p, h* | MW | *Day-Ahead Energy Purchase*—The QSE *q*’s energy purchased in the DAM at the Settlement Point *p* for the hour *h* that includes the 15-minute Settlement Interval. |
| DAES *q, p, h* | MW | *Day-Ahead Energy Sale*—The QSE *q*’s energy sold in the DAM at the Settlement Point *p* for the hour *h* that includes the 15-minute Settlement Interval. |
| RTQQEPSNAP *q, p, i* | MW | *QSE-to-QSE Energy Purchase by QSE by point*—The QSE *q*’s Energy Trades in which the QSE is the buyer at the delivery Settlement Point *p* for the 15-minute Settlement Interval *i*, in the COP and Trades Snapshot. |
| RTQQESSNAP *q, p, i* | MW | *QSE-to-QSE Energy Sale by QSE by point*—The QSE *q*’s Energy Trades in which the QSE is the seller at the delivery Settlement Point *p* for the 15-minute Settlement Interval *i*, in the COP and Trades Snapshot. |
| RTQQEPADJ *q, p, i* | MW | *QSE-to-QSE Energy Purchase by QSE by point*—The QSE *q*’s Energy Trades in which the QSE is the buyer at the delivery Settlement Point *p* for the 15-minute Settlement Interval *i*, in the last COP and Trades Snapshot at the end of the Adjustment Period for that Settlement Interval. |
| RTQQESADJ *q, p, i* | MW | *QSE-to-QSE Energy Sale by QSE by point*—The QSE *q*’s Energy Trades in which the QSE is the seller at the delivery Settlement Point *p* for the 15-minute Settlement Interval *i*, in the last COP and Trades Snapshot at the end of the Adjustment Period for that Settlement Interval. |
| *q* | none | A QSE. |
| *p* | none | A Settlement Point. |
| *r* | none | A Generation Resource that is QSE-committed or planning to operate as a Quick Start Generation Resource (QSGR) for the Settlement Interval as shown by the Resource Status of OFFQS in the COP and Trades Snapshot and/or Adjustment Period snapshot; or RUC-decommitted for the Settlement Interval (subject to paragraphs (1) and (2) above); or a Switchable Generation Resource (SWGR) released by a non-ERCOT Control Area Operator (CAO) to operate in the ERCOT Control Area due to an ERCOT RUC instruction for an actual or anticipated EEA condition. If the Settlement Interval is a RUCAC-Interval, *r* represents the Combined Cycle Generation Resource that was QSE-committed at the time the RUCAC was issued. |
| *z* | none | A previous RUC process for the Operating Day. |
| *i* | none | A 15-minute Settlement Interval. |
| *h* | none | The hour that includes the Settlement Interval *i*. |
| *ruc* | none | The RUC process for which this RUC Shortfall Ratio Share is calculated. |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***[NPRR1009, NPRR1014, NPRR1029, NPRR1032, and NPRR1054: Replace applicable portions of Section 5.7.4.1.1 above with the following upon system implementation of the Real-Time Co-Optimization (RTC) project for NPRR1009; or upon system implementation for NPRR1014, NPRR1029, NPRR1032, or NPRR1054:]***  (1) In calculating the shortfall amount for each QSE, the Resource capacity shall be calculated for a Generation Resource or ESR, that is not a DC-Coupled Resource, and that meets any of the following conditions:  (a) QSE-committed;  (b) Planning to operate as a Quick Start Generation Resource (QSGR) for the Settlement Interval as shown by the COP Status of OFFQS in the RUC Snapshot for the RUC Process and/or Adjustment Period; or  (c) A Switchable Generation Resource (SWGR) that is released by a non-ERCOT Control Area Operator (CAO) to operate in the ERCOT Control Area due to an ERCOT RUC instruction for an actual or anticipated EEA condition and that is shown as On-Line in its COP; or  (d) If the Settlement Interval is a RUCAC-Interval, the Combined Cycle Generation Resource that was QSE-committed at the time the RUCAC was issued, excluding the condition for SWGRs as describe in paragraph (c) above.  (2) In calculating the amount short for each QSE, the available capacity of a DC-Coupled Resource shall be calculated for each RUC Snapshot, and at the end of the Adjustment Period. The available capacity of a DC-Coupled Resource at the RUC Shapshot shall be the HSL values reflected in the COP at the time of the RUC execution. The available capacity of a DC-Coupled Resource at the end of the Adjustment Period is calculated for each RUC Snapshot by adding the capacity value of the Energy Storage System (ESS) that is included in the HSL of the DC-Coupled Resource, as submitted in the COP, at the end of the Adjustment period, to the HSL of the IRR as reflected in the COP at the time of the RUC execution as follows:  The DCRCAPSNAP variable at the RUC Snapshot is calculated as:  **DCRCAPSNAP *ruc, q, r, h =* RUCHSL*ruc, q, r, h***  The DCRCAPADJ variable at the end of the Adjustment Period is calculated as:  **DCRCAPADJ *ruc, q, r, h =* (RUCHSL*ruc, q, r, h* - RUCHSLESS*ruc, q, r, h***) **+**  **HSLESS *q, r, h***  The above variables are defined as follows:   | **Variable** | **Unit** | **Definition** | | --- | --- | --- | | *DCRCAPSNAP ruc, q, r, h* | MW | *DC-Coupled Resource Capacity at Snapshot*—The Resource Capacity of DC-Coupled Resource *r* represented by the QSE *q* for the hour *h*, according to the RUC Snapshot for the RUC process. | | *RUCHSLESS ruc, q, r, h* | MW | *High Sustained Limit of ESS at Snapshot* —The portion of the HSL of the DC-Coupled Resource due to the ESS that is part of the DC-Coupled Resource *r* represented by QSE *q* for the hour *h*, according to the RUC Snapshot for the RUC process. | |  |  |  | |  |  |  | | RUCHSL *ruc, q, r, h* | MW | *High Sustained Limit at RUC Snapshot*—The HSL of Generation Resource *r* represented by the QSE *q* for the hour *h*, according to the RUC Snapshot for the RUC Process *ruc*. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. | | *DCRCAPADJ ruc, q, r, h* | MW | *DC-Coupled Resource Capacity at Adjustment Period*—The Resource Capacity of DC-Coupled Resource *r* represented by the QSE *q* for the hour *h*, at the end of the Adjustment Period. | | *HSLESS q, r, h* | MW | *High Sustained Limit for ESS at Adjustment Period* —The portion of the HSL of the DC-Coupled Resource due to the ESS that is part of the DC-Coupled Resource *r* represented by QSE *q* for the hour *h*, at the end of the Adjustment Period. | | *q* | none | A QSE. | | *r* | none | A DC-Coupled Resource that is QSE-committed or RUC-decommitted for the Settlement Interval (subject to paragraph (4) below) or a Switchable Generation Resource (SWGR) released by a non-ERCOT Control Area Operator (CAO) to operate in the ERCOT Control Area due to an ERCOT RUC instruction for an actual or anticipated EEA condition. | | *h* | none | An hourly Settlement Interval. | | *ruc* | none | A RUC process for which this DC-Coupled Resource Capacity is calculated. |   (3) In calculating the amount short for each QSE, the HSL values as reflected in the COP at the time of the RUC execution shall be considered the available capacity of an IRR when determining responsibility for the corresponding RUC charges, regardless of the Real-Time output of the IRR. Therefore, for an IRR, the RCAPSNAP variable used below shall be equal to the HSL value as reflected in the QSE’s COP at the time of the RUC execution.  (4) In calculating the amount short for each QSE, the QSE must be given a capacity credit if a Resource was given notice of decommitment within the two hours before the Operating Hour as a result of the RUC process as follows:  (a) Non-Intermittent Renewable Resources (IRRs) will have the RCAPSNAP and RCAPADJ variables used below set equal to the RCAPSNAP value for the Resource immediately before the decommitment instruction was given;  (b) DC-Coupled Resources will have the DCRCAPSNAP and DCRCAPADJ variables used below set equal to the DCRCAPSNAP value for the Resource immediately before the decommitment instruction was given.  (5) In calculating the short amount for each QSE, if the RCAPSNAP for a non-IRR was credited to the QSE during the RUC Snapshot but the Resource experiences a Forced Outage within two hours before the start of the Settlement Interval, then the RCAPSNAP for that Resource is also credited to the QSE in the RCAPADJ. If the Resource is a DC-Coupled Resource, then the DCRCAPSNAP for that Resource from the RUC Snapshot is credited to the QSE in the DCRCAPADJ.  (6) In calculating the short amount for each QSE, if the DCIMPSNAP was credited to the QSE during the RUC Snapshot but the entire Direct Current Tie (DC Tie) experiences a Forced Outage within two hours before the start of the Settlement Interval, then the DCIMPSNAP is also credited to the QSE in the RTDCIMP.  (7) For Combined Cycle Generation Resources, if more than one Combined Cycle Generation Resource is shown On-Line in its COP for the same Settlement hour, then the provisions of paragraph (6)(a) of Section 3.9.1, Current Operating Plan (COP) Criteria, apply in the determination of the On-Line Combined Cycle Generation Resource for that Settlement hour.  (8) The capacity shortfall ratio share of a specific QSE for a particular RUC process is calculated, for a 15-minute Settlement Interval, as follows:  **RUCSFRS *ruc, i, q* = RUCSF *ruc, i, q* / RUCSFTOT *ruc, i***  Where:  RUCSFTOT *ruc, i* = RUCSF *ruc, i, q*  (9) The RUC Shortfall in MW for one QSE for one 15-minute Settlement Interval is:  **RUCSF *ruc, i, q* = Max (0, Max (RUCSFSNAP *ruc, q, i*, RUCSFADJ *ruc, q, i*) – RUCCAPCREDIT *q, i, z*)**  (10) The RUC Shortfall in MW for one QSE for one 15-minute Settlement Interval, as measured at the RUC Snapshot, is:  **RUCSFSNAP *ruc ,q ,i* = Max (RUCOSFSNAP *ruc, q, i* , RUCASFSNAP *ruc, q, i*)**  (11) The overall shortfall in MW that a QSE had according to the RUC Snapshot for a 15-minute Settlement Interval is:  **RUCOSFSNAP *ruc, q, i* = Max (0, ((RTAML *q, p, i* \* 4) + ASONPOSSNAP *ruc, q, i* – RUCCAPSNAP *ruc, q, i*))**  The QSE’s On-Line Ancillary Service Position according to the RUC Snapshot for a 15-minute Settlement Interval is:  **ASONPOSSNAP *ruc, q, i* = RUPOSSNAP *ruc, q, h* + RRPOSSNAP *ruc, q, h* + Max (0, (ECRPOSSNAP *ruc, q, h* + NSPOSSNAP *ruc, q, h* – ASOFFOFRSNAP *ruc, q, r, h*))**  The amount of capacity that a QSE had according to the RUC Snapshot for a 15-minute Settlement Interval is:  **RUCCAPSNAP *ruc, q, i* = RCAPSNAP *ruc, q, r, h* + DCRCAPSNAP *ruc, q, r, h* + (RUCCPSNAP *ruc, q, h* – RUCCSSNAP *ruc, q, h*) + (DAEP *q, p, h* –DAES *q, p, h*) + (RTQQEPSNAP *ruc, q, p, i* – RTQQESSNAP *ruc, q, p, i*) +  DCIMPSNAP *ruc, q, p, i* + ASOFRLRSNAP *ruc, q, r, h***  (12) The Ancillary Service shortfall calculation compares the Ancillary Service capability of the QSE, measured by the submitted Ancillary Service Offers, to the Ancillary Service Position. Because the same Resource capacity can be represented in Ancillary Offers for multiple products, the aggregated capability is accounted for by grouping Ancillary Service types in the calculation below. The Ancillary Service shortfall in MW that a QSE had according to the RUC Snapshot for a 15-minute Settlement Interval is:  **RUCASFSNAP *ruc, q, i* = Max (0, ASCAP1SNAP *ruc, q, i* , ASCAP2SNAP *ruc, q, i*, ASCAP3SNAP *ruc, q, i* , ASCAP4SNAP *ruc, q, i*, ASCAP5SNAP *ruc, q, i*) + Max (0, ASCAP6SNAP *ruc, q, i*)**  Where:  ASCAP1SNAP *ruc, q, i* = RUPOSSNAP *ruc, q, h* – ASOFR1SNAP *ruc, q, r, h*  ASCAP2SNAP *ruc, q, i* = RRPOSSNAP*ruc, q, h* –  ASOFR2SNAP *ruc, q, r, h*  ASCAP3SNAP *ruc, q, i* = (RUPOSSNAP *ruc, q, h* + RRPOSSNAP *ruc, q, h*) – ASOFR3SNAP *ruc, q, r, h*  ASCAP4SNAP *ruc, q, i* = (RUPOSSNAP *ruc, q, h* + RRPOSSNAP *ruc, q, h*  + ECRPOSSNAP *ruc, q, h*) – ASOFR4SNAP *ruc, q, r, h*  ASCAP5SNAP *ruc, q, i* = (RUPOSSNAP *ruc, q, h* + RRPOSSNAP *ruc, q, h*+ ECRPOSSNAP *ruc, q, h* + NSPOSSNAP *ruc, q, h*) – ASOFR5SNAP *ruc, q, r, h*  ASCAP6SNAP *ruc, q, i =* RDPOSSNAP *ruc, q, h* – ASOFR6SNAP *ruc, q, r, h*  (13) The RUC Shortfall in MW for one QSE for one 15-minute Settlement Interval, as measured at the end of the Adjustment Period, is:  **RUCSFADJ *ruc, q, i* = Max (RUCOSFADJ *ruc, q, i*, RUCASFADJ *q, i* )**  (14) The overall shortfall in MW that a QSE had at the end of the Adjustment Period for a 15-minute Settlement Interval, but including capacity from IRRs as seen in the RUC Snapshot and capacity from DC-Coupled Resources, is:  **RUCOSFADJ *ruc, q, i*  = Max (0, ((RTAML *q, p, i* \*4) + ASONPOSADJ *q, i* – (RCAPSNAP *ruc, q, r, h* +  DCRCAPADJ *ruc, q, r, h* + RUCCAPADJ *q, i*)))**  Where:  The On-Line Ancillary Service Position the QSE had at the end of the Adjustment Period for a 15-minute Settlement Interval is:  ASONPOSADJ *q ,i* = RUPOSADJ *q, h* + RRPOSADJ *q, h* + Max (0, (ECRPOSADJ *q, h* + NSPOSADJ *q,h* – ASOFFOFRADJ *q, r, h* ))  The amount of capacity that a QSE had at the end of the Adjustment Period for a 15-minute Settlement Interval, excluding capacity from IRRs and DC-Coupled Resources, is:  RUCCAPADJ *q, i* = RCAPADJ *q, r, h* + (RUCCPADJ *q, h* – RUCCSADJ *q, h*) + (DAEP *q, p, h* – DAES *q, p, h*) + (RTQQEPADJ *q, p, i* – RTQQESADJ *q, p, i*) +  RTDCIMP *q, p* + ASOFRLRADJ *q, r, h*  (15) The Ancillary Service shortfall calculation compares the Ancillary Service capability of the QSE, measured by the submitted Ancillary Service Offers, to the Ancillary Service Position. Because the same Resource capacity can be represented in Ancillary Offers for multiple products, the aggregated capability is accounted for by grouping Ancillary Service types in the calculation below. The Ancillary Service shortfall in MW that a QSE had at the end of the Adjustment Period for a 15-minute Settlement Interval is:  **RUCASFADJ *q, i* = Max (0, ASCAP1ADJ *q, i* , ASCAP2ADJ *q, i* , ASCAP3ADJ *q, i* , ASCAP4ADJ *q, i* , ASCAP5ADJ *q, i*) + Max (0, ASCAP6ADJ *q, i* )**  Where:  ASCAP1ADJ *q, i* = RUPOSADJ *q, h* –  ASOFR1ADJ *q, r, h*  ASCAP2ADJ *q, i* = RRPOSADJ *q, h* –  ASOFR2ADJ *q, r, h*  ASCAP3ADJ *q, i* = (RUPOSADJ *q, h* + RRPOSADJ *q, h* ) –  ASOFR3ADJ *q, r, h*  ASCAP4ADJ *q, i* = (RUPOSADJ *q, h* + RRPOSADJ *q, h* + ECRPOSADJ *q, h*) –  ASOFR4ADJ *q, r, h*  ASCAP5ADJ *q, i* = (RUPOSADJ *q, h* + RRPOSADJ *q, h* + ECRPOSADJ *q, h* + NSPOSADJ *q, h* ) –  ASOFR5ADJ *q, r, h*  ASCAP6ADJ *q, i* = RDPOSADJ *q, h* – ASOFR6ADJ *q, r, h*  The above variables are defined as follows:   | Variable | Unit | Definition | | --- | --- | --- | | **RUCSFRS *ruc, i, q*** | none | *RUC Shortfall Ratio Share*—The ratio of the QSE *q*’s capacity shortfall to the sum of all QSEs’ capacity shortfalls, for the RUC process *ruc*, for the 15-minute Settlement Interval *i*. | | RUCSF *ruc, i, q* | MW | *RUC Shortfall*—The QSE *q*’s capacity shortfall for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | RUCSFTOT *ruc, i* | MW | *RUC Shortfall Total*—The sum of all QSEs’ capacity shortfalls, for a RUC process *ruc*, for a 15-minute Settlement Interval *i*. | | RUCSFSNAP *ruc, q, i* | MW | *RUC Shortfall at Snapshot*—The QSE *q*’s capacity shortfall will be the maximum of the QSE’s overall shortfall or Ancillary Service shortfall, as calculated for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | RUCSFADJ *ruc, q, i* | MW | *RUC Shortfall at End of Adjustment Period*—The QSE *q*’s end of Adjustment Period capacity shortfall will be the maximum of the QSE’s overall shortfall or Ancillary Service shortfall, as calculated for the RUC process *ruc*, for the 15-minute Settlement Interval *i*. | | RUCCAPCREDIT *q, i, z* | MW | *RUC Capacity Credit*—The QSE *q*’s capacity credit resulting from capacity paid through the RUC Capacity-Short Amount for RUC process *z* for the 15-minute Settlement Interval *i*. | | RUCOSFSNAP *ruc, q, i* | MW | *RUC Overall Shortfall at Snapshot* —The QSE *q*’s overall capacity shortfall according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | RUCASFSNAP *ruc, q, i* | MW | *RUC Ancillary Service Shortfall at Snapshot* —The QSE *q*’s Ancillary Service capacity shortfall according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | ASONPOSSNAP *ruc ,q ,i* | MW | *Ancillary Service On-Line Position at Snapshot –* The QSE *q’s* total On-Line Ancillary Service position according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i.* | | RUPOSSNAP *ruc, q, h* | MW | *Regulation Up Position at Snapshot* ⎯The QSE *q’s* Real-Time Reg-Up Ancillary Service Position according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. | | RRPOSSNAP *ruc, q, h* | MW | *Responsive Reserve Service Position at Snapshot* ⎯The QSE *q’s* Real-Time RRS Ancillary Service Position according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. | | ECRPOSSNAP *ruc, q, h* | MW | *ERCOT Contingency Reserve Service Position at Snapshot* ⎯The QSE *q’s* Real-Time ECRS Ancillary Service Position according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. | | NSPOSSNAP *ruc, q, h* | MW | *Non-Spin Reserve Service Position at Snapshot* ⎯The QSE *q’s* Real-Time Non-Spin Ancillary Service Position according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. | | RDPOSSNAP *ruc, q, h* | MW | *Regulation Down Position at Snapshot* ⎯The QSE *q’s* Real-Time Regulation Down Service (Reg-Down) Ancillary Service Position according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. | | ASOFFOFRSNAP *ruc, q, r, h* | MW | *Ancillary Service Offline Offers at Snapshot –*The capacity represented by validated Ancillary Service Offers for ECRS and Non-Spin for Resource *r* represented by QSE *q* according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFRLRSNAP *ruc, q, r, h* | MW | *Ancillary Service Offer per Load Resource at Snapshot –* The capacity represented by validated Ancillary Service Offers for Reg-Up, Non-Spin, RRS, and ECRS for the Load Resource *r* represented by QSE *q* according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASCAP1SNAP *ruc, q, i* | MW | *Ancillary Service Net Capacity Level 1 at Snapshot* ⎯The net capacity for Reg-Up for QSE *q*, according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | ASCAP2SNAP *ruc, q, i* | MW | *Ancillary Service Net Capacity Level 2 at Snapshot* ⎯The net capacity for RRS for QSE *q*, according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | ASCAP3SNAP *ruc, q, i* | MW | *Ancillary Service Net Capacity Level 3 at Snapshot* ⎯The net capacity for Reg-Up and RRS for QSE *q*, according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | ASCAP4SNAP *ruc, q, i* | MW | *Ancillary Service Net Capacity Level 4 at Snapshot* ⎯The net capacity for Reg-Up, RRS, and ECRS for QSE *q*, according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | ASCAP5SNAP *ruc, q, i* | MW | *Ancillary Service Net Capacity Level 5 at Snapshot* ⎯The net capacity for Reg-Up, RRS, ECRS, and Non-Spinning Reserve (Non-Spin) for QSE *q*, according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | ASCAP6SNAP *ruc, q, i* | MW | *Ancillary Service Net Capacity Level 6 at Snapshot* ⎯The net capacity for Reg-Down for QSE *q*, according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | ASOFR1SNAP *ruc, q, r, h* | MW | *Ancillary Service Offer Level 1 at Snapshot –* The capacity represented by validated Reg-Up Ancillary Service Offers for Resource *r* represented by QSE *q* according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR2SNAP *ruc, q, r, h* | MW | *Ancillary Service Offer Level 2 at Snapshot –* The capacity represented by validated RRS Ancillary Service Offers for Resource *r* represented by QSE *q* according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR3SNAP *ruc, q, r, h* | MW | *Ancillary Service Offer Level 3 at Snapshot –* The capacity represented by validated Reg-Up and RRS Ancillary Service Offers for Resource *r* represented by QSE *q* according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR4SNAP *ruc, q, r, h* | MW | *Ancillary Service Offer Level 4 at Snapshot –* The capacity represented by validated Reg-Up, RRS, and ECRS Ancillary Service Offers for Resource *r* represented by QSE *q* according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR5SNAP *ruc, q, r, h* | MW | *Ancillary Service Offer Level 5 at Snapshot –* The capacity represented by validated Reg-Up, RRS, ECRS, and Non-Spin Ancillary Service Offers for Resource *r* represented by QSE *q* according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR6SNAP *ruc, q, r, h* | MW | *Ancillary Service Offer Level 6 at Snapshot –* The capacity represented by validated Reg-Down Ancillary Service Offers for Resource *r* represented by QSE *q* according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | RUCOSFADJ *ruc, q, i* | MW | *RUC Overall Shortfall at End of Adjustment Period* —The QSE *q’s* overall capacity shortfall at the end of the Adjustment Period, including capacity from IRRs as seen in the RUC Snapshot for the RUC process *ruc* and capacity from DC-Coupled Resources, for the 15-minute Settlement Interval *i*. | | RUCASFADJ *q, i* | MW | *RUC Ancillary Service Shortfall at End of Adjustment Period* —The QSE *q’s* Ancillary Service capacity shortfall at the end of the Adjustment Period for the 15-minute Settlement Interval *i*. | | ASONPOSADJ *q ,i* | MW | *Ancillary Service On-Line Position at End of Adjustment Period –* The QSE *q’s* total On-Line Ancillary Service position at the end of the Adjustment Periodfor the 15-minute Settlement Interval *i.* | | RUPOSADJ *q, h* | MW | *Regulation Up Position at End of Adjustment Period* ⎯The QSE *q’s* Reg-Up Ancillary Service Position at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. | | RRPOSADJ *q, h* | MW | *Responsive Reserve Service Position at End of Adjustment Period* ⎯The QSE *q’s* RRS Ancillary Service Position at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. | | ECRPOSADJ *q, h* | MW | *ERCOT Contingency Reserve Service Position at End of Adjustment Period* ⎯The QSE *q’s* ECRS Ancillary Service Position at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. | | NSPOSADJ *q, h* | MW | *Non-Spin Reserve Service Position at End of Adjustment Period* ⎯The QSE *q’s* Non-Spin Ancillary Service Position at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. | | RDPOSADJ *q, h* | MW | *Regulation Down Position at End of Adjustment Period* ⎯The QSE *q’s* Reg-Down Ancillary Service Position at the end of the Adjustment period for the hour *h* that includes the 15-minute Settlement Interval. | | ASOFFOFRADJ *q, r, h* | MW | *Ancillary Service Offline Offers at End of Adjustment Period –*The capacity represented by validated Ancillary Service Offers for ECRS and Non-Spin for Resource *r* represented by QSE *q* at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFRLRADJ *q, r, h* | MW | *Ancillary Service Offer per Load Resource at End of Adjustment Period –* The capacity represented by validated Ancillary Service Offers for Reg-Up, Non-Spin, RRS, and ECRS for the Load Resource *r* represented by QSE *q* at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP Status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h.* | | ASCAP1ADJ *q, i* | MW | *Ancillary Service Net Capacity Level 1 at End of Adjustment Period* ⎯The net capacity at the end of the Adjustment Period for Reg-Up for QSE *q*, for the 15-minute Settlement Interval *i*. | | ASCAP2ADJ *q, i* | MW | *Ancillary Service Net Capacity Level 2 at End of Adjustment Period* ⎯The net capacity at the end of the Adjustment Period for RRS for QSE *q*, for the 15-minute Settlement Interval *i*. | | ASCAP3ADJ *q, i* | MW | *Ancillary Service Net Capacity Level 3 at End of Adjustment Period* ⎯The net capacity at the end of the Adjustment Period for Reg-Up and RRS for QSE *q*, for the 15-minute Settlement Interval *i*. | | ASCAP4ADJ *q, i* | MW | *Ancillary Service Net Capacity Level 4 at End of Adjustment Period* ⎯The net capacity at the end of the Adjustment Period for Reg-Up, RRS, and ECRS for QSE *q*, for the 15-minute Settlement Interval *i*. | | ASCAP5ADJ *q, i* | MW | *Ancillary Service Net Capacity Level 5 at End of Adjustment Period* ⎯The net capacity at the end of the Adjustment Period for Reg-Up, RRS, ECRS, and Non-Spin for QSE *q*, for the 15-minute Settlement Interval *i*. | | ASCAP6ADJ *q, i* | MW | *Ancillary Service Net Capacity Level 6 at End of Adjustment Period* ⎯ The net capacity at the end of the Adjustment Period for Reg-Down for QSE *q*, for the 15-minute Settlement Interval *i*. | | ASOFR1ADJ *q, r, h* | MW | *Ancillary Service Offer Level 1 at End of Adjustment Period –* The capacity represented by validated Reg-Up Ancillary Service Offers for Resource *r* represented by QSE *q* at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR2ADJ *q, r, h* | MW | *Ancillary Service Offer Level 2 at End of Adjustment Period –* The capacity represented by validated RRS Ancillary Service Offers for Resource *r* represented by QSE *q* at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR3ADJ *q, r, h* | MW | *Ancillary Service Offer Level 3 at End of Adjustment Period –* The capacity represented by validated Reg-Up and RRS Ancillary Service Offers for Resource *r* represented by QSE *q* at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR4ADJ *q, r, h* | MW | *Ancillary Service Offer Level 4 at End of Adjustment Period –* The capacity represented by validated Reg-Up, RRS, and ECRS Ancillary Service Offers for Resource *r* represented by QSE *q* at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR5ADJ *q, r, h* | MW | *Ancillary Service Offer Level 5 at End of Adjustment Period–* The capacity represented by validated Reg-Up, RRS, ECRS, and Non-Spin Ancillary Service Offers for Resource *r* represented by QSE *q* at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | ASOFR6ADJ *q, r, h* | MW | *Ancillary Service Offer Level 6 at End of Adjustment Period –* The capacity represented by validated Reg-Down Ancillary Service Offers for Resource *r* represented by QSE *q* at the end of the Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. A Resource’s offered capacity is only included in the sum to the extent that the Resource’s COP status and Ancillary Service Capability indicate it would be capable of providing the Ancillary Service during the hour *h*. | | RTAML *q, p, i* | MWh | *Real-Time Adjusted Metered Load*—The QSE *q*’s Adjusted Metered Load (AML) at the Settlement Point *p* for the 15-minute Settlement Interval *i*. | | RUCCAPSNAP *ruc, q, i* | MW | *RUC Capacity Snapshot at time of RUC*—The amount of the QSE *q*’s calculated capacity in the RUC Snapshot for the RUC process *ruc* for a 15-minute Settlement Interval *i*. | | RCAPSNAP *ruc, q, r, h* | MW | *Resource Capacity at Snapshot*—The available capacity of Generation Resource or ESR *r,* that is not a DC-Coupled Resource, represented by the QSE *q*, according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. For ESRs and Generation Resources that are not IRRs, the available capacity shall be equal to HSL. For WGRs and PVGRs, the available capacity shall be equal to the WGRPP and the PVGRPP, respectively. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. | | *DCRCAPSNAP ruc, q, r, h* | MW | *DC-Coupled Resource Capacity at Snapshot*—The Resource Capacity of DC-Coupled Resource *r* represented by the QSE *q* for the hour *h*, according to the RUC Snapshot for the RUC process *ruc*. | | DCRCAPADJ *ruc, q, r, h* | MW | *DC-Coupled Resource Capacity at Adjustment Period*—The Resource Capacity of DC-Coupled Resource *r* represented by the QSE *q* for the hour *h*, at the end of the Adjustment Period. | | DCIMPSNAP *ruc, q, p, i* | MW | *DC Import at Snapshot*—The approved aggregated DC Tie Schedule submitted by QSE *q* as an importer into the ERCOT System through DC Tie *p*, according to the RUC Snapshot for the RUC process *ruc* for the 15-minute Settlement Interval *i*. | | RTDCIMP *q, p* | MW | *Real-Time DC Import per QSE per Settlement Point*—The aggregated final, approved DC Tie Schedule submitted by QSE *q* as an importer into the ERCOT System through DC Tie *p*, for the 15-minute Settlement Interval. | | RUCCPSNAP *ruc, q, h* | MW | *RUC Capacity Purchase at Snapshot*—The QSE *q*’s capacity purchase, according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. | | RUCCSSNAP *ruc, q, h* | MW | *RUC Capacity Sale at Snapshot*—The QSE *q*’s capacity sale, according to the RUC Snapshot for the RUC process *ruc* for the hour *h* that includes the 15-minute Settlement Interval. | | RUCCAPADJ *q, i* | MW | *RUC Capacity at End of Adjustment Period*—The amount of the QSE *q*’s calculated capacity, excluding capacity for IRRs and DC-Coupled Resources, at the end of the Adjustment Period for a 15-minute Settlement Interval *i.* | | RCAPADJ *q, r, h* | MW | *Resource Capacity at End of Adjustment Period*—The HSL of a non-IRR Generation Resource or ESR *r,* that is not a DC-Coupled Resource, represented by the QSE *q* at the end of the Adjustment Period, for the hour *h* that includes the 15-minute Settlement Interval. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. | | RUCCPADJ *q, h* | MW | *RUC Capacity Purchase at End of Adjustment Period*—The QSE *q*’s capacity purchase, at the end of Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. | | RUCCSADJ *q, h* | MW | *RUC Capacity Sale at End of Adjustment Period*—The QSE *q*’s capacity sale, at the end of Adjustment Period for the hour *h* that includes the 15-minute Settlement Interval. | | DAEP *q, p, h* | MW | *Day-Ahead Energy Purchase*—The QSE *q*’s energy purchased in the DAM at the Settlement Point *p* for the hour *h* that includes the 15-minute Settlement Interval. | | DAES *q, p, h* | MW | *Day-Ahead Energy Sale*—The QSE *q*’s energy sold in the DAM at the Settlement Point *p* for the hour *h* that includes the 15-minute Settlement Interval. | | RTQQEPSNAP *ruc, q, p, i* | MW | *Real-Time QSE-to-QSE Energy Purchase at Snapshot*—The QSE *q*’s Energy Trades in which the QSE is the buyer at the delivery Settlement Point *p* for the 15-minute Settlement Interval *i*, in the RUC Snapshot for the RUC process *ruc*. | | RTQQESSNAP *ruc, q, p, i* | MW | *Real-Time QSE-to-QSE Energy Sale at Snapshot*—The QSE *q*’s Energy Trades in which the QSE is the seller at the delivery Settlement Point *p* for the 15-minute Settlement Interval *i*, in the RUC Snapshot for the RUC process *ruc*. | | RTQQEPADJ *q, p, i* | MW | *Real-Time QSE-to-QSE Energy Purchase at End of Adjustment Period*—The QSE *q*’s Energy Trades in which the QSE is the buyer at the delivery Settlement Point *p* for the 15-minute Settlement Interval *i*, at the end of the Adjustment Period for that Settlement Interval. | | RTQQESADJ *q, p, i* | MW | *Real-Time QSE-to-QSE Energy Sale at End of Adjustment Period*—The QSE *q*’s Energy Trades in which the QSE is the seller at the delivery Settlement Point *p* for the 15-minute Settlement Interval *i*, at the end of the Adjustment Period for that Settlement Interval. | | *q* | none | A QSE. | | *p* | none | A Settlement Point. | | *r* | none | A Generation Resource, an ESR, or a Load Resource. | | *z* | none | A previous RUC process for the Operating Day. | | *i* | none | A 15-minute Settlement Interval. | | *h* | none | The hour that includes the Settlement Interval *i*. | | *ruc* | none | The RUC process for which this RUC Shortfall Ratio Share is calculated. | |