|  |  |  |  |
| --- | --- | --- | --- |
| NPRR Number | [1121](https://www.ercot.com/mktrules/issues/NPRR1121) | NPRR Title | Add a Posting Requirement to the Exceptional Fuel Cost Submission Process |
| Date of Decision | July 14, 2022 |
| Action | Approved |
| Timeline | Normal |
| Effective Date | Upon system implementation |
| Priority and Rank Assigned | Priority – 2022; Rank – 3590  |
| Nodal Protocol Sections Requiring Revision  | 4.4.9.4.1, Mitigated Offer Cap |
| Related Documents Requiring Revision/Related Revision Requests | None |
| Revision Description | This Nodal Protocol Revision Request (NPRR) replaces the Market Notice currently used in the Exceptional Fuel Cost submission process to notify Market Participants when such costs have been submitted for an Operating Day with an automated report. |
| Reason for Revision |  Addresses current operational issues. Meets Strategic goals (tied to the [ERCOT Strategic Plan](http://www.ercot.com/content/wcm/lists/144926/ERCOT_Strategic_Plan_2019-2023.pdf) or directed by the ERCOT Board). Market efficiencies or enhancements Administrative Regulatory requirements Other: (explain)*(please select all that apply)* |
| Business Case | Currently the Exceptional Fuel Cost submission process includes a Market Notice to communicate to the stakeholders when such costs have been submitted for an Operating Day. The Market Notice process can be time-consuming and requires coordination across ERCOT groups. This NPRR replaces the Market Notice process with an automated report, which is a more efficient long-term solution.  |
| Credit Work Group Review | ERCOT Credit Staff and the Credit Work Group (Credit WG) have reviewed NPRR1121 and do not believe that it requires changes to credit monitoring activity or the calculation of liability. |
| PRS Decision | On 3/9/22, PRS voted unanimously to recommend approval of NPRR1121 as submitted. All Market Segments participated in the vote.On 4/14/22, PRS voted unanimously to endorse and forward to TAC the 3/9/22 PRS Report and 2/22/22 Impact Analysis for NPRR1121 with a recommended priority of 2022 and rank of 3590. All Market Segments participated in the vote. |
| Summary of PRS Discussion | On 3/9/22, ERCOT Staff presented NPRR1121. Some participants questioned whether the automated report justified the anticipated cost of implementing NPRR1121. ERCOT Staff expressed hope costs savings might be realized by associating the project with others for new reporting requirements.On 4/14/22, Market Participants discussed a recommended priority and rank. ERCOT Staff confirmed that a Qualified Scheduling Entity’s (QSE’s) submission of Exceptional Fuel Cost will generate in an automated report being posted to the ERCOT website one day after the submission’s Operating Day. |
| TAC Decision | On 5/25/22, TAC voted unanimously to recommend approval of NPRR1121 as recommended by PRS in the 4/14/22 PRS Report. All Market Segments participated in the vote. |
| Summary of TAC Discussion | On 5/25/22, participants reviewed the 2/22/22 Impact Analysis. |
| ERCOT Opinion | ERCOT supports approval of NPRR1121. |
| ERCOT Market Impact Statement | ERCOT Staff has reviewed NPRR1121 and believes that it improves market communication and transparency by replacing the Market Notice currently used in the Exceptional Fuel Cost submission process to notify Market Participants when such costs have been submitted with an automated report. |
| Board Decision | On 6/21/22, the ERCOT Board voted unanimously to recommend approval of NPRR1121 as recommended by TAC in the 5/25/22 TAC Report. |
| PUCT Decision | On 7/14/22, the PUCT approved NPRR1121 and accompanying ERCOT Market Impact Statement as presented in Project No. 52934, Review of Rules Adopted by the Independent Organization. |

|  |
| --- |
| Sponsor |
| Name | Dave Maggio |
| E-mail Address | David.Maggio@ercot.com |
| Company | ERCOT |
| Phone Number | 512-248-6998 |
| Cell Number |  |
| Market Segment | Not applicable |

|  |
| --- |
| **Market Rules Staff Contact** |
| **Name** | Jordan Troublefield |
| **E-Mail Address** | Jordan.Troublefield@ercot.com |
| **Phone Number** | 512-248-6521 |

|  |
| --- |
| **Comments Received** |
| **Comment Author** | **Comment Summary** |
| None |  |

|  |
| --- |
| **Market Rules Notes** |

Please note that the following NPRR(s) also propose revisions to the following section(s):

* NPRR1058, Resource Offer Modernization
	+ Section 4.4.9.4.1

|  |
| --- |
| Proposed Protocol Language Revision |

4.4.9.4.1 Mitigated Offer Cap

(1) Energy Offer Curves may be subject to mitigation in Real-Time operations under Section 6.5.7.3, Security Constrained Economic Dispatch, using a Mitigated Offer Cap (MOC). ERCOT shall construct an incremental MOC curve in accordance with Section 6.5.7.3 such that each point on the MOC curve is calculated as follows:

|  |
| --- |
| ***[NPRR1014: Replace paragraph (1) above with the following upon system implementation:]***(1) Energy Offer Curves and Energy Bid/Offer Curves may be subject to mitigation in Real-Time operations under Section 6.5.7.3, Security Constrained Economic Dispatch, using a Mitigated Offer Cap (MOC). For Generation Resources, ERCOT shall construct an incremental MOC curve in accordance with Section 6.5.7.3 such that each point on the MOC curve is calculated as follows: |

MOC *q, r, h* = Max [GIHR *q, r* \* Max(FIP, WAFP *q, r, h*), (IHR *q, r* \* FPRC *q, r* + OM *q, r*) \* CFMLT *q, r*]

Where,

If a QSE has submitted an Energy Offer Curve on behalf of a Generation Resource and the Generation Resource has approved verifiable costs, then

FPRC *q, r* = Max(WAFP *q, r, h*, FIP + FA *q, r*) \* RTPERFIP *q, r* / 100 + FOP \* RTPERFOP *q, r* / 100

If a QSE has not submitted an Energy Offer Curve on behalf of a Generation Resource and the Generation Resource has approved verifiable costs, then

FPRC *q, r* = Max(WAFP *q, r, h*, FIP + FA *q, r*) \* GASPEROL *q, r* / 100 + FOP \* OILPEROL *q, r* / 100 + (SFP + FA *q, r*) \* SFPEROL *q, r* / 100

The above variables are defined as follows:

| Variable | Unit | Definition |
| --- | --- | --- |
| MOC *q, r, h* | $/MWh | *Mitigated Offer Cap per Resource*—The MOC for Resource *r*, for the hour. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| GIHR *q, r* | MMBtu/MWh | *Generic Incremental Heat Rate*—The generic, single-value, incremental heat rate. For Generation Resources with a Commercial Operations Date on or before January 1, 2004, the generic incremental heat rate shall be set to 10.5. For Generation Resources that have a Commercial Operations Date after January 1, 2004, this value shall be set to 14.5. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| IHR *q, r* | MMBtu/MWh | *Verifiable Incremental Heat Rate per Resource*—The verifiable incremental heat rate curve for Resource *r,* as approved in the verifiable cost process. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| FIP | $/MMBtu | *Fuel Index Price*—The natural gas index price as defined in Section 2.1, Definitions. |
| RTPERFIP *q, r* | none | *Fuel Index Price Percentage*—The percentage of natural gas used by Resource *r* to operate above LSL, as submitted with the energy offer curve. |
| FOP | $/MMBtu | *Fuel Oil Price*—The fuel oil index price as defined in Section 2.1. |
| RTPERFOP *q, r* | none | *Fuel Oil Price Percentage*—The percentage of fuel oil used by Resource *r* to operate above LSL, as submitted with the energy offer curve. |
| SFP | $/MMBtu | *Solid Fuel Price—*The solid fuel index price is $1.50.  |
| FPRC *q, r* | $/MMBtu | *Fuel Price Calculated per Resource*—The calculated index price for fuel for the Resource based on the Resources fuel mix. Where for a Combined Cycle Train, the Resource r is a Combined Cycle Generation Resource within the Combined Cycle Train.  |
| GASPEROL *q, r* | none | *Percent of Natural Gas to Operate Above LSL*—The percentage of natural gas used by Resource *r* to operate above LSL, as approved in the verifiable cost process. Where for a Combined Cycle Train, the Resource r is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| OILPEROL *q, r* | none | *Percent of Oil to Operate Above LSL*—The percentage of fuel oil used by Resource *r* to operate above LSL, as approved in the verifiable cost process. Where for a Combined Cycle Train, the Resource r is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| SFPEROL *q, r* | none | *Percent of Solid Fuel to Operate Above LSL*—The percentage of solid fuel used by Resource *r* to operate above LSL, as approved in the verifiable cost process. Where for a Combined Cycle Train, the Resource r is a Combined Cycle Generation Resource within the Combined Cycle Train. |
| FA *q, r* | $/MMBtu | *Fuel Adder*—The fuel adder is the average cost above the index price Resource *r* has paid to obtain fuel. Where for a Combined Cycle Train, the Resource *r* is a Combined Cycle Generation Resource within the Combined Cycle Train. See the Verifiable Cost Manual for additional information. |
| OM *q, r* | $/MWh | *Variable Operations and Maintenance Cost above LSL*—The O&M cost for Resource *r* to operate above LSL, including an adjustment for emissions costs, as approved in the verifiable cost process. Where for a Combined Cycle Train, the Resource r is a Combined Cycle Generation Resource within the Combined Cycle Train. See the Verifiable Cost Manual for additional information. |
| CFMLT *q, r* | none | *Capacity Factor Multiplier*—A multiplier based on the corresponding monthly capacity factor as described in paragraph (1)(d) below.  |
| WAFP *q, r, h* | $/MMBtu | *Weighted Average Fuel Price*—The volume-weighted average intraday, same-day and spot price of fuel submitted to ERCOT during the Adjustment Period for a specific Resource and specific hour within the Operating Day, as described in paragraph (1)(f) below.  |
| *q* | none | A QSE. |
| *r* | none | A Generation Resource. |
| *h* | none | The Operating Hour.  |

(a) For a Resource contracted by ERCOT under paragraph (4) of Section 6.5.1.1, ERCOT Control Area Authority, ERCOT shall increase the O&M cost such that every point on the MOC curve is greater than the SWCAP in $/MWh.

|  |
| --- |
| ***[NPRR1008 and NPRR1014: Replace applicable portions of paragraph (a) above with the following upon system implementation of the Real-Time Co-Optimization (RTC) project for NPRR1008; or upon system implementation for NPRR1014:]***(a) For a Resource contracted by ERCOT under paragraph (4) of Section 6.5.1.1, ERCOT Control Area Authority, ERCOT shall increase the O&M cost such that every point on the MOC curve is greater than the effective Value of Lost Load (VOLL) in $/MWh. |

(b) Notwithstanding the MOC calculation described in paragraph (1) above, the MOC for ESRs shall be set at the SWCAP. No later than December 31, 2023, ERCOT and stakeholders shall submit a report to TAC that includes a recommendation to continue the existing approach or a proposal to implement an alternative approach to determine the MOC for ESRs.

|  |
| --- |
| ***[NPRR1008 and NPRR1014: Replace applicable portions of paragraph (b) above with the following upon the system implementation of the Real-Time Co-Optimization (RTC) project for NPRR1008; or upon system implementation for NPRR1014:]***(b) Notwithstanding the MOC calculation described in paragraph (1) above, the MOC for ESRs shall be set at the RTSWCAP. No later than December 31, 2023, ERCOT and stakeholders shall submit a report to TAC that includes a recommendation to continue the existing approach or a proposal to implement an alternative approach to determine the MOC for ESRs. |

(c) For Quick Start Generation Resources (QSGRs) the MOC shall be adjusted in accordance with Verifiable Cost Manual Appendix 7, Calculation of the Variable O&M Value and Incremental Heat Rate used in Real Time Mitigation for Quick Start Generation Resources (QSGRs).

|  |
| --- |
| ***[NPRR1008 and NPRR1014: Insert applicable portions of paragraph (d) below upon system implementation of the Real-Time Co-Optimization (RTC) project for NPRR1008; or upon system implementation for NPRR1014; and renumber accordingly:]***(d) For On-line hydro Generation Resources not operating in Synchronous Condenser Fast-Response mode, the MOC shall be adjusted in accordance with Verifiable Cost Manual, Appendix 12, Calculation of the Variable O&M Value and Incremental Heat Rate used in Real Time Mitigation for On-Line Hydro Generation Resources not operating in Synchronous Condenser Fast-Response mode. |

(d) The multipliers for the MOC calculation above are as follows:

(i) 1.10 for Resources running at a ≥ 50% capacity factor for the previous 12 months;

(ii) 1.15 for Resources running at a ≥ 30 and < 50% capacity factor for the previous 12 months;

(iii) 1.20 for Resources running at a ≥ 20 and < 30% capacity factor for the previous 12 months;

(iv) 1.25 for Resources running at a ≥ 10 and < 20% capacity factor for the previous 12 months;

(v) 1.30 for Resources running at a ≥ 5 and < 10% capacity factor for the previous 12 months;

(vi) 1.40 for Resources running at a ≥ 1 and < 5% capacity factor for the previous 12 months; and

(vii) 1.50 for Resources running at a less than 1% capacity factor for the previous 12 months.

(e) The previous 12 months’ capacity factor must be updated by ERCOT by the 20th day of each month using the most recent data for use in the next month. ERCOT shall post to the MIS Secure Area the capacity factor for each Resource before the start of the effective month.

(f) During the Adjustment Period, a QSE representing a Resource may submit Exceptional Fuel Cost as a volume-weighted average fuel price for use in the MOC calculation for that Resource. To qualify as Exceptional Fuel Cost, the submission must meet the following conditions:

(i) For all Resources, the weighted average fuel price must exceed FIP for the applicable Operating Day, plus a threshold parameter value of $1/MMBtu, plus the applicable fuel adder. For Resources without approved verifiable costs, the fuel adder will be set to the default value assigned to Resources with approved verifiable costs, as defined in the Verifiable Cost Manual. The threshold parameter value in this paragraph shall be recommended by the Wholesale Market Subcommittee (WMS) and approved by the Technical Advisory Committee (TAC). ERCOT shall update the threshold value on the first day of the month following TAC approval unless otherwise directed by the TAC. ERCOT shall provide a Market Notice prior to implementation of a revised parameter value.

(ii) Fixed cost (fees, penalties and similar non-gas costs) may not be included in the calculation of the weighted average fuel price.

(iii) All intra-day, same day, and spot fuel purchases must be included in the calculation of the weighted average fuel price in paragraph (1) above. These must account for at least 10% of the total fuel volume burned by the applicable Resource for the hour for which the weighted average fuel price is computed. As noted in paragraph (l) below, the methodology used in the allocation of the cost and volume of purchased fuel to the Resource for the hour is subject to validation by ERCOT.

(iv) Weighted average fuel prices must be submitted individually for each Operating Hour for which they are applicable. Values submitted outside of the Adjustment Period will be rejected and not used in the calculation of the MOC for the designated Operating Hour.

(g) ERCOT may notify the Independent Market Monitor (IMM) if a QSE submits an Exceptional Fuel Cost.

(h) The day following an Operating Day for which an Exceptional Fuel Cost is submitted, ERCOT shall post a report on the ERCOT website indicating the affected Operating Hours and the number of Resources for which a QSE submitted Exceptional Fuel Cost for a particular Operating Day.

(i) No later than 1700 Central Prevailing Time (CPT) on the 15th day following an Exceptional Fuel Cost submission, the submitting QSE shall provide ERCOT with the calculation of the weighted average fuel price, intraday or same-day fuel purchases, and any available supporting documentation. Such information may include, but is not limited to, documents of the following nature: relevant contracts between the QSE or Resource Entity and fuel supplier, trade logs, transportation, storage, balancing and distribution agreements, calculation of the weighted average fuel price, or any other documentation necessary to support the Exceptional Fuel Cost price and volume for the applicable period(s).

(j) No later than 1700 Central Prevailing Time (CPT) on the 60th day following an Exceptional Fuel Cost submission, the submitting QSE shall provide ERCOT with all supporting documentation not previously provided to ERCOT. No supporting documentation will be accepted after the 60th day.

(k) The accuracy of submitted Exceptional Fuel Cost and the need for purchasing intraday or same-day gas must be attested to by a duly authorized officer or agent of the QSE representing the Resource. The attestation must be provided in a standardized format acceptable to ERCOT and submitted with the other documentation described in paragraph (i) above.

(l) ERCOT will use the supporting documentation to validate the Exceptional Fuel Cost for the applicable period. Validation will include, but not be limited to, the cost and the quantity of purchased fuel, Resource-specific heat rates, and the methodology used in the allocation of the cost and volume of purchased fuel to the Resource for the applicable hour used in the weighted average fuel price calculation. In connection with the validation process ERCOT may request additional documentation or clarification of previously submitted documentation. Such requests must be honored within ten Business Days.

(m) At ERCOT’s sole discretion, submission and follow-up information deadlines may be extended on a case-by-case basis.