**July 25, 2022**

**Definition of Large Flexible Load**

A stand-alone Load interconnected to ERCOT greater than 75.0 MWs or is co-located load (with generation and Load) greater than 20 MWs that meets the requirements of one of the following:

**SCED Flexible Load**

A connected large load dispatched by SCED and is:

1. capable of operating at an ERCOT specified Base Point and responding by changing its load level to subsequent Base Points issued by ERCOT at a specified ramp rate without physical damage to its internal processes used by that load’s business functions.

**Interruptible Load**

A connected large load that:

1. If load is co-located provides continuously telemetered generation, updated every 2 seconds

1. provides continuously telemetered load power information to ERCOT, updated every 2 seconds,
2. is not considered an ERCOT Load Resource and does not provide an Ancillary Service,
3. is capable of interrupting its load at a specified ramp rate when instructed by ERCOT,
4. agrees not to return to normal load levels until instructed by ERCOT