**DEFINITION**

**Interruptible Load:** Load registered to participate in the RTM as Load Resource or ERS and, when not participating as LR or ERS, curtailable by ERCOT using a Manual Load Shed instruction in EEA through the Load’s QSE and thereby excluded from TO’s Manual Load Shed and UFLS obligation calculations.