September 14, 2022

**Definition of Large Flexible Load**

A Load greater than or equal to 75.0 MWs that meets the requirements of one of the following:

**SCED Flexible Load**

 A large load dispatched by SCED and is capable of operating at an ERCOT specified Base Point and responding by changing its load level to subsequent Base Points issued by ERCOT at a specified ramp rate, or

**Interruptible Load**

 A large load that:

1. provides continuously telemetered load power information to ERCOT, updated every 2 seconds,
2. If load is co-located with generation, the generation provides continuously telemetered power, updated every 2 seconds,
3. is not considered an ERCOT Load Resource and does not provide an Ancillary Service,
4. is capable of interrupting its load at a specified ramp rate when instructed by ERCOT for transmission issues or system capacity needs, and
5. agrees not to return to normal load levels until instructed by ERCOT.