**Texas**

**Standard**

**Electronic**

**Transaction**

**814\_21:**

##### ESI ID Maintenance Response

Electronic Data Interchange

ANSI ASC X12 Ver/Rel 004010

Transaction Set 814

**Texas 814\_21:**

ESI ID Maintenance Response

This transaction set:

... from ERCOT to TDSP, is used to respond to the 814\_20 Create/Maintain/Retire ESI ID Request.

... from the current CR to ERCOT, is no longer valid as of TX SET 4.0.

... from the new CR to ERCOT, is no longer valid as of TX SET 4.0.

Document Flow:

* ERCOT to TDSP

The Functional Acknowledgement (997) transaction set from the receiver of the originating transaction to the sender of the originating transaction, is used to acknowledge the receipt of the originating transaction and indicate whether the transaction passed ANSI X12 validation. This acknowledgement does not imply that the originating transaction passed Texas SET validation. “CR, TDSP, or ERCOT shall respond with a 997 within 24 hours of receipt of an inbound transaction.”

|  |  |  |
| --- | --- | --- |
|  |  | **Summary of Changes** |
| November 30, 2010  Version 3.0A |  | Initial Release |
| June 11, 2012  Version 4.0 |  | Updated examples for TX SET 4.0 |
| November 11, 2024  Version 5.0 |  | No changes for Texas SET 5.0 |

814\_21 Example #1 of 2

Create ESI ID Accept Response – ERCOT to TDSP

|  |  |  |
| --- | --- | --- |
| ERCOT to TDSP Create ESI ID Request is Accepted | | |
| ST~814~000000001 | | Transaction Type, Transaction Set Control Number |
| BGN~11~200805101201001~20080510~~~200805101956534~~21 | | Response, Unique Transaction Number, Transaction Date, Original Transaction ID, SET Transaction Number |
| N1~8S~TDSP NAME~1~009876543~~40 | | TDSP Name and DUNS Number, Receiver |
| N1~AY~ERCOT~1~183529049~~41 | | ERCOT Name and DUNS Number, Sender |
| LIN~1~SH~EL~SH~MP | | Maintain Premise |
|  | ASI~WQ~021 | Accept Addition |
|  | REF~Q5~~12345678910111231 | ESI ID |
| SE~8~000000001 | | Number of Segments, Transaction Set Control Number |

814\_21 Example #2 of 2

Maintain ESI ID Notification Accept Response – ERCOT to TDSP

|  |  |  |
| --- | --- | --- |
| ERCOT to TDSP Change ESI ID information – Notification of a Change in Read Cycle ERCOT Accepts Change in Read Cycle | | |
| ST~814~000000001 | | Transaction Type, Transaction Set Control Number |
| BGN~11~200805101201001~20080510~~~200805101956534~~21 | | Response, Unique Transaction Number, Transaction Date, Original Transaction ID, SET Transaction Number |
| N1~8S~TDSP NAME~9~9876543211000~~40 | | TDSP Name and DUNS Number, Receiver |
| N1~AY~ERCOT~1~183529049~~41 | | ERCOT Name and DUNS Number, Sender |
| LIN~1~SH~EL~SH~MP | | Maintain Premise |
|  | ASI~WQ~001 | Accept Change |
|  | REF~Q5~~12345678910111231 | ESI ID |
| SE~8~000000001 | | Number of Segments, Transaction Set Control Number |