Summary of Nodal Operating Guide Revisions

Effective:  August 1, 2026
Section 2:
NOGRR282 – Board Priority - Large Computational Load Ride-Through Requirements
This Nodal Operating Guide Revision Request (NOGRR) establishes frequency and voltage ride-through requirements for Large Computational Loads (LCLs).
Revised Subsections:  2.6.4 (new) and 2.15 (new)
NOGRR283 – Board Priority - Related to NPRR1309, Dispatchable Reliability Reserve Service Ancillary Service

This Nodal Operating Guide Revision Request (NOGRR) develops Dispatchable Reliability Reserve Service (DRRS) as a new Ancillary Service; and given that DRRS has at least a four-hour duration, the Non-Spinning Reserve (Non-Spin) duration requirements are reduced from four hours to two hours.

Revised Subsections:  2.3, 2.3.2.1, 2.3.4 (new), and 2.3.4.1 (new) [effective upon system implementation of Nodal Protocol Revision Request (NPRR) 1309, Dispatchable Reliability Reserve Service Ancillary Service]
Section 6:
NOGRR255 – High Resolution Data Requirements
This Nodal Operating Guide Revision Request (NOGRR) establishes high resolution data requirements. 

Revised Subsections:  6.1.2.2 and 6.1.3.2.2 [unboxed due to effective date of August 1, 2026] 
Section 9:
NOGRR283 – Board Priority - Related to NPRR1309, Dispatchable Reliability Reserve Service Ancillary Service

See Section 2 above.

Revised Subsection:  9.4.5 (new) [effective upon system implementation of Nodal Protocol Revision Request (NPRR) 1309]
Section 11:
NOGRR281 – Related to NPRR1307, Revised Definition of Mitigation Plan

This Nodal Operating Guide Revision Request (NOGRR) modifies when an approved Mitigation Plan can be executed.

Revised Subsection:  11.5 [effective upon system implementation of Nodal Protocol Revision Request (NPRR) 1307, Revised Definition of Mitigation Plan]
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