Summary of Nodal Protocol Revisions
Effective:  October 29, 2026

Section 2:
NPRR1198 – Congestion Mitigation Using Topology Reconfigurations
This Nodal Protocol Revision Request (NPRR) defines Extended Action Plan (EAP), revises the defined term Remedial Action Plan (RAP), adds EAP and RAP as types of Constraint Management Plan (CMP) suitable for the market use of the ERCOT Transmission Grid, and removes language limiting the application of these CMPs to congestion issues for which there exists no feasible Security-Constrained Economic Dispatch (SCED) solution.
Revised Subsection:  2.1 [unboxed due to system implementation]
Section 3:
[bookmark: _Hlk207268233]NPRR1281 – Improvements to Alternate FFSS Resource Designation
[bookmark: _Hlk207268246]This Nodal Protocol Revision Request (NPRR) strengthens the relationship between the Settlement of Firm Fuel Supply Service (FFSS) and operations by clarifying the FFSS Hourly Rolling Equivalent Availability Factor language to ensure the accurate calculation of the Firm Fuel Supply Service Standby Fee.
Revised Subsection:  3.14.5 [unboxed due to system implementation]
Section 6:
NPRR1198 – Congestion Mitigation Using Topology Reconfigurations
See Section 2 above.
Revised Subsection:  6.5.1.1 [unboxed due to system implementation]
NPRR1327 – As-Built for NPRR1281, Improvements to Alternate FFSS Resource Designation
This Nodal Protocol Revision Request (NPRR) documents the as-built solution for NPRR1281, Improvements to Alternate FFSS Resource Designation.
Revised Subsection:  6.6.14.2 [unboxed due to system implementation]
Section 8:
NPRR1281 – Improvements to Alternate FFSS Resource Designation
See Section 3 above.
Revised Subsection:  8.1.1.2.1.6 [unboxed due to system implementation]
NPRR1327 – As-Built for NPRR1281, Improvements to Alternate FFSS Resource Designation
See Section 6 above.
Revised Subsection:  8.1.1.2.1.6 [unboxed due to system implementation]
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