	ERCOT Operating Procedure Manual

Reliability Unit Commitment (RUC) Desk
	



Power Operations Bulletin # 2033
ERCOT has posted/revised the Reliability Unit Commitment manual.

The Various Changes are shown below.

A copy of the procedure can be found at:

http://www.ercot.com/mktrules/guides/procedures/index.html
3.2
Review, Approve and Post HRUC Results

Procedure Purpose:  Monitor RUC applications to determine if systems are functioning properly.  Verify results and correct for any warning or error messages.  Review and approve final results for market posting.

	Protocol Reference


	4.4.8
	5.1
	5.3(3)
	5.5.1

	
	5.5.2
	5.5.3
	6.1(2)
	6.4.9.1.2

	Guide Reference
	
	
	
	

	NERC Standard


	EOP-011-4

R2, R2.2, R2.2.3, R2.2.3.1
	IRO-001-4

R1
	TOP-001-6

R1, R2
	TOP-002-4 R1, R2, R3, R4, R4.1, R4.4, R5


	Version: 2 
	Revision: 1
	Effective Date:  July 29, 2026


	Step
	Action

	Note
	See Desktop Guide Common to Multiple Desks Section 2.16 if the savecase function fails when running RUC

	Monitor
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>HRUC Displays>Workflow>HRUC Workflow

Market Operation>Reliability Unit Commitment>HRUC Displays>Workflow>HRUC Workflow Messages

· Monitor the HRUC Workflow display to determine when it is complete, 

ENSURE: 
· The workflow has completed before the study is approved and published.  

IF:

· The study is approved before it completes,

· Incorrect RUC deployments are sent to QSE’s 

THEN:
· Make hotline call to notify QSE’s that deployments for HRUC are invalid,

· Notify Director Control Room Operations and/or Designee,

· ERCOT may use information from the DAM processes as decision support during the HRUC processes.

	System Summary
	REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>HRUC Displays>UC Displays>Output Display Menu>System Outputs>Summary

IF:

· All load forecasts seem unreasonable;

THEN:

· Select the most reasonable forecast, AND

· Call the Load Forecasting group for guidance on updating the weather or load forecast

· Notify by e-mail the following distribution lists of the issue:

· Load Forecasting Department

· 1 ERCOT Shift Supervisors



	Excess Generation
	During periods of low load and excess generation:

PERIODICALLY REVIEW:

· Splunk Dashboard Viewer under the MOS_DEV folder:

· “Last Approved HRUC Capacity” which is based on the last ran HRUC solution

VERIFY:

· TOTAL_LOAD is less than SS_LSL,

IF:

· Load forecast is reasonable AND the decision needs to be made in the near future,

THEN:

· Decommit generation from the HRUC next study,

· Priority should be on WGR’s or Resources that resolve congestion;

IF:

· The decision needs to be made immediately,

THEN:

· Issue an electronic Dispatch Instruction confirmation

·  Priority should be given to WGRs and Resources that resolve congestion 

· Choose “DECOMMIT” as the Instruction Type from Resource tab
· Enter “ERCOT requested RUC decommit/capacity surplus” in Other Information.
When issuing a VDI or confirmation, ensure the use of three-part communication:

· Issue the Operating Instruction

· Receive a correct repeat back

· Give an acknowledgement

	STNET Study
	The Transmission and Security Desk Operator has the primary responsibility to perform these voltage studies, however if needed as a backup this step is provided.

Each hour run a STNET study for two hours out (example it is 0100, run study for 0300) to review voltage violations. 

IF:

· Voltage contingencies exist;
THEN:

· Check “Voltage Tracking Issues” spreadsheet on SharePoint to ensure the contingency is not listed

· If not listed, convey the voltage violations to the Transmission and Security Desk Operator with the potential resolution

· Create a savecase, use naming convention “SC_RUC(HE)_(DATE)

· Make at least one detailed log entry per shift that the studies are being executed.   If any new voltage violations are identified that do not have a solution, log the information, and notify the Transmission and Security Desk Operator of the new violation(s)

· Update the “Voltage Tracking Issues” spreadsheet listing the new voltage violation with the contingency resolution.

IF:

· Unsolved contingencies exist;
THEN:

· Communicate any unsolved contingency to the Shift Engineer and Transmission and Security Desk Operator with potential solutions.

· Some potential solutions could be transmission switching, creation of a manual constraint, bringing on an additional Resource, returning a planned outage, or development of a CMP

· Validate the resolution

· Update the “Voltage Tracking Issues” spreadsheet listing the new unsolved contingency with the contingency resolution.

	Violated Constraints
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>HRUC Displays>DSP Displays> DSP Binding Constraint Summary

Market Operation>Reliability Unit Commitment>HRUC Displays>DSP Displays> DSP Constraint Summary

REVIEW:

· Violated constraints.  If needed, notify Operations Support Engineer to determine the validity; 

IF:

· Invalid, no further action is required;

IF:

· Valid; AND

· Related to a phase shifter tap settings,

THEN:

· Notify Operations Support Engineer to determine if adjusting a Phase Shifter would reduce the flow, 

· Create Suggestion Plan for Constraint,

· Manually RUC commit resources as needed, 

IF:

· Valid; AND no Suggestion Plan or Resource is available to commit within the timeframe of the violated constraint,

THEN:

· Notify the Operations Support Engineer and Transmission and Security Desk Operator to determine if an outage can be withdrawn within the timeframe, 

IF:

· No outage can be withdrawn within the timeframe of the violated constraint,

THEN:

· Notify Operations Support Engineer to develop a Congestion Management Plan and provide it to the TO and Transmission and Security Desk Operator, Notify Shift Supervisor to contact the Director Control Room Operations and/or Designee of actions taken

Refer to Desktop Guide RUC Section 2.14.

	Capacity Reserve Margin
	Monitor:

· Available Committed Capacity Margin and the Available Capacity Margin columns.
IF:

· If the Available Committed Capacity Margin threshold is less than minimum requirement OR;

· If the Available Capacity Margin threshold is less than the minimum requirements:

THEN:

· Inform Shift Supervisor
Refer to Desktop Guide RUC Section 2.24

	HRUC Committed

Units
	REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>HRUC Displays>DSI Displays>External Input Data>MF Generator Parameter
IF:

· HRUC recommends the commitment of any unit;
THEN:

· Determine the validity, 

· Determine the temporal constraints for each of the unit’s recommendation.

· Refer to Desktop Guide RUC Section 2.23.

IF:

· Temporal constraint exceedances at the same facility do not conflict,

· The resource start-up time allows enough time to re-evaluate the need for its commitment in future HRUC Study Periods, and 

· There is no reliability reason requiring the resource commitment decision to be made immediately;

THEN:

· De-select the resource prior to approving the HRUC study by changing ‘Commit’ to ‘blank’ and list reason,

IF:

· Temporal constraint exceedances at the same facility,

· There is a reliability reason requiring the resource commitment decision to be made immediately;

· Resources returning from outages

· Congestion or Capacity deficiencies that are creating HRUC performance issues

THEN:

· Log the reason for not de-selecting the resource.

NOTE:  A reason must be entered for commit, decommit, and uncommitting, otherwise a message window will pop up in DSP approval process.

Examples below:
· Evaluate later (should be used when waiting until the last possible hour to commit)

· Short start (should be used for units that can start within 1 hour)

· Voltage support 

· Valley import

· Valley Reliability

· Capacity
· Capacity (AS shortage)
· Constraint name (SLWSCRL5) * Do not use special characters

· Minimum Run Time

When issuing a confirmation, ensure the use of three-part communication:

· Issue the Operating Instruction

· Receive a correct repeat back

· Give an acknowledgement



	EMR Resources
	Resources with “EMR” Resource status can only be RUC committed during Emergency conditions.

	RMR

Resources
	QSEs will show a COP status of EMR when Resources are available.  RMR Resources will only be dispatched from the Hourly Reliability Unit Commitment (HRUC).

	RMR

Commitment
	WHEN:

· The Resource is needed for transmission congestion to mitigate a potential transmission exceedance that will affect reliability and no other market Resources are available, OR
· A capacity reserve shortage is projected, and no market Resources are available to meet the projected system demand, and there is a risk of an EEA event; 
THEN:

· Determine if an RMR Resource will need to be considered in HRUC Study Period;

ISSUE:

· Watch for projected reserve capacity shortage with no market solution;

THEN:

· Ensure COP status is “EMR”, and the resource start-up time allows enough time to procure the RMR for the hours showing to be deficient with risk of an EEA event;
SELECT:

· Commit Resource before HRUC is approved
· Commit Resource,

· List the Reliability reason (RMR for Transmission or Capacity).
NOTE: If a RMR Resource is committed for a Reliability reason, identify the transmission constraint or reason in the commitment instruction.

Call QSE with any modification to the Delivery Plan as a result of a commitment.

	Hotline
	Q#77 - Typical Hotline Script for Watch for projected reserve capacity shortage 
Notify the Transmission and Security Desk Operator to make Hotline call to TOs.

	Post
	Typical ERCOT Website posting: 

ERCOT issued a Watch for a projected reserve capacity shortage with no market solution available. HRUC recommended RMR Resources have been committed.

	Cancel
	WHEN:

· Committed RMR Resources are off-line

THEN:

· Making hotline call to QSEs

· Cancelling ERCOT Website posting

· Notify the Transmission and Security Desk Operator to make hotline call to TOs.

Q#78 - Typical Hotline Script for canceling Watch for projected reserve capacity shortage 



	Manual Commitment
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>HRUC Displays>DSP Displays> DSP RUC Commitment/Decommitment Summary

Market Operation>Reliability Unit Commitment>HRUC Displays>DSI Displays> External Input Data>MF Generator Parameters

IF:

· Additional resources are needed to solve for transmission issues (such as for voltage support) and were not picked up in the HRUC run;
THEN:

· RUC commit unit before HRUC is approved
· Change ‘blank’ to ‘Commit’,

· List reason RUC commit for (constraint name, valley import or voltage support), a message window will pop up in DSP approval process if no reason is provided.

· Give courtesy call to QSE when commitments are made

	Manual Commitment to bring a Unit of a Combined Cycle On-line 
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>HRUC Displays>DSP Displays>DSP Combined Cycle Plant Suggestion Plan
IF:

· Additional resources are needed to solve for transmission issues  and were not picked up in the HRUC run;
THEN:

· RUC commit higher configuration of a Combined Cycle before HRUC is approved
· Determine the temporal constraints for the higher configuration.

· Change ‘blank’ to ‘Commit’,

· List reason RUC commit for (constraint name, valley import or voltage support), a message window will pop up in DSP approval process if no reason is provided.

· Give courtesy call to QSE when commitments are made

Refer to Desktop Guide Reliability Unit Commitment Desk 2.20

	Note
	· Resources cannot be decommitted for just a portion of a DAM-Committed Interval, which is a one-hour interval.  

· ERCOT may only decommit a Resource to resolve transmission constraints that are otherwise unsolvable or to maintain the reliability of the ERCOT System.  Qualifying Facilities (QFs) may be decommitted only after all other types of Resources have been assessed for decommitment. 

· If ERCOT communicates HRUC commitments and decommitments verbally to a QSE, then the same Resource attributes communicated programmatically must be communicated when ERCOT gives a verbal Resource commitment or decommitment.

· QSE’s shall acknowledge the notice of commit or decommit by updating their COP.

	HRUC  Decommitted

Resources
	REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>HRUC Displays>DSP Displays> DSP RUC Commitment/Decommitment Summary
IF:

· If HRUC recommends decommitments; 

Determine if: 

· Outage related,
· Possible Network Model error/ Normal Breaker status variances,
· COP error for Combine Cycle configurations / JOU,
· Qualifying Facilities should be de-committed ONLY as a last resort, 
THEN:

· If this is a true decommitment:

· Confirm Decommitment

· List reason (most likely reason is ‘transmission outage’), a message window will pop up in DSP approval process if no reason is provided

· If Decommitment is error related:

· No action is required

	Note
	Canceling unintended RUC Commits must be completed before additional RUC Commitments are issued on the same Resource(s). Doing it after the new RUC Commitment cancels all RUC Commitments for the resource.

	Canceling

RUC

Commitments
	REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>HRUC Displays>DSI Displays>DSI Data Processes>DSI Operator Manual Commitment
IF:

· A Resource is RUC committed that needs to be canceled;
· Only cancel RUC commits if the ERCOT Operator Resource commitment was unintended.

THEN:

· Issue electronic Dispatch Instruction to cancel the RUC instruction
· Choose “CANCEL RUC COMMIT” as the Instruction Type

· Enter “unintended commitment” in other information
When issuing a VDI or confirmation, ensure the use of three-part communication:

· Issue the Operating Instruction

· Receive a correct repeat back

· Give an acknowledgement      


	Post
	Notice Type: Operational Information
Notice Priority: Low

Audience: Public
Typical ERCOT Website posting: 

Cancelled RUC commitment at timestamp [Date & Time] for [resource] for [Date & Time] due to unintended commitment.

	VSAT and RUC perform AC Analysis

	Note
	IF:

· RUC cannot complete the process;
THEN:

· Notify the Transmission and Security Desk Operator and additional personnel as required. 

	Validate
	REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>HRUC Displays>UC Displays>Output Display Menu>System Outputs>Summary

VERIFY:

· Input data

· Updated Time

· Results are reasonable

	Approval
	HRUC must be approved by XX:50

REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>HRUC Displays>DSP Displays> DSP Execution Control Parameters

IF:

· The HRUC results are reasonable and after all necessary modifications have been made;

THEN:

· Sort the RUC Commitment column before approving so it shows commitments at the top of the screen that currently may be lower in the table but not shown in the window;
· Approve the results (all RUC commitment, operator manual commitment/decommit/blank out must have a reason, otherwise a message window will pop up), OR

IF:

· The results are unacceptable;

THEN:

· Click on Disapprove button, AND
· Follow the Manage HRUC Timeline Failure in the next section.

IF:

· Disapprove button was selected in error;

THEN:

· Contact Service Desk to open ticket for EMMS Production Support to correct it.

	After 

Approval
	AFTER:

· Approval button is pushed;

THEN:

· Double check display Market Participation>Physical Market>Market Results>HRUC> HRUC Results, 

· Make sure the records in this display matches data in display Market Operation>Reliability Unit Commitment>HRUC Displays >DSP Displays>DSP RUC Commitment/Decommitment Summary.
IF:

· Displays are different, the RUC commitments thought to be blanked out were sent out;

THEN:

· Notify the Service Desk to call the On-Call EMMS Production support, and
· Issue electronic Dispatch Instructions to cancel RUC instructions
When issuing a VDI or confirmation, ensure the use of three-part communication:

· Issue the Operating Instruction

· Receive a correct repeat back

· Give an acknowledgement

	Log
	Log actions taken.


4.3
Review, Approve and Post DRUC Results

Procedure Purpose:  To work collaboratively with Market Operations Support Personnel in reviewing, and if necessary, modifying DRUC data, to approve and post the final DRUC results.

	Protocol Reference
	4.4.8
	5.1 (9)
	5.3(3)
	5.5.1(9)

	
	5.5.2
	5.5.3(2)
	6.4.9.1(3)
	

	Guide Reference
	
	
	
	

	NERC Standard


	IRO-008-3 

R1, R2, R3, R7
	TOP-001-6 R25
	TOP-002-4 R1, R2, R3, R4, R4.1,  R4.4, R5
	


	Version: 2 
	Revision: 1
	Effective Date:  July 29, 2026


	Step
	Action

	Note
	See Desktop Guide Common to Multiple Desks Section 2.16 if the savecase function fails when running RUC

	Monitor
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>DRUC Displays>Workflow>DRUC Workflow

Market Operation>Reliability Unit Commitment>DRUC Displays>Workflow>DRUC Workflow Messages

	Review
	REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>DRUC Displays>UC Displays>Output Display Menu>System Outputs>Summary 

When DRUC has completed.  If necessary, work with Market Operations and Operations Support Engineer to review the results.

· Monitor the DRUC Workflow display to determine when it is complete, 

ENSURE: 
· The workflow has completed before the study is approved and published,  

IF:

· The study is approved before it completes,

· Incorrect RUC deployments are sent to QSE’s 

THEN:
· Make hotline call to notify QSE’s that deployments for DRUC are invalid,

· Notify the Director Control Room Operations and/or Designee immediately,

· Abnormal system condition in the summary display after IUC (Initial Unit Commitment component of MMS) and NCUC (Network Constrained Unit Commitment component of MMS). 

· For Under Generation, prepare for following “DRUC Committed Units” section of this procedure 

· For Over generation, check for COP or Load Forecast errors

· For System Lambda greater than $10, check intermediate NSM (Network Security Manager Component of MMS) results for constraint violation. 

For abnormal constraints in the NSM outputs and abnormal commitments in IUC and NCUC outputs, refer to Desktop Guide RUC  Section 2.6, step 5.

	Note
	· Resources with NO Current Operating Plan (COP) entry are considered as “Unavailable” in RUC.

· Resources with “EMR” Resource status can only be RUC committed during Emergency conditions.

	System Summary
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>DRUC Displays>UC Displays>Output Display Menu>System Outputs>Summary

Market Operation>Reliability Unit Commitment>DRUC Displays>UC Displays>Output Display Menu>System Outputs>Summary Line Flow

DETERMINE IF:

· The load forecast is reasonable for each hour,

· Any under/over generation;

THEN:

· Be aware of these when running HRUC. 

	Violated Constraints
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>DRUC Displays>DSP Displays> DSP Binding Constraint Summary

Market Operation>Reliability Unit Commitment>DRUC Displays>DSP Displays> DSP Constraint Summary
REVIEW:

· Violated constraints.  If needed, notify Operations Support Engineer to determine the validity; 

IF:

· Invalid, no further action is required,

· Valid;

THEN

· Locate the constraint on the DSP Constraint Summary display,

· Create a Suggestion Plan for the identified violated constraint

· Review the temporal constraints of the suggested resources

· If resource start-up time allows enough time to re-evaluate the need for its commitment, be aware of these conditions when running HRUC,

· RUC commit resources as needed prior to DRUC approval if needed due to temporal constraints.

IF:

· Valid; AND no Suggestion Plan or Resource is available to commit within the timeframe of the violated constraint,

THEN:

· Notify Operations Support Engineer and Transmission and Security Desk Operator to determine if an outage can be withdrawn within the timeframe, 

IF:

· No outage can be withdrawn within the timeframe,

THEN:

· Notify Operations Support Engineer to develop a Congestion Management Plan and provide it to the TO and Transmission and Security Desk Operator,

· Notify Shift Supervisor to contact the Director Control Room Operations and/or Designee of actions taken

Refer to Desktop Guide RUC Section 2.6.

	Note
	RUC Desk Operators can decide to postpone a commitment if the startup time is well into the future. It will be left up to future HRUC solutions to commit the unit.

	DRUC Committed

Units
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>DRUC Displays>DSI Displays>External Input Data>MF Generator Parameter
Market Operation>Reliability Unit Commitment>DRUC Displays>DSP Displays>DSP RUC Commitment/Decommitment Summary
IF:

· DRUC recommends the commitment of any unit;
THEN:

· Determine the validity,

· Determine the temporal constraints for each of the units,

IF:

· The resource start-up time allows enough time to re-evaluate the need for its commitment in future HRUC Study Period, AND 

· There is no reliability reason requiring the resource commitment decision to be made immediately;

THEN:

· De-select the resource prior to approving the DRUC study by changing ‘Commit’ to ‘blank’ and list reason.

IF:

· There is reliability reason requiring the resource commitment decision to be made immediately;

· Resources with long start-up times

· Resources returning from outages

· Congestion or Capacity deficiencies that may create HRUC performance issues

THEN:

· Log the reason for not de-selecting the resource.
NOTE:  A reason must be entered for commit, decommit, uncommitting, examples below:

· Evaluate later (should be used when waiting until the last possible hour to commit)

· Short start (should be used for units that can start within 1 hour)

· Voltage support

· Valley import
· Capacity (AS shortage)
· Constraint name (SLWSCRL5) * Do not use special characters

When issuing a confirmation, ensure the use of three-part communication:

· Issue the Operating Instruction

· Receive a correct repeat back

· Give an acknowledgement



	Excess Generation
	During periods of low load and excess generation:

PERIODICALLY REVIEW:

· Splunk Dashboard Viewer under the MOS_DEV folder:

· “6 DRUC Capacity” which is based on the last ran DRUC

VERIFY:

· TOTAL_LOAD is less than SS_LASL,

IF:

· Load forecast is reasonable AND the decision can be made in the future,

THEN:

· Issue OCN for Excess Reserve Capacity
· Notify the Transmission and Security Desk Operator to make Hotline call to TOs
· Post message on the ERCOT Website
Q#87 - Typical Hotline Script for OCN for Excess Capacity
Typical ERCOT Website Posting:
ERCOT issued an OCN due to a projected excess reserve capacity for [HE XX – HE XX]. 

WHEN:

· Projected excess reserve capacity;

THEN:

· Making hotline call to QSEs

· Cancelling ERCOT Website posting

· Notify the Transmission and Security Desk Operator to make hotline call to TOs.

Q#88 - Typical Hotline Script to Cancel OCN for Excess Capacity


	DRUC

Committed 

For Capacity

Shortage
	IF:

· DRUC recommends Resource(s) for capacity;
THEN

· Determine if start-up time allows enough time to re-evaluate, and

· De-select the Resource(s) prior to approving the DRUC,

After DRUC is approved:

· Issue an OCN for projected reserve capacity shortage
· Notify the Transmission and Security Desk Operator to make Hotline call to TOs
· Post message on the ERCOT Website
Q#89 - Typical Hotline Script for OCN for committing capacity in DRUC
Typical ERCOT Website Posting:
ERCOT issued an OCN due to a projected capacity shortage for [HE XX – HE XX]. 

WHEN:

· Projected reserve capacity shortage no longer exists;

THEN:

· Making hotline call to QSEs

· Cancel ERCOT Website posting

· Notify the Transmission and Security Desk Operator to make hotline call to TOs.

Q#90 - Typical Hotline Script cancellation for OCN for committing capacity in DRUC


	Manual Commitment
	REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>DRUC Displays>DSP Displays> DSP RUC Commitment/Decommitment Summary

IF:

· Additional resources are needed to solve for transmission issues (such as voltage support) and were not picked up in the DRUC run, 
· The resource start-up time doesn’t allow enough time to re-evaluate the need for its commitment in the HRUC Study Period, OR

· A Resource was given a WRUC instruction and chose not to self-commit for all hours needed;

THEN:

· Change ‘blank’ to ‘Commit’

· List reason (capacity, constraint name or voltage issue).
· Give courtesy call to QSE when commitments are made

	Note
	Resources cannot be decommitted for just a portion of a DAM-Committed Interval, which is a one-hour interval.  ERCOT may only decommit a Resource to resolve transmission constraints that otherwise cannot be resolved.  Qualifying Facilities (QFs) may be decommitted only after all other types of Resources have been assessed for decommitment.

	DRUC  Decommitted

Resources
	REVIEW REFERENCE DISPLAYS:

Market Operation>Reliability Unit Commitment>DRUC Displays>DSP Displays> DSP RUC Commitment/Decommitment Summary
IF:

· If RUC recommends commitments/decommitments; 

DETERMINE IF: 

· Outage related’
· Possible Network Model error’
· COP error for Combine Cycle configurations / JOU,
· Qualifying Facilities should be de-committed ONLY as a last resort; 
THEN:

· If this is a true decommitment:

· Confirm Decommitment

· List reason (most likely reason is ‘transmission outage’)

· If Decommitment is error related:

· No action is required

	Note
	Once you have completed your review of DRUC, consult with Market Operations to ensure they see no issues before approving. 

	Validate
	REVIEW REFERENCE DISPLAY:

Market Participation>Physical Market>SASM Market>AS Responsibility - QSE 

Market Operation>Reliability Unit Commitment>DRUC Displays>UC Displays>Output Display Menu>System Outputs>Summary

VERIFY:

· Input data

· Updated Time

· Results are reasonable

	Approval
	DRUC must be approved by 1600

REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>DRUC Displays>DSP Displays> DSP Execution Control Parameters

IF:

· The DRUC results are reasonable after all necessary modifications have been made;

THEN:

· Sort the RUC Commitment column before approving so it shows commitments at the top of the screen that currently may be lower in the table but not shown in the window;
· Approve the results, OR

IF:

· The results are unacceptable;

THEN:

· Click on Disapprove button
· Follow the Manage DRUC Failure/Timeline Deviation procedure.

IF:

· Disapprove button was selected in error;

THEN:

· Contact Service Desk to open ticket for EMMS Production Support to correct it.

	Note
	If the RUC Desk Operator disapproves the results, the results will be saved in the database for future analysis and will not be published to the MPs.

	After 

Approval
	AFTER:

· Approval button is pushed;

THEN:

· Double check display Market Participation>Physical Market>Market Results>DRUC> DRUC Results, 

· Make sure the records in this display matches data in display Market Operation>Reliability Unit Commitment>DRUC Displays >DSP Displays>DSP RUC Commitment/Decommitment Summary.
IF:

· Displays are different, the RUC commitments thought to be blanked out were sent out;

THEN:

· Notify the Service Desk to call the On-Call EMMS Production support, and
· Issue VDIs to cancel RUC instructions
When issuing a VDI or confirmation, ensure the use of three-part communication:

· Issue the Operating Instruction

· Receive a correct repeat back

· Give an acknowledgement

	Canceling

RUC

Commitments
	REVIEW REFERENCE DISPLAY:

Market Operation>Reliability Unit Commitment>HRUC Displays>DSI Displays>DSI Data Processes>DSI Operator Manual Commitment 

IF:

· A Resource is RUC committed and needs to be canceled;
· Only cancel RUC commits if the ERCOT Operator Resource commitment was unintended.
THEN:

· Issue an electronic Dispatch Instruction confirmation to cancel the RUC instruction
· Choose “CANCEL RUC COMMIT” as the Instruction Type

· Enter “unintended commitment” in other information

When issuing a VDI or confirmation, ensure the use of three-part communication:

· Issue the Operating Instruction

· Receive a correct repeat back

· Give an acknowledgement
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