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Power Operations Bulletin # 2036
ERCOT has posted/revised the Scripts manual.

The Various Changes are shown below.

A copy of the procedure can be found at:

http://www.ercot.com/mktrules/guides/procedures/index.html 

Q#7 OCN: Anticipated EEA warning for loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations: 

“This is ERCOT Operator [first and last name], at [xx:xx], ERCOT is issuing an OCN providing advance notice to loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations that grid conditions may require action. No actions are currently required other than the affected generators and loads be ready in the event conditions decline on the ERCOT Grid.  Any questions?  Thank you”.
Q#9 Operating Instruction to QSEs with loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations:
“This call requires everyone to remain on the line until it is complete.  [QSE] I will be asking you for the repeat back.  This is ERCOT Operator [first and last name], at [xx:xx], ERCOT is issuing an Operating Instruction to QSEs with loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations to reduce their electricity consumption or switch to their backup generation and redirect that capacity back to the ERCOT Grid.  This instruction shall be completed within 30 minutes. [QSE] please repeat this back to me.”
If repeat back is CORRECT, “That is correct, thank you.”

If INCORRECT, repeat the process until the repeat back is correct.
Q#17 Cancelling the Operating Instruction for QSEs with loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations:
“This call requires everyone to remain on the line until it is complete.  [QSE] I will be asking you for the repeat back.  This is ERCOT Operator [first and last name], at [xx:xx], ERCOT is cancelling the Operating Instruction for QSEs with loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations to reduce their electricity consumption or switch to their backup generation and redirect that capacity back to the ERCOT Grid.  Please return to normal operations at your earliest convenience.
[QSE] please repeat this back to me.”
If repeat back is CORRECT, “That is correct, thank you.”

If INCORRECT, repeat the process until the repeat back is correct.
T#4 OCN: Anticipated EEA warning for loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations:

“This is ERCOT Operator [first and last name], at [xx:xx], ERCOT is issuing an OCN providing advance notice to loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations that grid conditions may require action. No actions are currently required other than the affected generators and loads be ready in the event conditions decline on the ERCOT Grid.  Any questions?  Thank you”.
T#6 Operating Instruction to QSEs with loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations:
“This is ERCOT Operator [first and last name], at [xx:xx], ERCOT is issuing an Operating Instruction to QSEs with loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations to reduce their electricity consumption or switch to their backup generation and redirect that capacity back to the ERCOT Grid.  This instruction shall be completed within 30 minutes. Any questions?  Thank you”.
T#14 Cancelling the Operating Instruction for QSEs with loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations:
“This is ERCOT Operator [first and last name], at [xx:xx], ERCOT is cancelling the Operating Instruction for QSEs with loads that have generators in net-metering arrangements subject to PUCT-imposed curtailment obligations to reduce their electricity consumption or switch to their backup generation and redirect that capacity back to the ERCOT Grid.  Any questions?  Thank you”.
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