Generation Interconnection Procedure Meeting

Detailed Agenda


ERCOT is currently revising and updating the "Generation Interconnection or Change Request Procedure".  A meeting to present and discuss the draft of the procedures is planned for Wednesday, August 30, 2006 from 9:00 AM to 4:00 PM at the Austin Control Center (MET Center) in Room 206A.

In general, this draft is a “re-packaging” of the current procedures with the following major changes/updates:

Transparency

Provide more data relating to generation interconnection requests in screening study and full interconnection study phases


Screening Study Phase



Post MW level, county location and fuel type


Full Interconnect Study Phase



All projects would be public



Studies would be posted when completed



Supports planning process

Retroactive for active all interconnection requests 

Accounting

ERCOT no longer collects deposit for full interconnection studies (FIS) ERCOT continues to collect modeling fee ERCOT continues to collect screening study fee FIS costs paid directly by requester to TSP Costs and payment schedule part of FIS Study Scope and agreement

Technical Requirements

Add Low Voltage Ride Through (LVRT) capability as outlined in NERC/FERC requirements for wind farms signing interconnection agreements as of January 1, 2007 and later Clarify ERCOT requirements and enforcement, including Reactive Requirements, Stability Software Models, Power System Stabilizers and data requirements

