|  |  |  |  |
| --- | --- | --- | --- |
| **Resource/Metric** | **Protocol Reference (§)** | **X (%)** | **Y (MW)** |
| Base Point Deviation, Over-Consumption, Controllable Load Resource | 6.6.5.1.1.3 | 25 | 2 |
| Base Point Deviation, Under-Consumption, Controllable Load Resource | 6.6.5.1.1.4 | 15 | 2 |
| Base Point Deviation, Over-Consumption, Controllable Load Resource with Ancillary Service responsibility | 6.6.5.1.1.3 | 15 | 2 |
| Base Point Deviation, Under-Consumption, Controllable Load Resource with Ancillary Service Responsibility | 6.6.5.1.1.4 | 10 | 2 |
| CLREDP | 8.1.1.4.1(9) | 25 | 2 |
| CLREDP with Ancillary Service Responsibility | 8.1.1.4.1(9) | 15 | 2 |
| **Resource/Metric** | **Protocol Reference (§)** | **Factor** | |
| Load Resource Reserve Discount Factor for Controllable Load Resources carrying Ancillary Service Resource Responsibility (LRDF 1) | 6.5.7.5 (o) | 1.0 | |
| Load Resource Reserve Discount Factor for Controllable Load Resources not carrying Ancillary Service Resource Responsibility (LRDF 2) | 6.5.7.5 (o) | 1.0 | |