**R5 Market Facing Changes (PROD Release 11/01 – 11/03)**

From Market Notice M-B093016-01 Release – Retail/Wholesale: Implementation of market-facing changes for November 2016

|  |  |
| --- | --- |
| **Change ID** | **Market Notice Description** |
| ITCM-29344  NPRR712 | Protocol language of paragraph (3) of Section 8.1.2 related to NPRR712 will be implemented to update the monthly DRUC and HRUC Performance report |
| ITCM-27484 | New link on the MIS for 2021 GINR Screening, Steady-State, Short-Circuit and Facilities Reports (EMIL ID: NP1-344-M, Report ID: 13948) to be located at Grid >Resource Integration > Partial Generation Interconnection (INR) Studies |
| ITCM-27481 | New link on the MIS for 2021 GINR Stability and SSO Reports (EMIL ID: NP1-343-M, Report ID: 13947) located at Grid > Resource Integration > TSP Generation Interconnection (INR) Studies portlet. |
| ITCM-27480 | New link on the MIS for 2017 Regional Transmission Plan Postings (EMIL ID: PG7-159-M, Report ID: 13946) located at Grid > Regional Planning > Regional Transmission Planning (5 year Transmission Plan) portlet. |
| ITCM-25484 | MIS Link name change for PR174-28:  Name Change to: Transmission Outage Schedule Statistics  from: Advanced Transmission Outage Statistics  (NP8-406-ER, Rpt ID 10095) |
| ITCM-23790  ITCM-23757  NPRR495  NPRR736  NPRR770 | Modify the Ancillary Service Capacity Monitor information provided by ERCOT both through Inter-Control Center Communications Protocol (ICCP) telemetry and the Market Information System (MIS) Public Area |
| ITCM-17229 | Currently, front-end validation accepts bids/offers of Curve type that are also multi-hour blocked, but the DAM clearing does not honor the multi-hour block, as noted in the Market Submission Validation Rules document on the MIS:  "Offers submitted as a curve are always allowed to be awarded differing quantities in each hour."  With this release, we are adding a new validation rule that would reject a bid or offer that was a curve and also multi-hour blocked. Only Fixed and Variable types are permitted for multi-hour blocks. |
| ITCM-15031  ITCM-15030  NOGRR143 | Updates the existing historical governor test form in the NDCRC to align with the generator governor performance report per BAL-001-TRE |

**R6 Market Facing Changes (PROD Release 12/06 – 12/08)**

NOTE: This list may not be all inclusive of changes going into the release and could change prior to the release.

|  |  |
| --- | --- |
| **Change ID** | **Market Notice Description** |
| ITCM-10314  NPRR754 | Revise the posting frequency of the Load Forecast Distribution Factors report (EMIL ID NP4-159-CD, Report ID 12324) to require posting of the report only when the factors are changed. Report name to be changed to Load Distribution Factors from Load Forecast Distribution Factors |
| ITCM-30828  PGRR046 | New portlet and link on MIS on Groups and Rules > Transmission Service Provider Information page:  New Portlet: Models  New Link: GIC System Models (PG6-105-M, 14546) |
| [ITCM-26634](https://corp.ercot.com/jira/browse/ITCM-26634) | Add ERCOT boundaries to Standard Gradient LMP Contour Maps |