**DMTF Preliminary Outline for Final Report**

**Introduction**

* Reference issues identified in ROS-approved scope for DMTF

**Process for Submitting, Reviewing, and Maintaining Dynamic Models**

* Recommend that ERCOT staff coordinate with RDWG on how to implement a requirement to use templates for dynamic model submission in the RARF
* Recommend that ERCOT staff continue Template development as necessary
* Recommend that DWG develop MOD-026/027 process guidelines to facilitate consistency among TSPs regarding model submission requirements and model usability evaluations

**Acceptable/Obsolete Model List Development**

* Adopted NERC SAMS model list – implemented in DWG Procedure Manual

**Specialized Dynamic Models - EMTP (PSCAD) Model**

* Recommend that ERCOT staff coordinate with RDWG on how to implement PSCAD model requirements (reference draft guidelines document)
* Recommend that Resource Entities be required to submit PSCAD models through the RARF so that they are subject to normal ERCOT confidentiality protocols eliminating the need for ERCOT and TSPs to sign specialized NDAs

**The Requirement and Limitation of User-Defined Dynamic Models (UDM)**

* Recommend that DWG include UDM requirements in their Procedure Manual (reference draft guidelines document)