**Section 2:**

**NOGRR233 –Related to NPRR1094, Allow Under Frequency Relay Load to be Manually Shed During EEA3**

This Nodal Operating Guide Revision Request (NOGRR) allows a Transmission Operator (TO) and a Transmission and/or Distribution Service Provider (TDSP) to manually shed Load connected to under-frequency relays during an Energy Emergency Alert (EEA) Level 3 if the affected TO can meet its overall Under-Frequency Load Shed (UFLS) requirement in Section 2.6.1, Automatic Firm Load Shedding, and its Load shed obligation under Section 4.5.3.4, Load Shed Obligation.

**Revised Subsection: 2.6.1**

**Section 4 :**

**NOGRR236 – Related to NPRR1105, Option to Deploy Distribution Voltage Reduction Measures Prior to Energy Emergency Alert (EEA)**

This Nodal Operating Guide Revision Request (NOGRR) provides ERCOT the ability to instruct Transmission and/or Distribution Service Providers (TDSPs) to deploy any available distribution voltage reduction measures prior to ERCOT declaring an Energy Emergency Alert (EEA) if ERCOT determines it is possible that the deployment of these measures could avoid the need to declare an EEA and ERCOT does not expect to need these measures to reduce the amount of Load shedding that may be needed in EEA Level 3. These revisions also clarify the role of TDSPs in determining whether distribution voltage reduction should be implemented.

**Revised Subsection: 4.5.3.1**

**NOGRR237 – Related to NPRR1106, Deployment of Emergency Response Service (ERS) Prior to Declaration of Energy Emergency Alert (EEA)**

This Nodal Operating Guide Revision Request (NOGRR) aligns the Nodal Operating Guide with Protocol changes proposed by NPRR1106, allowing ERCOT to deploy ERS prior to an Energy Emergency Alert (EEA).

**Revised Subsection: 4.5.3.1**

**NOGRR238 – Alignment Changes for December 17, 2021 Nodal Operating Guide – NPRR1094, NPRR1105, NPRR1106**

This Nodal Operating Guide Revision Request (NOGRR) aligns Energy Emergency Alert (EEA) language in Section 4.5.3.3 with Protocol Section 6.5.9.4.2, EEA Levels.

**Revised Subsection: 4.5.3.3**

**Administrative Changes:**

Non-substantive administrative changes were made such as spelling corrections, formatting, and correcting Section numbering and references.

**Revised Subsection: 4.5.3.1, 4.5.3.3**