**Section 2:**

NPRR989 – BESTF-1 Energy Storage Resource Technical Requirements

This Nodal Protocol Revision Request (NPRR) establishes technical requirements for Energy Storage Resources (ESRs) for Voltage Support Service (VSS) (including Reactive Power capability), and Primary Frequency Response.

Revised Subsection: 2.1 [partially unboxed due to system implementation]

**Section 3:**

NPRR989 – BESTF-1 Energy Storage Resource Technical Requirements

*See Section 2 above.*

Revised Subsections: 3.15, 3.15.1, and 3.15.3 [partially unboxed due to system implementation]

NPRR1038 – BESTF-8 Limited Exemption from Reactive Power Requirements for Certain Energy Storage Resources

This Nodal Protocol Revision Request (NPRR) establishes a limited exemption from Reactive Power requirements for certain Energy Storage Resources (ESRs). The exemption is available only to an ESR that achieved Initial Synchronization prior to December 16, 2019 and applies only to the extent the ESR is unable to comply with the Reactive Power requirements when it is charging. In order to qualify for the exemption, the Resource Entity for the ESR must submit a notarized attestation to ERCOT stating that the ESR would be unable to comply with the Reactive Power requirements without making physical or software changes. The NPRR does not exempt any ESR from the responsibility to provide Reactive Power when discharging.

Revised Subsection: 3.15 [unboxed due to system implementation of NPRR989]

**Section 6:**

NPRR989 – BESTF-1 Energy Storage Resource Technical Requirements

*See Section 2 above.*

Revised Subsection: 6.5.7.7 [partially unboxed due to system implementation]

**Section 8:**

NPRR989 – BESTF-1 Energy Storage Resource Technical Requirements

*See Section 2 above.*

Revised Subsections: 8.1.1.2.1.4 and 8.5.1 [partially unboxed due to system implementation]

NPRR1040 – Compliance Metrics for Ancillary Service Supply Responsibility

This Nodal Protocol Revision Request (NPRR) establishes compliance metrics for Ancillary Service Supply Responsibility.

Revised Subsections: 8.1.1.3 and 8.1.1.4.1 [unboxed due to system implementation]

**Section 16:**

NPRR1165 – Revisions to Requirements of Providing Audited Financial Statements and Providing Independent Amount

This Nodal Protocol Revision Request (NPRR) strengthens ERCOT’s market entry eligibility and continued participation requirements for ERCOT Counter-Parties (i.e., Qualified Scheduling Entities (QSEs) and Congestion Revenue Right (CRR) Account Holders).

Revised Subsections: 16.2.1, 16.11, 16.11.5, 16.11.8, 16.16.1, 16.16.2, 16.16.3, and 16.17 [unboxed due to system implementation]

**Section 22:**

NPRR1165 – Revisions to Requirements of Providing Audited Financial Statements and Providing Independent Amount

*See Section 16 above.*

Revised Attachment: J [unboxed due to system implementation]