Summary of Planning Guide Revisions

Effective:  October 29, 2026
Section 3:
PGRR113 – Related to NPRR1198, Congestion Mitigation Using Topology Reconfigurations
This Planning Guide Revision Request (PGRR) revises the Planning Guide to provide that ERCOT will first consider transmission needs without Constraint Management Plan (CMP) actions in its Regional Transmission Plan studies and will then only model a CMP in the Regional Transmission Plan in certain limited circumstances.  A CMP will not be planned to resolve a planning criteria performance deficiency unless it is expected that system conditions will change such that the CMP will no longer be needed within the next five years.

Revised Subsection:  3.1.4.1.1 [unboxed due to system implementation of Nodal Protocol Revision Request (NPRR) 1198, Congestion Mitigation Using Topology Reconfigurations]
Section 4:
PGRR113 – Related to NPRR1198, Congestion Mitigation Using Topology Reconfigurations

See Section 3 above.
Revised Subsection:  4.1.1.2 [unboxed due to system implementation of NPRR1198]
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